Bell 206 Aircraft Airworthiness Check


INSTRUCTIONS:  Discrepancies of airworthiness conditions must be entered in the aircraft logbook.  Correction of discrepancies must be accomplished prior to flight.

	#
	Fuselage

	1. 
	Check seat belts for general condition and security

	2. 
	Check windshields for cleanliness and obvious damage.

	3. 
	Check pitot tube and static ports for general condition and security.

	4. 
	Inspect antennas for general condition and security.

	5. 
	Inspect battery compartment for loose wiring and corrosion. Check battery for general condition and security.

	6. 
	Function check nav, strobe, landing, interior, and caution lights. Electric cargo hook release, pitot heat, and defog motors.

	7. 
	Inspect interior of pilot and passenger compartments for proper storage of loose equipment, general cleanliness, and overall condition.

	8. 
	Check the fire extinguisher for general condition, security, and inspection due date.  Ensure safety pin is installed and secured in place with a safety tie.

	9. 
	Check life vests (if applicable) for general condition and security.  Be sure to check the life vests’ inspection due date, CO2 bottles for tightness and inflation valve locks for integrity.

	10. 
	Check life raft (if applicable) for general condition, security, and inspection due date.

	11. 
	Check the First Aid Kit for proper sealing and inspection due date.

	12. 
	Check the Survival Kit for proper sealing and inspection due date.

	13. 
	Ensure passenger briefing cards are in the aircraft.

	14. 
	Check the fuselage exterior for general condition, security, and evidence of fuel or oil leaks.


	#
	Landing Gear

	1. 
	Inspect landing gear attachment fittings for obvious damage and cracks. Inspect cross tubes and skid tubes for general condition and security.

	2. 
	Inspect cargo hook assembly for general condition and security.

	3. 
	Check float covers (if applicable) for general condition and security.

	4. 
	Check float bottles (if applicable) for proper mounting, general condition, and security.

	5. 
	Check float bottles (if applicable) for proper inflation pressure.

	6. 
	(If installed) Inspect flite steps for security of attachment and damage.

	7. 
	(If installed) Inspect cargo for security of attachment and damage.



	
#
	Tailboom

	1. 
	Inspect tailboom for dents, wrinkles, general condition, and security. 

	2. 
	Inspect horizontal stabilizer, fins, and position lights for general condition and security. Inspect horizontal stabilizer slat supports for cracks.

	3. 
	Inspect tail rotor gearbox for evidence of oil leakage, general condition, and security.

	4. 
	Check tail rotor gearbox for proper oil level.

	5. 
	Clean tail rotor blades.

	6. 
	Inspect tail rotor hub, blades, and pitch change mechanism for general condition and security. Grease tail rotor hub bearings.

	7. 
	Inspect vertical fin and anti-collision light for general condition and security.



	#
	Fuel System

	1. 
	Take fuel sample from main tank. Turn on boost bumps and fuel valve and take fuel sample from airframe fuel filter.

	2. 
	Verify illumination of airframe fuel filter caution light on caution panel by depressing differential switch “press to test” button on filter head. Turn battery switch off.

	3. 
	Inspect fuel sample for cleanliness, water, and debris.

	4. 
	Inspect fuel cap for proper operation and that placard stating type and quantity of fuel used is present in area of fuel cap.



	#
	Powerplant

	1. 
	Inspect engine area for evidence of oil and fuel leaks.

	2. 
	Inspect all engine lines and electrical wiring for general condition and security. Inspect all engine fuel, oil, and air tube “B” nuts for proper alignment, torque seal, and safety wire.

	3. 
	Inspect engine mounts for general condition and security.

	4. 
	Inspect compressor inlet for obvious obstruction or damage.

	5. 
	Inspect Keflex drive shaft for broken, lose or missing hardware. Inspect flex frame and mount bolt stripes for evidence of slippage. Inspect flex frame joints for fretting.  DO NOT DISTURB OR TIGHTEN FLEXFRAME NUTS OR BOLTS.

	6. 
	Inspect engine exhaust stack for cracks, general condition, and security.

	7. 
	Inspect #1 tail rotor drive shaft for general condition, and security. Inspect fore and aft Thomas couplings for cracks. 

	8. 
	Inspect oil cooler upper surface for obstructions, evidence of oil leakage, general condition, and security.

	9. 
	Inspect engine oil reservoir for general condition and security. Check for proper oil level.

	10. 
	Inspect engine external NiCad filter for bypass indication. 



	#
	Transmission

	1. 
	Inspect transmission mounts and restraints for general condition and security. 

	2. 
	Inspect transmission for evidence of oil leaks, general condition, and security. Check for proper oil level.

	3. 
	Inspect transmission oil filter for bypass indication.

	4. 
	Check hydraulic filter indicator buttons for bypass condition.

	5. 
	Check hydraulic reservoir for proper oil level.

	6. 
	Inspect hydraulic lines and servo actuators for leaks, general condition, and security.

	7. 
	Inspect linkage pivot bolts on hydraulic servo actuators for freedom of rotation and security.

	8. 
	Inspect flight control tubes and bellcranks from servo actuators to swashplate for general condition and security.

	9. 
	Inspect swashplate assembly for damage and excessive play. 

	10. 
	Inspect main rotor pitch change links for general condition and security.

	11. 
	Inspect main rotor hub for general condition and security. Check for anti-slippage marks on the pillow block retention hardware. Grease main rotor hub.

	12. 
	Inspect main rotor blades for cleanliness and overall condition. Inspect for cracks, corrosion, and de-bonding of doublers



	#
	General

	1. 
	Review aircraft computer status sheet and logbook for upcoming maintenance. Comply with items due during the next eight hours, next calendar day or during the aircraft cycles predicted for the next flight day.

	2. 
	Check accuracy of aircraft time in logbook. Check addition, verify correct hour meter time recorded, and compare hour meter time to aircraft time. Verify correct entry onto input sheet.



