	MARITIME HELICOPTERS
	BELL 206L SERIES AAIP

	
	

	Page No:
	C-10

	Revision:
	8

	Issue Date:
	11/01/20

	
	
	             Daily Airworthiness Check

	
	
	

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


NOTE:  The Daily Airworthiness Check will be completed and signed off I/A/W MHI GMM Chapter 2
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0025.1 GENERAL

	
	
	

	1.1 Review aircraft computer status run, Deferred/MEL list and logbook ladder for maintenance and/or inspection requirements.  
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) have been accomplished.
	
	

	
	
	

	A 0025.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0025.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0025.4 FUSELAGE

	
	
	

	4.1 Seat belts for general condition and security
	
	

	
	
	

	4.2 Windshields for cleanliness and obvious damage.
	
	

	
	
	

	4.3 Pitot tube and static ports for general condition and security.
	
	

	
	
	

	4.4 Antennas for general condition and security.
	
	

	
	
	

	4.5 Battery compartment for loose wiring and corrosion. Check battery for general condition and security
	
	

	
	
	

	4.6 Function check nav, strobe, landing, interior, and caution lights. Electric cargo hook release, pitot heat, and defog motors.
	
	

	
	
	

	4.7 Interior of pilot and passenger compartments for proper storage of loose equipment, general cleanliness, and overall condition.
	
	

	
	
	

	4.8 Fire extinguisher for general condition, security, and inspection due date.  Ensure safety pin is installed and secured in place with a safety tie.
	
	

	
	
	

	4.9 Life vests (if applicable) for general condition and security.  Be sure to check the life vests’ inspection due date, CO2 bottles for tightness and inflation valve locks for integrity.
	
	

	
	
	

	4.10 Life raft (if applicable) for general condition, security, and inspection due date.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.11 First Aid Kit for proper sealing and inspection due date.
	
	

	
	
	

	4.12 Survival Kit for proper sealing and inspection due date.
	
	

	
	
	

	4.13 Ensure passenger briefing cards are in the aircraft.
	
	

	
	
	

	4.14 Fuselage exterior for general condition, security, and evidence of fuel or oil leaks.
	
	

	
	
	

	A 0025.5 LANDING GEAR

	
	
	

	5.1 Landing gear attachment fittings for obvious damage and cracks. Inspect cross tubes and skid tubes for general condition and security.
	
	

	
	
	

	5.2 Cargo hook assembly for general condition and security.
	
	

	
	
	

	5.3 Float covers (if applicable) for general condition and security.
	
	

	
	
	

	5.4 Float bottles (if applicable) for proper mounting, general condition, and security.
	
	

	
	
	

	5.5 Float bottles (if applicable) for proper inflation pressure.
	
	

	
	
	

	5.6 (If installed) Inspect flite steps for security of attachment and damage.
	
	

	
	
	

	5.7 (If installed) Inspect cargo for security of attachment and damage.
	
	

	
	
	

	A 0025.6 TAILBOOM

	
	
	

	6.1 Tailboom for dents, wrinkles, general condition, and security.
	
	

	
	
	

	6.2 Horizontal stabilizer, fins, and position lights for general condition and security.
	
	

	
	
	

	6.3 Horizontal stabilizer slat supports for cracks.
	
	

	
	
	

	6.4 Tail rotor gearbox for evidence of oil leakage, general condition, and security.
	
	

	
	
	

	6.5 Tail rotor gearbox for proper oil level.
	
	

	
	
	

	6.6 Clean tail rotor blades.
	
	

	
	
	

	6.7 Tail rotor hub, blades, and pitch change mechanism for general condition and security. Grease tail rotor hub bearings.
	
	

	
	
	

	6.8 Vertical fin and anti-collision light for general condition and security.
	
	

	
	
	






	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0025.7 FUEL SYSTEM

	
	
	

	7.1 Take fuel sample from main tank. Turn on boost bumps and fuel valve and take fuel sample from airframe fuel filter.
	
	

	7.2 Verify illumination of airframe fuel filter caution light on caution panel by depressing differential switch “press to test” button on filter head. Turn battery switch off.
	
	

	
	
	

	7.3 Inspect fuel sample for cleanliness, water, and debris.
	
	

	
	
	

	7.4 Inspect fuel cap for proper operation and that placard stating type and quantity of fuel used is present in area of fuel cap.
	
	

	
	
	

	A 0025.8 POWERPLANT

	
	
	

	8.1 Engine area for evidence of oil and fuel leaks.
	
	

	8.2 All engine lines and electrical wiring for general condition and security. Inspect all engine fuel, oil, and air tube “B” nuts for proper alignment, torque seal, and safety wire.
	
	

	
	
	

	8.3 Engine mounts for general condition and security.
	
	

	
	
	

	8.4 Compressor inlet for obvious obstruction or damage.
	
	

	
	
	

	8.5 Keflex drive shaft for broken, lose or missing hardware. Inspect flex frame and mount bolt stripes for evidence of slippage. Inspect flex frame joints for fretting.  
NOTE: DO NOT DISTURB OR TIGHTEN FLEXFRAME NUTS OR BOLTS.
	
	

	
	
	

	8.6 Engine exhaust stack for cracks, general condition, and security.
	
	

	
	
	

	8.7 #1 tail rotor drive shaft for general condition, and security. Inspect fore and aft Thomas couplings for cracks.
	
	

	
	
	

	8.8 Oil cooler upper surface for obstructions, evidence of oil leakage, general condition, and security
	
	

	
	
	

	8.9 Engine oil reservoir for general condition and security. Check for proper oil level.
	
	

	
	
	

	8.10 Engine external NiCad filter for bypass indication.
	
	

	
	
	

	A 0025.9 TRANSMISSION

	
	
	

	8.11 Transmission mounts and restraints for general condition and security.
	
	

	8.12 Evidence of oil leaks, general condition, and security. Check for proper oil level.
	
	

	
	
	

	8.13 Transmission oil filter for bypass indication.
	
	

	
	
	

	8.14 Hydraulic filter indicator buttons for bypass condition.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	8.15 Hydraulic reservoir for proper oil level.
	
	

	
	
	

	8.16 Hydraulic lines and servo actuators for leaks, general condition, and security.
	
	

	
	
	

	8.17 Linkage pivot bolts on hydraulic servo actuators for freedom of rotation and security.
	
	

	
	
	

	8.18 Flight control tubes and bellcranks from servo actuators to swashplate for general condition and security.
	
	

	
	
	

	8.19 Swashplate assembly for damage and excessive play.
	
	

	
	
	

	8.20 Main rotor pitch change links for general condition and security.
	
	

	
	
	

	8.21 Main rotor hub for general condition and security. Check for anti-slippage marks on the pillow block retention hardware. 
	
	

	
	
	

	8.22 Grease main rotor hub.
	
	

	
	
	

	8.23 Main rotor blades for cleanliness and overall condition. Inspect for cracks, corrosion, and de-bonding of doublers.
	
	

	
	
	

	A 0025.10 POST INSPECTION

	
	
	

	9.1 Condition and security of all cowling and access panels, all secure.
	
	

	
	
	

	9.2 Aircraft documents for proper entries.
	
	

	
	
	

	9.3 Review aircraft computer status sheet and logbook for upcoming maintenance. Comply with items due during the next eight hours, next calendar day or during the aircraft cycles predicted for the next flight day.
	
	

	
	
	

	9.4 Check accuracy of aircraft time in logbook. Check addition, verify correct hour meter time recorded, and compare hour meter time to aircraft time. Verify correct entry onto input sheet.
	
	

	
	
	






