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	SECTION:
	
	C 0050 – ICA OF INSTALLED EQUIPMENT

	TYPE:
	
	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0050.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	C  0050.2 

	2.1 
	
	

	
	
	

	2.2 
	
	

	
	
	

	2.3 
	
	

	
	
	

	2.4 
	
	

	
	
	

	2.5 
	
	

	
	
	

	2.6 
	
	

	
	
	

	2.7 
	
	

	2.8 
	
	

	
	
	

	2.9 
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0050.3 DART SKID TUBES - ICA-D206-642

	
	
	

	3.1 Inspect all areas of the installation visually for mechanical damage (nicks and scratches) and corrosion. It is acceptable to have nicks, scratches, or corrosion damage up to 0.010" (0.4 mm) deep anywhere on the skidtube.
	
	

	NOTE: Blend out scratches/nicks/corrosion in the skidtube using 400 grit abrasive cloth to a maximum depth of 0.010" (0.4 mm). There should be a smooth transition from the surrounding tube to the affected area. After clean up, touch up affected area with chemical film material (Alodine 1200 or 1201) per MIL-C-5541, one coat of MIL-P-85582 or MIL-P-23377 primer, and 2-3 coats of MIL-C-83285 polyurethane paint to match original finish.
	

	3.2 Check wearshoes for excessive wear/damage. Wearshoes need to be replaced when 2 sequential tabs are cracked or when the wearshoe has wear, scratches, nicks, or corrosion damage of any size deeper than 0.030" (0.8 mm). Wearshoes with hard surfacing should be replaced when the hard surfacing has worn through.
	
	

	
	
	

	3.3 Inspect the skidtube assembly for serious damage in any of the areas indicated by “X” in Figure 5-2.
	
	

	NOTE: Serious damage is defined as follows:

- cracks that exceed 0.25” (6.4 mm) in length

- localized denting deeper than 0.015” (0.4 mm)

- skidtube dimensions beyond the limits shown in Figure 5-3 
  (adjust limits for corrosion/wear as described in item 5.2.1 above)
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This type of damage is unacceptable anywhere along the straight section of the tube. Replace parts per item 5.2.12.
	
	

	3.4 Inspect the sides of the skidtube for excessive wear/damage. Oents up to 2.00" (51 mm) long x 1.00" (25 mm) wide x 0.12" (3.0 mm) deep are acceptable in the areas indicated 'OK' in Figure 5-2. Oamaged areas should be a minimum of 3.00" (76 mm) apart.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	

	3.5 Cracks on the sides (areas indicated by 'OK' in Figure 5-2) of the skidtubes that do not exceed 1.00" (25 mm) in length can be repaired by T.I.G. welding as follows:
	

	
	

	3.5.1 Clean area of paint, etc.
	
	

	
	
	

	3.5.2 Grind a chamfer 0.050" (1.3 mm) x 45° along crack
	
	

	
	
	

	3.5.3 T.I.G. weld per MIL-STO-2219 Class 'C' using 5356 filler rod and grind flush
	
	

	
	
	

	3.5.4 Touch up affected areas with chemical film material (Alodine 1200 or 1201) per MIL-C-5541, one coat of MIL-P-85582 or MIL-P-23377 primer, and 2-3 coats of MIL-C-83285 polyurethane coat to match original finish
	
	

	NOTE: It is unacceptable to perform weld repairs on the skidtubes in the saddle areas. Weld repairs must be a minimum of 1" (25 mm) apart.
	

	3.6 Inspect the area between the saddles for bow or sharp bends. A smooth bow in the skidtube from saddle to saddle is acceptable as long as permanent deflection does not exceed 0.50" (13 mm). Maximum deflection should be at or near the midpoint between the saddles.
	
	

	
	
	

	3.7 Inspect the aft cap for damage. If cracked or porous, replace the cap in accordance with item 7.12.
	
	

	
	
	

	3.8 Inspect the tow rings and associated attachment hardware for cracks, bending, wear and suitability for continued service. Cracks in the tow ring may be repaired by TIG welding per MILSTO-2219 using an ER70S-6 filler rod (when repairing the 02707-043 Tow Ring) or using an RG-45 filler rod (when repairing the 02968-043 Tow Ring) or using a TIG174 filler rod (when repairing the 03407-043 Tow Ring). Replace unserviceable/non-repairable parts per item 7.12.
	
	

	
	
	

	3.9 Inspect the ground handling lugs and associated attachment hardware for cracks, bending, wear and suitability for continued service. Cracks in the ground handling lugs may be repaired by TIG welding per MIL-STO-2219 using an ER70S-6 filler rod (when repairing the 02659 GHW lug) or using an ER316L or ER308L filler rod (when repairing the 03414-041 GHW lug). Replace unserviceable/non-repairable parts per item 7.12.
	
	

	
	
	

	3.10 Check saddles for signs of yielding (Le. buckled or twisted flanges or noticeable increases in the size of gaps between the saddles and the crosstube/skidtube), cracking, or elongation of holes. Saddle holes may be elongated by up to 0.025" (0.6 mm). Saddles with any signs of cracks should be replaced immediately per item 5.2.12. Scratches or corrosion damage up to 0.010" (0.25 mm) deep can be blended out with scotchbrite up to 0.010" (0.25 mm) deep. Touch up repaired areas with chemical film material (Alodine 1200 or 1201) per MIL-C-5541, one coat of MIL-P-85582 or MIL-P-23377 primer, and 2-3 coats of MIL-C-85285 polyurethane coating to match original finish. Ensure that the saddles are sealed in accordance with Section 32. The torque on all saddle fasteners are within acceptable limits of Section 32.2 and adjust per the instructions in Section 32.2 of the ICA.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.11 Inspect all areas of the skidtube for suitability of the paint finish. Touch up affected areas with chemical film material (Alodine 1200 or 1201) per MIL-C-5541 (aluminum only), one coat of MIL-P-85582 or MIL-P-23377 primer, and 2-3 coats of MIL-C-83285 polyurethane paint to match original finish. Clean off flaking anti-skid and touch up with Black Anti-Skid paint per MIL-W-5044 Type 2.
	
	

	
	
	

	3.12 Any part which does not meet the limitations described above is considered to be excessively damaged or unserviceable. Replace all excessively damaged or unserviceable parts per Chapter 32 of the ICA.
	
	

	
	
	

	C  0050.4 POST INSPECTION

	
	
	

	4.1 Inspect for operation and leaks.
	
	

	
	
	

	4.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	4.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	
	

	
	
	

	4.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – C 0050 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


