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	Revision:
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	SECTION:
	
	A 0100 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	100 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 4, 5, 12, 65

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0100.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0100.2 [bookmark: _Hlk512334205]TAIL ROTOR DRIVESHAFT

	
	
	

	2.1 [bookmark: _Hlk528931929]Examine the entire tail rotor driveshaft for condition and security. Examine the components as follows. Includes AFT and FWD short shafts.
	Chapter 65
	

	
	
	

	2.1.1 All bearings, hangers for loose and working rivets.
	
	

	
	
	

	2.1.2 All disc pack couplings for condition.
	
	

	
	
	

	2.1.3 All driveshaft tube assemblies. 
	
	

	
	
	

	2.2 Lubricate short shaft and tail rotor driveshaft splines – C-525 or C-561
	Chapter 12
12-42
	

	NOTE: Grease with C-525 or C561 every 100 hours or when a new component is installed.
	

	EFFECTIVITY: Pre TB 407-02-35
	

	2.3 Lubricate oil cooler blower hangar (2 places) and tail rotor driveshaft hangar bearings (4 places) – C-001
	Chapter 12
12-40, 41
	

	
WARNING
DO NOT PURGE LUBRICATE THE OIL COOLER BLOWER OR TAIL ROTOR DRIVESHAFT HANGAR BEARINGS.

THESE BEARINGS HAVE A BROWN ELASTOMER SEAL. MIXING GREASE (C-001) MOBIL 28 LUBRICANT (C-026) OR ANY OTHER GREASE WILL DAMAGE THE BEARING. THE BEARING MUST BE SCRAPPED IF GREASES HAVE BEEN MIXED.
	

	2.3.1 Do a torque check of all disc pack coupling attachment hardware (150 to 180 inch-pounds) to include AFT and FWD short shafts.
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0100.3 TAILBOOM  SRUCTURE

	
	ASB 407-07-80A
BHT-407-MM-1
Figure 4-7
	

	3.1 Inspect the complete tailboom assembly for general condition. Use a 10X Magnifying glass to inspect for cracks in tailboom skin.
	
	

	EFFECTIVITY: Tailboom P/N 407-030-801-107 & 407-530-014-101/-103
	

	A 0100.4 MAIN ROTOR 

	
	
	

	4.1 Perform yoke inspection
	Chapter 4
Fig 4-2
	

	A 0100.5 POST INSPECTION

	
	
	

	5.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	5.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	5.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	5.5 Make an entry in the appropriate logbook regarding a retorque check of the disc pack coupling attachment hardware in 10 to 25 hours.
	Table 5-3
	

	
	
	





Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0100 – 100 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




