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	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 206L Series MM-1 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1202.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 1202.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	A 1202.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this AAIP inspection.
	CSSD-PSE-87-001 
	

	
	
	

	A 1202.4 TAILBOOM ASB 206L-99-115

	NOTE: This inspection is to be complied with every 1200 hours of tailboom operation after compliance with ASB 206L-99-115, except as follows:

EFFECTIVITY: The inspection is not required for tailbooms;                        
P/N 206-033-004-181/-199 and subsequent
P/N 206-704-727-101, P/N 206-074-727-103
P/N 206-707-727-105
All tailbooms upgraded per PSE letter and reidentified as an equivalent of 206-033-004-199.
	

	4.1 Prepare tailboom assembly for inspection by removing the following components:
	
	

	
	
	

	4.1.1 Auxiliary fin assembly.
	
	

	
	
	

	4.1.2 Slat assembly.
	
	

	
	
	

	4.1.3 Stabilizer and support.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.2 Gain access to inside of tailboom from right side. Using a bright light, perform inspection of skin on inside surface of left side of tailboom for cracks.
	
	

	
	
	

	4.2.1 Inspect skin in area where doubler is attached.
	
	

	
	
	

	4.2.2 Inspect each rivet location for signs of loose or working rivets and for cracks that start at rivet holes.
	
	

	
	
	

	4.3 Using a 10X magnifying glass, perform a visual inspection of external left side of tailboom at doubler and skin around doubler in the following areas:
	
	

	
	
	

	4.3.1 Inspect internal edge of doubler for cracks.
	
	

	
	
	

	4.3.2 Inspect support attachment holes for cracks.
	
	

	
	
	

	4.3.3 Inspect each rivet location for loose or working rivets and cracks that start from rivet holes.
	
	

	
	
	

	4.3.4 Inspect edge of doubler for delamination between skin and doubler.
	
	

	
	
	

	4.3.5 Inspect tailboom skin area up to 1.00 inch (25.40 mm) area around doubler for cracks.
	
	

	
	
	

	4.4 Using a 10X magnifying glass, perform a visual inspection of external right side of tailboom skin stabilizer cutout.
	
	

	
	
	

	4.4.1 Inspect edge of cutout for cracks in skin.
	
	

	
	
	

	4.4.2 Inspect support attachment holes for cracks in skin.
	
	

	
	
	

	4.5 If a crack is detected in tailboom skin or doubler, contact Product Support Engineering as follows:
	
	

	
	
	

	A 1202.5 POST INSPECTION

	
	
	

	5.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-206L-FM-1
	

	
	
	

	5.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.3 Perform Functional Check Flight if required per Bell 206L Series Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	5.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – A 1202 – 1200 Hour Tailboom Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




