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	C 0020 – ICA OF INSTALLED EQUIPMENT
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0020.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	C 0020.2 BELL BARRIER FILTER SYSTEM – AFS-BH206L3L4-IBF-KIT-ICA 

	
	

	2.1 STRUCTURAL COMPONENT INSPECTIONS
	

	
	

	2.1.1 Visually inspect the following components:
	

	
	

	2.1.1.1 Air induction cowling.  
	
	

	
	
	

	2.1.1.2 Access door.  
	
	

	
	
	

	2.1.1.3 Adapter frame assembly.
	 
	

	
	
	

	2.1.1.4 By-pass blower assembly.
	
	

	
	
	

	2.1.1.5 OML/IML covers and close out angles.
	
	

	
	
	

	2.2 SYSTEMS AND ELECTRICAL COMPONENT INSPECTIONS
	

	
	

	2.2.1 Visually inspect the following components:
	

	
	

	2.2.1.1 Wiring and wiring harness, connectors, back shells, circuit breaker, cockpit switch / indicator, differential pressure switch, filter maintenance Aid, and actuator.
	
	

	2.2.2 Function check the following:
	Table 1
	

	
	
	

	2.2.2.1 Circuit breaker
	
	

	
	
	

	2.2.2.2 Cockpit switch
	
	

	
	
	

	2.2.2.3 Indicator
	
	

	
	
	

	2.2.2.4 Differential pressure switch
	
	

	
	
	

	2.2.2.5 Filter maintenance aid and actuator
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0020.3 AAI REPLACEMENT SKID TUBES – AA-01145

	Note:  Removal of Skid Tubes from the helicopter is not required for inspection. If any damage is noted during the inspection, refer to Section 3.2, Repair.
	

	Note:  Particular care should be taken to inspect in the areas of the fasteners in the Skid Tubes and all attaching components.
	

	Note: The indications of corrosion are 1) corrosion deposits (a white or gray powder on aluminum), 2) pits in the aluminum surface, 3) blisters, bulging, or flaking of protective coatings.
	

	3.1 Inspect the skid tubes for scratches, nicks, dents, and corrosion. Refer to Section 3.1 .1 for damage and repair limits and to Figure 1 for damage and repair zones
	
	

	Note:  Only one damage rework is permissible per zone. If the damage limits are exceeded, the skid tube must be replaced.
	

	3.2 Visually inspect the Skid Shoes for damage. Refer to Section 3.2.3 for repair instructions.
	
	

	
	
	

	3.3 Inspect the wingwalk coating on the top 1/3 of each skid tube. Refer to Section 3.2.4 for repair instructions.
	
	

	
	
	

	C 0020.4 DART UTILITY BASKET – MMS-D206-540

	4.1 Inspect for damage or wear.
	
	

	
	
	

	4.2 Replace damaged or worn parts per drawing D206-540.
	
	

	
	
	

	C 0020.5 PARAVION DZUS SNOW DEFLECTORS – PR-407SD-100M

	5.1 Inspect snow deflectors assemblies for cracks or delaminating.
	
	

	
	
	

	5.2 Remove and replace as the above conditions exist.
	
	

	
	
	

	C 0020.6 ONBOARD CARGO HOOK – ICA 123-007-00

	
	
	

	6.1 Visually inspect for corrosion on the exterior of cargo hook and suspension system components. 
	Table 5-2
	

	Note:  Corrosion on the cargo hook side plates is cause for immediate overhaul. Additionally, any exfoliation corrosion in the upper attach lug area of the cargo hook is cause for immediate replacement of the side plate. Contact Onboard Systems for the latest revision of the cargo hook service manual.
	

	6.2 Move the cargo hook and the suspension system throughout their full ranges of motion and observe the manual and electrical release cables to ensure that they have enough slack. The cables must not be the stops that prevent the cargo hook or suspension from moving freely in all directions.
	
	

	
	
	

	6.3 Move the cargo hook carriage back and forth on the beam to ensure that it rolls freely and that there are no obstructions within the beam
	
	

	
	
	

	6.4 Move all suspension system components at their pivot points to verify that they rotate freely.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.5 Visually inspect the manual release cable for damage and security.
	
	

	
	
	

	6.6 Visually inspect the external electrical release harness and load weigh harness (if installed) for damage and security.
	
	

	
	
	

	C 0020.7 PARAVION ENGINE RELIGHT SYSTEM - PR-206ER-120M

	
	
	

	7.1 Verify system operation by placing the switch in the test position and listening for activation of the Ignition Exciter Assembly.
	
	

	
	
	

	7.2 Verify system operation by Arming the system when the aircraft is at flight idle (/ground Idle).  Caution light should activate.
	
	

	
	
	

	7.3 See the applicable Bell Model Maintenance Manual for Instructions to verify operation of the EXCITER ASSEMBLY and IGNITER ASSEMBLY.
	
	

	
	
	

	7.4 Verify that the warning light activates and press to test function works.
	
	

	
	
	

	C 0020.8 POST INSPECTION

	
	
	

	8.1 Inspect for operation and leaks.
	
	

	
	
	

	8.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	BHT-206L-FM-1
	

	
	
	

	8.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – C 0020 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


