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	1Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	
	
	
	
	
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C30 Series Operation and MM Table 607, BHT 206L Series MM-1 Chapter 5
NOTE: This inspection is for ONLY for engines operating with 3rd Generation oil 

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0051.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	B 0051.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	B 0051.3 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	3.1 Inspect the following:
	

	
	

	3.1.1 Engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	
	

	
	
	

	3.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	

	3.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened
	
	

	
	
	

	3.1.4 Compressor impeller leading edges for damage
	72-30-00, para 4. B.
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	3.1.5 Examine the engine cowling and doors for condition and security. Replace anti-chaff tape as needed.  
	Chapter 53
	

	
	
	

	3.1.5.1 Using a bright light and mirror, inspect exposed upper a lower edges of the joints between aluminum longerons and titanium engine pan.
	
	

	
	
	

	3.1.5.2 Check edge of sealant coating should is visible
	
	

	
	
	

	3.1.5.3 Any indications of corrosion or cracks is unacceptable.
	
	

	
	
	

	3.1.5.4 Examine engine pan area for evidence of loose fasteners and damage. Restore cracked or missing sealant form engine pan.
	
	

	
	
	

	3.1.5.5 Examine engine pan drains. Make sure that they are not clogged.
	
	

	
	
	

	3.1.6 Fluid flexible and rigid lines.
	
	

	
	
	

	3.1.7 Electrical harness.
	Chapter 96
	

	
	
	

	3.1.8 Exhaust stack.
	
	

	
	
	

	3.1.9 Engine mounts fittings and legs. Pay particular attention for loose fasteners
	Chapter 71
	

	
	
	

	3.2 Examine the firewalls for condition and security.
	Chapter 71
	

	
	
	

	3.3 Examine the engine pan drains. Make sure that they are not clogged. Restore broken or missing sealant from engine pan.
	
	

	
	
	

	3.4 Examine the engine controls for condition, correct operations and security.
	
	

	
	
	

	3.4.1 Check fuel control and power turbine governor for proper rigging.
	73-20-01/02,

PARA 2.C.
	

	3.5 All linkages for any looseness, condition and security.
	72-21-01 para 1.B.
	

	
	
	

	3.6 Check oil supply level.
	
	

	NOTE: If the engine has been idle for more than 15 minutes, motor the engine for 30 seconds to scavenge any oil that may have drained into the gearbox from the oil tank. Failure to completely scavenge the oil from the gearbox will cause a false indication of high oil consumption.
	72-00-00,Table 101

Troubleshooting items 17 and 18
	

	CAUTION: NORMAL ENGINES USE A MINIMAL AMOUNT OF OIL. HOWEVER, ANY SUDDEN INCRREASE IN OIL CONSUMTION IS INDICATIVE OF OIL SYSTEM PROBLEMS AND MUST BE CORRECTED.
	

	NOTE: Check oil supply level within 15 minutes of engine shutdown.


	

	3.7 Inspect for extension of scavenge oil filter bypass indicator. If indicator is extended, clean oil filter.
	72-60-00 para 1.C
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0051.4 ENGINE FUEL SYSTEM

	
	

	It is possible for the impending oil filter bypass indicator to extend during a start of a cold soaked engine, giving an erroneous indication of a dirty oil filter. If the impending filter bypass indicator is extended, run the engine until the oil is at operating temperature and push the indicator button in. If the button remains in throughout the normal speed range

of the engine, the filter does not require cleaning.


	

	Inspect for extension of impending fuel filter bypass indicator (if installed).  If indicator is extended, replace fuel filter. If contamination is present, inspect fuel filter in the fuel control and filter in the fuel nozzle. 
	73-10-05, para 2

73-20-02, para 5 A
	

	CAUTION:

WHEN THERE IS EVIDENCE THE AIRFRAME OR ENGINE FUEL FILTER HAS BEEN BYPASSED, THE GAS PRODUCER FUEL CONTROL INLET FILTER AND THE FUEL NOZZLE FILTER, MUST BE CLEANED. (REFER TO SPECIAL NSPECTIONS, 72--00--00, TABLE 608.) IF ANY CONTAMINATION IS FOUND IN THE FUEL NOZZLE FILTER, THE FUEL CONTROL MUST BE SENT TO AN AUTHORIZED REPAIR FACILITY FOR INTERNAL CLEANING. REFERENCE MUST ALSO BE MADE TO THE AIRFRAME MAINTENANCE MANUAL FOR FUEL SYSTEM MAINTENANCE FOLLOWING FUEL CONTAMINATION. 
	

	4.1 Examine airframe fuel filter assembly for evidence of leakage and security.
	Chapter 28
	

	Note: The following step does not apply to helicopters equipped with fuel filter assembly 222-366-621-103.
	

	4.1.1 Remove outlet port fitting from filter head.
	
	

	
	
	

	4.1.2 Pass a 0.020 inch (0.50 mm) wire through the bleed hole in outlet port side of filter head to ensure hole is not obstructed.
	
	

	
	
	

	4.2 Remove fuel filter canister.
	
	

	
	
	

	4.3 Remove and inspect fuel filter for any contaminants.
	
	

	
	
	

	4.4 Install new filter and o-rings.
	
	

	
	
	

	4.5 Reinstalled fuel filter canister.
	
	

	
	
	

	4.6 Remove fuel nozzle.
	73-10-03
	

	
	
	

	4.7 Disassemble fuel nozzle.
	73-10-03
	

	
	
	

	4.8 Cleaned and inspected fuel nozzle filter assembly.
	73-10-03
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.9 Visually inspect the outer combustion case (sheet metal and weld seams) for cracks. Pay particular attention to the weld seams in the area of the igniter plugs, dummy plug, drain valves, fuel nozzle bosses, armpit braze patch and adjacent areas. Use a bright light and mirror as necessary
	72--40--00

Para 2.B.(1), (2), (3) and (4)
	

	Note: Removal of the outer combustion case is not required. . Perform a Leak Tec check for installed OCC’s and an FPI for removed OCC’s.
	

	4.10 Assemble fuel nozzle.
	73-10-03
	

	
	
	

	4.11 Install fuel nozzle with proper number of spacers.
	73-10-03
	

	
	
	

	4.12 Purge airframe and engine fuel system as follows:
	Chapter 28
	

	
	
	

	4.12.1 Turn both fuel boost pumps ON.
	
	

	
	
	

	4.12.2 Depress airframe fuel filter bypass valve “press to test” button on fuel filter head until there is no evidence of air coming out the lower fuel filter drain port and out of the fuel filter outlet supply line.
	
	

	
	
	

	4.12.3 Then proceed with Rolls-Royce engine fuel system purging procedure.
	
	

	
	
	

	4.12.4 Ensure air is purged from fuel filter head.
	
	

	
	
	

	4.13 Verify illumination of airframe fuel filter caution light by depressing differential switch “press to test” button on filter head.
	Chapter 96
	

	
	
	

	B 0051.5 POST INSPECTION

	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.2 Make sure applicable servicing requirements have been carried out.
	Chapter 12
	

	
	
	

	5.3 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	5.4 Perform compressor fresh water rinse.
	72-30-00
	

	
	Para 5. A. 
	

	5.5 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	BHT-206L-FM-1
	

	
	
	

	5.6 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	5.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 206L Series AAIP 300 Hour / 12 Month – B 0051NT – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


