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	NO TOLERANCE 

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C30 Series Operation and MM Table 607, BHT 206L Series MM-1 Chapter 5

NOTE: This inspection is for ONLY for engines operating with 3rd Generation oil 

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0052.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	B 0052.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	B 0052.3 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	3.1 Inspect the following:
	

	
	

	3.1.1 Engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	
	

	
	
	

	3.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	

	3.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened
	
	

	
	
	

	3.1.4 Engine inlet bellmouth for obstruction and general condition.
	Chapter 71
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	3.1.5 Examine the engine cowling and doors for condition and security. Replace anti-chaff tape as needed.  
	Chapter 53
	

	
	
	

	3.1.6 Fluid flexible and rigid lines. Pay particular attention for chafing damage and kinked lines.
	Chapter 71
	

	
	
	

	3.1.7 Electrical harness.
	Chapter 96
	

	
	
	

	3.1.8 Exhaust stack for condition and security.
	Chapter 71
	

	
	
	

	3.1.9 Engine mounts fittings and legs.
	Chapter 71
	

	
	
	

	3.1.10 Examine the firewalls for condition and security.
	Chapter 53
	

	
	
	

	3.1.11 Examine the engine pan drains. Make sure that they are not clogged. Restore broken or missing sealant from engine pan.
	
	

	
	
	

	3.1.12 Examine the engine controls for condition, correct operations and security.
	
	

	
	
	

	3.1.12.1 Inspect fuel control lever bolt hole and bolt for wear. Replace parts as required.
	Chapter 76
	

	
	
	

	3.1.13  Linkage for any looseness.
	
	

	
	
	

	3.2 Perform FCU Screw Inspection.
	CEB A-73-3075
	

	
	
	

	B 0052.4 STARTER-GENERATOR

	
	
	

	4.1 Remove starter generator. Examine mounting pad, cooling duct and retention clamp for condition.
	Chapter 71
	

	4.2 Examine the components as follows for condition, security and wear:
	
	

	
	
	

	4.2.1 Brushes
	
	

	
	
	

	4.2.2 Commutator. Replace starter generator if not smooth and bright or if showing excessive wear.
	Chapter 96
	

	
	
	

	4.2.3 Splines on starter generator shaft and engine gear shaft
	Chapter 71
	

	
	
	

	B 0052.5 ENGINE CONTROLS

	
	
	

	5.1 Examine engine controls for condition and security.
	Chapter 76
	

	5.2 Verify operation of engine N1 control as follows:
	
	

	
	
	

	5.2.1 Ensure proper throttle friction.
	
	

	
	
	

	5.2.2 Check freedom of full throttle grip travel and idle release operation. Return to closed position. Check copilot throttle if installed.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.2.3 Ensure fuel control stop lever contact with minimum and maximum stops before throttle grip reaches travel limit.
	
	

	NOTE: If dual controls are installed, it is permissible for pointer to be 0.078 inch (1.98 mm) below 40° mark when copilot twist grip is used.
	

	5.2.4 Rotate throttle grip to idle detent, fuel control pointer should be no more than 0.01 inch (0.25 mm) below the 40° mark on the quadrant.
	
	

	
	
	

	5.2.5 Verify control linkage for excessive looseness, lost motion, and binding.
	
	

	
	
	

	5.3 Verify operation of engine N2 control as follows:
	
	

	
	
	

	5.3.1 Position N2 governor actuator to full DECREASE (extended).
	
	

	
	
	

	5.3.2 Lift collective stick full up.
	
	

	
	
	

	5.3.3 Position N2 governor actuator to full INCREASE (retracted).
	
	

	
	
	

	5.3.4 Verify for clearance between governor stop and lever stop arm.
	
	

	
	
	

	5.3.5 Lower collective stick full down.
	
	

	
	
	

	5.3.6 Position N2 governor actuator to full DECREASE (extended).
	
	

	
	
	

	5.3.7 Verify for clearance between governor stop and lever stop arm.
	
	

	
	
	

	5.3.8 Verify control linkage for excessive looseness, lost motion, and binding.
	
	

	
	
	

	5.4 Check oil supply level.
	
	

	NOTE

If the engine has been idle for more than 15 minutes, motor the engine for 30 seconds to scavenge any oil that may have drained into the gearbox from the oil tank. Failure to completely scavenge the oil from the gearbox will cause a false indication of high oil consumption.
	72-00-00,Table 101

Troubleshooting 
items 17 and 18
	

	CAUTION:  NORMAL ENGINES USE A MINIMAL AMOUNT OF OIL. HOWEVER, ANY SUDDEN INCRREASE IN OIL CONSUMTION IS INDICATIVE OF OIL SYSTEM PROBLEMS AND MUST BE CORRECTED.
	

	NOTE

Check oil supply level within 15 minutes of engine shutdown.
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.5 Inspect for extension of scavenge oil filter bypass indicator. If indicator is extended, clean oil filter.
	72-60-00 para 1.C
	

	
	
	

	It is possible for the impending oil filter bypass indicator to extend during a start of a cold soaked engine, giving an erroneous indication of a dirty oil filter. If the impending filter bypass indicator is extended, run the engine until the oil is at operating temperature and push the indicator button in. If the button remains in throughout the normal speed range

of the engine, the filter does not require cleaning.

	

	5.6 Inspect for extension of impending fuel filter bypass indicator.  If indicator is extended, replace fuel filter. If contamination is present, inspect fuel filter in the fuel control and filter in the fuel nozzle. 
	73-20-02, para 5 A.
	

	5.7 On power and accessory gearbox cover, check the applied torque on all turbine and exhaust collector support-to-gearbox retaining nuts.


	72-50-00, Para 1.B.
	

	NOTE: Torque must be 120-150 lb in.  Compliance with M250 CEB--72--3017 cancels this periodic inspection requirement.
	

	B 0052.6 POST INSPECTION

	
	
	

	6.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.2 Make sure applicable servicing requirements have been carried out.
	Chapter 12
	

	
	
	

	6.3 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	6.4 Perform compressor fresh water rinse.
	72-30-00
	

	
	Para 5. A. 
	

	6.5 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	BHT-206L-FM-1
	

	
	
	

	6.6 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	6.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 206L Series AAIP 300 Hour / 12 Month  – B 0052NT – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


