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	Revision:
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	B 0055NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	NO TOLERANCE 

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C30 Series Operation and MM Table 607, BHT 206L Series MM-1 Chapter 5

NOTE: This inspection is for ONLY for engines operating with 3rd Generation oil 

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0055.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce M250-C30 Operations and Maintenance Manual).
	250-C30 MP
	

	
	
	

	B 0055.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0055.3 FREEWHEEL ASSEMBLY

	5.1 Examine the freewheel assembly for condition, leaks and security.
	Chapter 63
	

	5.2 Examine the freewheel chip detector for metal particles.
	
	

	
	
	

	5.3 Examine the electrical circuit of the chip detectors for continuity.
	Chapter 96
	

	
	
	

	B 0055.4 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	4.1 Inspect the following:
	

	
	

	4.1.1 Engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	
	

	
	
	

	4.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened
	
	

	
	
	

	4.1.4 Without disassembly, turbine, exhaust collector supports and the air tubes for cracks, buckling and general condition.
	
	

	
	
	

	4.1.5 Examine the duct and the clamp for condition and security.
	
	

	
	
	

	4.1.6 Without disassembly, check the compressor discharge air tubes. Inspect for air leaks, dents, cracks, chafing, and proper clamping.
	72--40--00,

Table 203.
	

	
	
	

	4.1.7 Inspect compressor mount for cracks.
	72--00--00, PARA 1.A. (3),Engine--Inspection/
	

	
	Check 3
	

	4.1.8 Fuel system for evidence of leakage – Check condition and security of fittings and tubing
	
	

	
	
	

	4.1.9 Engine mount, fittings and legs for condition and security.
	Chapter 71
	

	
	
	

	4.1.10 Electrical harness for loose, chafed, frayed, or broken wires, loose connectors.
	
	

	
	
	

	4.1.11 Perform FCU Screw Inspection.
	CEB A-73-3075
	

	
	
	

	4.1.12 For aircraft with external energy absorbing ring installed, inspect ring upper bracket for cracks.
	
	

	
	
	

	4.1.13 Engine mount for condition and security.
	
	

	
	
	

	4.1.14 Inspect and perform operational check of thermocouple assembly. (TOT/MGT).
	77-20-01, para 2.B
	

	
	Chapter 95
	

	4.2 Check oil supply level.
	
	

	
	
	

	NOTE: If the engine has been idle for more than 15 minutes, motor the engine for 30 seconds to scavenge any oil that may have drained into the gearbox from the oil tank. Failure to completely scavenge the oil from the gearbox will cause a false indication of high oil consumption.
	72-00-00,Table 101
Troubleshooting items 17 and 18
	

	CAUTION: NORMAL ENGINES USE A MINIMAL AMOUNT OF OIL. HOWEVER, ANY SUDDEN INCRREASE IN OIL CONSUMTION IS INDICATIVE OF OIL SYSTEM PROBLEMS AND MUST BE CORRECTED.

NOTE: Check oil supply level within 15 minutes of engine shutdown.
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.3 Inspect for extension of scavenge oil filter bypass indicator. If indicator is extended, clean oil filter.
	72-60-00 para 1.C
	

	It is possible for the impending oil filter bypass indicator to extend during a start of a cold soaked engine, giving an erroneous indication of a dirty oil filter. If the impending filter bypass indicator is extended, run the engine until the oil is at operating temperature and push the indicator button in. If the button remains in throughout the normal speed range

of the engine, the filter does not require cleaning.


	

	4.4 Inspect the anti-icing solenoid valve and bleed air valve for loose, chafed, frayed or broken wires, loose connections and security of attachment.
	Chapter 75
	

	
	
	

	4.5 Remove the Pc filter.
	73--20--03.
	

	
	PARA 2. and 3
	

	4.6 Clean and inspect the Pc filter.
	
	

	
	
	

	4.7 Reinstall the Pc filter. 
	
	

	NOTE: If engine performance deteriorates, Pc filter cleaning interval may have to be reduced.
	

	4.8 On power and accessory gearbox cover, check the applied torque on all turbine and exhaust collector support-to-gearbox retaining nuts.


	72-50-00, Para 1.B.
	

	NOTE: Torque must be 120-150 lb in.  Compliance with M250 CEB--72--3017 cancels this periodic inspection requirement.
	

	B 0055.5 POST INSPECTION

	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.2 Make sure applicable servicing requirements have been carried out.
	Chapter 12
	

	
	
	

	5.3 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	5.4 Perform compressor fresh water rinse.
	72-30-00
	

	
	Para 5. A. 
	

	5.5 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	BHT-206L-FM-1
	

	
	
	

	5.6 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	5.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 206L Series AAIP 300 Hour / 12 Month – B 0055NT – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


