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	SECTION:
	
	B 0350NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 12 MONTH ENGINE OIL SERVICING

	NOTE:
	
	No  Tolerance



	 Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C30 Operation and Maintenance Manual.

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

INITIALS

	B 0350.1 GENERAL

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C30 MP
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C30 MP
	

	B 0350.2 ENGINE

	
	72-00-00, Para
	

	2.1 Drain the oil system and refill.


	8.D., Engine Servicing.
	

	Applicability – Only for engines running Third Generation oils
	

	2.2 Replace Purolator Nicad Filter.
	SB 082500.4
	

	
	
	

	B 0350.3 POST INSPECTION

	3.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	3.2 Make sure applicable servicing requirements have been carried out.
	Chapter 12
	

	3.3 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	3.4 Perform the scavenge oil filter bypass function check. (RR CSL3116)
	Facet Service Bulletin No. 090589
	

	3.5 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	BHT-206L-FM-1
	

	3.6 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	3.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 206L Series AAIP 300 Hour / 12 Month – B 0350NT – Engine oil servicing and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


