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	C 0010 ICA OF INSTALLED EQUIPMENT
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	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0010.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	C  0010.2 ARROW AVIATION GARMIN GTX 330 INSTALL – AA-206-GARMEN

	
	
	

	2.1 Check control head for loose, broken or worn parts.
	
	

	
	
	

	2.2 Check antenna’s for loose, broken or worn parts.
	
	

	
	
	

	2.3 Inspect antenna for condition and security
	
	

	
	
	

	2.4 Inspect control head for security and condition.  
	
	

	
	
	

	2.5 Inspect circuit breaker for correct operation.
	
	

	
	
	

	C  0010.3 PARAVION BLEED AIR CABIN HEATER – PR-206H-906H  

	
	

	3.1 ACCESS AREAS
	

	
	

	3.1.1 Remove cowlings and access panels as necessary to follow the bleed air tubing assemblies.
	
	

	
	
	

	3.1.2 Inspect valve for mounting security.
	
	

	
	
	

	3.1.3 Inspect valve for freedom of operation. Disassemble and clean if excessive operating friction exists.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	CAUTION: If tubing insulation is discolored, it must be pulled back to inspect tubing for a possible crack. Remove and replace the tubing assembly if a crack is found. If no discrepancy is found reposition insulation over tube.  If the fire-sleeve insulation is broken or torn, replace the tube assembly.
	

	
	
	

	3.1.4 Inspect bleed plumbing for insulation, security, and clearance with flight controls (.50" min).
	
	

	
	
	

	3.1.5 Verify security of control knob and placard.   
	
	

	
	
	

	3.1.6 The inlet end of the heater circuit contains an acoustical dampener/cabin air filter. This filter should be changed annually (prior to start of the heating season), or more often if it becomes blocked.
	
	

	NOTE:  The filter (P/N S-9501EC-7) can be ordered through the customer service department of Paravion® Technology, Inc.  
	

	3.1.7 The flexible ducting which connects the ejectors, and air inlet/outlet adapters contains an acoustical liner. This liner should be inspected annually to insure free air passage of the ducts.
	
	

	
	
	

	3.1.8 For compressor wash, turn heater valve off. The S-5030-2 valve assy will drain any water in the bleed air lines.
	
	

	
	
	

	C  0010.4 PRECISE FLIGHT PULSELITE – 00PMAN0002

	
	

	4.1 Check Pulselite for Proper Operation
	

	
	

	4.1.1 Connect Ground Power to the Aircraft or power the aircraft on the ramp.
	
	

	
	
	

	4.1.2 Activate pulselite system
	
	

	
	
	

	4.1.3 Observe that the external lights connected to the pulselight system are flashing.
	
	

	NOTE: These lights may be the landing, taxi, recognition logo, hover, or runway turnoff lights depending on installation. 
	

	4.1.4 Switch the external lights connected to the Pulselite system to steady on. 
	
	

	
	
	

	4.1.5 Observe that the external lights connected to the pulselight system are now on steady.
	
	

	
	
	

	4.2 Switch the pulselight control unit OFF and the connected landing / taxi / recognition / hover lights to OFF and observe that the external lights are off.
	
	

	
	
	

	4.3 Check wiring and connections for security and chaffing.
	
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0010.5 AAI Pc SAFETY VALVE KIT – AA-99066

	
	
	

	5.1 Check the Pc Safety Valve™ Knob for security and force required to rotate. If the knob is loose or difficult to rotate (cannot be actuated by hand), return the Pc Safety Valve TM to Aeronautical Accessories Inc. for repair/overhaul.
	
	

	
	
	

	5.2 Inspect all connecting lines to the Pc Safety Valves TM for chafing, dents (not to exceed .125 in. depth or having sharp radius ), or cracking (none allowed), replace if damaged beyond limits.
	
	

	
	
	

	5.3 Check for the proper torque on each Pc line B-nut (80-120 in-lbs).
	
	

	CAUTION: Lines should be tightened only when the proper free state alignment of lines is obtained.
	

	5.4 Examine the Decals and the Flow Tape on the connecting lines for discoloration or cracking. Replace any Decal or Flow Tape that is not legible.
	
	

	
	
	

	5.5 Inspect the Safety Clips and the Valve contact surfaces for wear (not to exceed .005) Report any anomalies to Aeronautical Accessories Inc. (Phone 423-538-5151). Ensure the Pc Safety Valve TM Knob is Safety Clipped in the open position per Figures 4 through 6.
	
	

	
	
	

	5.6 Inspect the Bracket Assembly for cracks in the Bracket or welds (none allowed). Check the safety wire on the Valve to Bracket attaching Nut and the torque on the Pc Filter Retaining Clamp Bolt (30-40 in-lbs).
	
	

	
	
	

	C  0010.6 DART AVIONICS CONSOLE – D206-549

	
	
	

	6.1 Inspect all areas for mechanics damage i,e, cracking and/or hole elongation. Replace any damaged or worn parts ICA chp 25.
	Chapter 5
	

	
	
	

	6.2 Check that all screws are securely fastened.
	
	

	
	
	

	6.3 Touch up paint as required with matte black per MIL-L-6805.
	
	

	
	
	

	C  0010.7 POST INSPECTION

	
	
	

	7.1 Inspect for operation and leaks.
	
	

	
	
	

	7.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	BHT-206L-FM-1
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – C 0010 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


