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1
INSPECTIONS EXCLUDED FROM AAIP 
Since the AAIP inspection program is not intended to prescribe maintenance functions, the following items will be tracked separately in the aircraft status report. 

A. Hand-held Fire Extinguishers
B. Static System and Altitude Reporting System per 14 CFR 91.411.
C. ATC Transponder Test and Inspections per 14 CFR 91.413.
D. Inspect Pitot-Static System per 14 CFR 91.411/413 
E. 36 Month Hydrostatic Retest of Emergency Floatation Gas Cylinder per AA-ICA407-11
F. 1500 Hour Mast Overhaul BHT-206L Series MM-1  Table 5-40

G. 2250 Hour / 60 Month Transmission Overhaul BHT-206L Series MM-1  Table 5-41

H. 3000 Hour Tail Rotor Gearbox Overhaul BHT-206L Series MM-1  Table 5-42

I. 300 Hour N1 and N2 Tach Gen Spline Insp/lube BHT-206L Series MM-1  Para 5-23 Item 16

J. Engine Wash – Rolls-Royce M250-C30 Series MM 72-30-00 Para 5.B

K. Freewheeling Unit 60 Month Insp BHT-206L Series MM-1  Para 5-36

L. 1200 Hr Tailboom Insp - Deleted. Now tracked as AD2002-25-07

M. Battery Recondition I/A/W BHT-ALL-SPM

N. 300 Tail Rotor Hub and Blade Track and Balance - BHT-206L-MM Chp 5-21

O. 150/300 hr Fuel Nozzle Cleaning/Inspections - Rolls-Royce M250-C30 Series MM 73-10-03 Para 5.B
P. Starter Generator 300 hour Insp -   BHT-206L Series MM-1  Chp 71
Q. 1200 Main Rotor Hub Inspection – BHT-206L-CR&0
R. 1500 Hour KaFlex Drivshaft Insp (Applicable to L3 only) – KAMATICS SIN3052 As Revised
