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	08/01/16

	SECTION:
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 206L MM-1 Chapter 4, 5, 12  BHT 206L MMS-6
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0056.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	A 0056.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0056.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this AAIP inspection.
	CSSD-PSE-87-001 
	

	3.2 
	
	

	A 0056.4 FUSELAGE (EXTERIOR)

	
	
	

	4.1 Examine the following; 
	Chapter 53
	

	
	
	

	4.1.1 Aft fuselage for dents, cracks, corrosion, delamination, lose or missing rivets and condition.
	Chapter 53
	

	
	
	

	4.1.2 Aft fuselage for indications of fuel or oil leaks.
	
	

	
	
	

	4.1.3 Fuel cap for condition and security.
	Chapter 28
	

	
	
	

	4.1.4 Grounding plug for condition.
	Chapter 96
	

	
	
	

	4.1.5 All fuselage drains for condition and freedom from obstructions.
	Chapter 6
	

	
	Chapter 53
	

	4.1.6 Heater and/or air conditioning inlets and outlets for cleanliness and absence of obstructions, (if installed).  
	Applicable Service
Instruction
	

	
	
	

	4.1.7 Examine baggage compartment door, seal, and latches for operation, condition, and security. 
	Chapter 53
	

	
	
	

	4.1.8 Verify operation of the baggage door ajar caution light, (if installed).
	Chapter 96
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.1.9 Forward fuselage for condition. 
	Chapter 53
	

	
	
	

	4.1.10 All cabin doors for condition and security. Give special attention to the following;
	Chapter 52
	

	
	
	

	4.1.10.1 Hinges 
	
	

	
	
	

	4.1.10.2  Seals
	
	

	
	
	

	4.1.10.3  Latches for proper adjustment, positive locking and wear
	
	

	
	
	

	4.1.10.4  Windows
	
	

	
	
	

	4.1.10.5  Handles
	
	

	
	
	

	4.1.11 External power door and receptacle for condition and security
	Chapter 53
	

	
	
	

	4.1.12 Battery compartment door, door seal and attachment for condition and security. 
	
	

	
	
	

	4.1.13 Components in battery compartment for condition and security.
	Chapter 52
	

	
	
	

	4.1.14 Cabin entry steps (if installed) for condition and security.
	Chapter 32
	

	
	
	

	4.1.15 Windshields and skylights for condition.
	Chapter 52
	

	
	
	

	4.1.16 Upper fuselage for evidence of water leaks.
	Chapter 53
	

	
	
	

	4.1.17 Lower fuselage for indication of fuel leaks, dents, crack, corrosion, delaminations, lose or missing rivets and condition
	
	

	
	
	

	4.1.18 All fuselage sealant joints for condition. Restore sealant as necessary.
	
	

	
	
	

	4.2 Drain moisture from pitot and static piping installation.
	Chapter 95
	

	
	
	

	A 0056.5 ELECTRICAL AND AVIONICS

	
	
	

	5.1 Examine antennas for condition and security.
	Chapter 96
	

	
	Chapter 97
	

	5.2 Examine all components, electrical wiring, cables, and connectors for chafing, general condition, and security.
	
	

	
	
	

	5.3 Examine all optional equipment installed in the aft fuselage area for condition and security.
	
	

	
	
	

	5.4 Verify proper operation of fuel sump drain valve switch.
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0056.6 POST INSPECTION

	
	
	

	6.1 Ensure applicable servicing requirements have been carried out.
	Chapter 12
	

	
	
	

	6.2 Check oil level of transmission, hydraulic tank, engine and tail rotor gearbox prior to running helicopter.
	
	

	
	
	

	6.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	BHT-206L-FM-1
	

	
	
	

	6.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.5 Perform Functional Check Flight if required per Bell 206L Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	6.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – A 0056 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




