	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0053.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0053.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	


	A 0053.3 STARTER-GENERATOR

	
	
	

	3.1 Examine the duct and the clamp for condition and security.
	
	

	
	
	

	A 0053.4  OIL SYSTEM

	
	
	

	4.1 Examine the engine/transmission oil cooling system for condition, leaks, and security.
	Chapters 63 & 79
	

	
	
	

	4.2 Examine the components as follows:
	
	

	
	
	

	4.2.1 Fluid flexible and rigid lines.
	
	

	
	
	

	4.2.2 Electrical harness.
	
	

	
	
	

	4.2.3 Oil tank and cooler.
	
	

	
	
	

	4.2.4 Oil cooler blower assembly.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0053.5  MAIN ROTOR SYSTEM

	
	
	

	5.1 Examine the main rotor system for condition and security.
	Chapters 62
	

	
	
	

	5.2 Examine the components as follows:
	

	
	

	5.2.1 Hub assembly
	
	

	
	
	

	5.2.2 Main rotor blades
	
	

	
	
	

	5.3 Examine the Swashplate and support for condition and security.  Examine the components as follows:
	Chapter 67
	

	
	
	

	5.3.1 [bookmark: _GoBack]Mast for cleanliness.
	Chapter 63
	

	
	
	

	5.3.2 Rotate the outer ring. Examine the duplex bearings for condition (do this check before you lubricate the duplex bearing).
	Chapter 67
	

	
	
	

	5.3.3 Seals for sign of too much grease leakage.
	
	

	
	
	

	5.3.4 Pivot sleeve for wear and damage.
	
	

	
	
	

	5.3.5 Collective lever.
	
	

	
	
	

	5.3.6 Swashplate drive assembly.
	
	

	
	
	

	5.3.7 Perform a Swashplate friction adjustment.
	
	

	NOTE: If friction has to be adjusted, it must be checked again in 10 to 25 hours.
	Chapter 5 & 
Chp 67-165
	

	A 0053.6 POST INSPECTION

	
	
	

	6.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	6.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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	A 0053 – AIRFRAME INSPECTION PROGRAM
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	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	



A 0053.7 
Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0053 – 300 Hour / 12 Month and was determined to be in an airworthy condition.
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	N
	End
	
	Aircraft Ending Total Time:
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	Aircraft Ending Total Cycles:
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	Certificate Type & No:
	




