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	SECTION:
	
	A 0630 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	600 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0630.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0630.2 MAIN ROTOR  HUB AND BLADE

	
CAUTION

FOR HELICOPTERS OPERATIING IN CORROSIVE ENVIRONMENT OUR EXTREME ENVIRONMENTAL CONDITIONS, THE RECOMMENDED INTEVAL FOR INSPECTION AND LUBRICATION MUST BE REDUCED TO 600 HOURS OR 6 MONTHS.
	
	

	2.1 Remove main rotor blades from the main rotor hub assembly.
	Chapter 62
	

	
	
	

	2.2 Remove oil and grease from the main rotor hub, blades, and blade bolts with clean cloths (C-516) dampened with aliphatic naphtha (C-305) or drycleaning solvent (C-304).
	
	

	
	
	

	2.3 Clean main rotor hub and blades with cleaning compound (C-318). Thoroughly rinse with fresh water and dry with clean cloth.
	
	

	
	
	

	2.4 Examine main rotor hub and blades for evidence of corrosion.  Pay particular attention to the surface around the blade bolt bushings installed in the grip tangs.
	Chapter 62
	

	
	
	

	2.5 If installed, examine the expandable blade bolts for condition and security.
	Chapter 62-3A
	

	
	
	

	2.6 If installed, lubricate the expandable blade bolts (2 Places) – C-561
	Chapter 12
	

	
	
	

	2.7 Install main rotor blades onto the main rotor hub assembly.
	Chapter 62-48
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0630.3 POST INSPECTION

	
	
	

	3.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	3.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	3.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	3.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0630 – 600 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




