	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 5
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1710.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 1710.2 MAIN ROTOR MAST INSPECTION

	
	
	

	2.1 Perform Mast 12 Month Inspection
	Chapter 63-6
	

	
	
	

	2.1.1 Remove Mast nut
	Chapter 62
	

	
	
	

	2.1.2 Remove the plastic cap plug from the mast diameter.
	
	

	
	
	

	2.1.3 Use a bright light and examine the mast inside diameter for corrosion and condition of the protective coating.
	
	

	NOTE
If there is corrosion, the mast must be removed, inspected and 
repaired as per the BHT-407-CR&O
	
	

	2.1.4 Install plastic cap plug
	
	

	CAUTION
DO NOT APPLY THIXOGEASE TO THE THREADS 
OF THE MAST OR MAST NUT
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	2.2 Remove the main rotor hub.
	Chapter 62
	

	NOTE
The mast pole may have been re-identified to one of the following after repair by Bell Helicopter Textron (BHT):
· 407-040-038-111R (replacement of the tungsten carbide coating by wear sleeve 406-040-026-103)
· 407-040-038-111T (repair of the tungsten carbide coating)
· 407-040-038-111T1 (expanded repair of the tungsten carbide coating)
	
	

	2.3 For the mast pole 407-040-038-101, -105, -109, or -111R, examine the lower cone clamping journal for sleeve debonding, voids, and corrosion.
	BHT-407-CR&O
Chapter 63
	

	
	
	

	2.4 For the mast pole 407-040-038-111, -111T, or -111T1, examine the lower cone clamping journal for corrosion.
	BHT-407-CR&O
Chapter 63
	

	
	
	

	2.5 Install the main rotor hub.
	Chapter 62
	

	
	
	

	2.5.1 Apply a thin layer of Thixogrease (C-561) to the surface of the upper cone that contacts the mast nut.
	
	[bookmark: _GoBack]

	NOTE
Do not disturb the lower cone hardware (If applicable)
	

	2.6 Install the mast nut
	Chapter 62
	

	
	
	

	2.7 Ensure the following entry is made in the aircraft logbook:
	
	

	“Torque check due after initial ground run for removal and installation of Main Rotor Hub Mast Nut. (Date, ACFT current TT, signature and certificate number”
	

	2.8 Ensure the following entry is made in the aircraft logbook:
	
	

	“Torque check due between (insert ACTT plus 1 hour) and (insert ACTT plus 5 hours) for removal and installation of Main Rotor Hub Mast Nut. (Date, ACFT current TT, signature and certificate number”
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	REFERENCE
	

	
	
	

	A 1710.3 POST INSPECTION

	
	
	

	3.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	3.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	3.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	3.4 Check torque the mast nut.
	Chapter 62
	

	
	Fig 62-32
	

	3.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 1710 – 12 Month Mast Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




