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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0120.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	C  0120.2 AAI CARGO MIRROR – AA-00120

	NOTE: Removal of Cargo Mirror from helicopter is not required for inspection. If any damage is noted during inspection, refer to Section 4.3 Repair or Section 5.0 Troubleshooting Information.
	

	
	
	

	2.1 Inspect Support Assembly with Mirror for nicks, scratches, dents, corrosion, cracks or broken glass.
	
	

	NOTE: The indications of corrosion are 1) corrosion deposits (a white or gray powder on aluminum or rust colored deposits on steel), 2) pits in aluminum or steel surfaces, 3) blisters, bulging or its flaking of protective coatings.
	

	2.2 Rotate Control Cable T-Handle counter-clockwise to unlock and verify proper operation and deployment/extension of the mirror.
	
	

	
	
	

	2.3 Push Control Cable T-Handle in to retract mirror and rotate T-Handle clockwise to lock.
	
	

	
	
	

	2.4 Ensure door latches are properly positioned on latch tabs on airframe.
	
	

	
	
	

	2.5 Inspect all Decals for condition.
	
	

	
	
	

	C  0120.3 AAI  PREFLIGHT STEP/HANDLE – AA-00123

	
	
	

	3.1 Inspect the Step/Handle for nicks, scratches, dents, corrosion, and cracks.
	Section 3.2
	

	NOTE: The indications of corrosion are 1) corrosion deposits (a white or gray powder on aluminum or rust colored deposits on steel), and in 2) pits in the aluminum or steel surface, 3) blisters, bulging or flaking of protective coatings.
	

	3.2 Inspect the attaching fasteners for security.
	
	

	
	
	

	3.3 Check the torque value on the attaching hardware and adjust as required to 50-70 in/lbs.
	
	

	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0120.4 AAI  FOLDING MAINTENANCE STEP – AA-00126  

	
	
	

	4.1 Inspect the folding maintenance step for nicks, scratches, dents, corrosion, and cracks or broken glass.
	Section 3.2
	

	NOTE: The indications of corrosion are 1) corrosion deposits (a white or gray powder on aluminum or rust colored deposits on steel), and in 2) pits in the aluminum or steel surface, 3) blisters, bulging or flaking of protective coatings.
	

	4.2 Check the folding function of this step.
	
	

	
	
	

	4.3 Inspect the attaching fasteners for security.
	
	

	4.4 Check the torque value on the attaching hardware and adjust as required to 50-70 in/lbs.
	
	

	
	
	

	4.5 Inspect Baggage Door Retention Strap for tears or frays and check attaching fasteners for security.
	
	

	
	
	

	C  0120.5 AAI CONSOLE INSTALLATION - AA-00131

	NOTE: Removal of door from helicopter is not required for inspection. If any damage is noted during inspection, refer to Section 3.2 Repair or Section 4.0 Troubleshooting information.
	

	5.1 Inspect for proper installation of hardware, any unusual wear patterns, corrosion and/or damage (scratches, nicks, dents, cracks). Ensure the damage limits presented in Table 1 are not exceeded and replace parts as required.
	Section 3.1
	

	NOTE: The indications of corrosion are 1) corrosion deposits (a white or gray powder on aluminum or rust colored deposits on steel), and in 2) pits in the aluminum or steel surface, 3) blisters, bulging or flaking of protective coatings.
	

	5.2 Inspect the attaching fasteners for security.
	
	

	
	
	

	5.3 Inspect Avionics equipment for security.
	
	

	
	
	

	C  0120.6 AAI BAGGAGE COMPARTMENT PROTECTORS - AA-02008

	
	
	

	6.1 Inspect the Baggage Compartment Protectors for scratches, dents, cracks, or deformation.
	
	

	
	
	

	6.2 Inspect the Baggage Compartment Protectors for security.
	
	

	
	
	

	C  0120.7 AAI STEERABLE LANDING LIGHT – F08-72000

	
	
	

	7.1 Verify that both LDG LT POWER and LDG LT CONTROL circuit breakers, located in overhead circuit breaker panel, are closed.
	Section 4.1
	

	
	
	

	7.2 Hold four-position thumb-switch, located in pilot's collective box, forward in the EXT (Alt: EXTEND) position. Verify that the Steerable Landing Light drives to a 90° position (approximate) at full travel.
	
	

	
	
	

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	7.3 At this time check Steerable Landing Light unit for security of attachment and for general overall condition.
	
	

	
	
	

	7.4 Set LOG LT (Alt: LANDING LIGHT) ON I OFF I STOW switch, located in pilot's collective box to ON. Verify that Steerable Landing Light illuminates
	
	

	
	
	

	7.5 Hold four-position thumb-switch aft in the RETR (Alt: RETRACT) position. Verify that Steerable Landing Light retracts completely.
	
	

	
	
	

	7.6 Hold four-position thumb-switch forward in the EXT (Alt: EXTEND) position until Steerable Landing Light is partially extended.
	
	

	
	
	

	7.6.1 Hold four-position thumb-switch in the LEFT position. Verify that light rotates full travel to the left.
	
	

	
	
	

	7.6.2 Hold four-position thumb-switch in the RIGHT position. Verify that light rotates full travel to the right.
	
	

	
	
	

	7.7 Set LDG LT (Alt: LANDING LIGHT) ON I OFF I STOW switch to OFF. Verify that light goes off.
	
	

	
	
	

	7.8 Set LDG LT (Alt: LANDING LIGHT) ON I OFF I STOW switch to STOW. Verify that light retracts to stowed position.
	
	

	
	
	

	7.9  Verify that both LDG LT POWER and LDG LT CONTROL circuit breakers are closed.
	
	

	
	
	

	7.10 Verify that the FWD REC (Alt: FWD RECOG LIGHT) circuit breaker, located in overhead circuit breaker panel, is closed. 
	
	

	
	
	

	7.11  Set FWD REC (Alt: FWD RECOG LIGHT) switch, located in the pilot's collective box, to ON. Verify that fixed landing light illuminates.
	
	

	
	
	

	7.12  Set FWD REC (Alt: FWD RECOG LIGHT) switch to OFF. Verify FWD REC (Alt: FWD RECOG LIGHT) circuit breaker closed.
	
	

	
	
	

	C  0120.8 AIR COMM ENGINE COMPARTMENT BLEED AIR SYSTEM – 407H-500M-1

	
	
	

	8.1 Remove system drain valve disassembled and clean.
	
	

	
	
	

	8.2 Check for corrosion on valve and any damage to the o-ring.  
	
	

	
	
	

	8.3 Check the function of the automatic drain valve:
	
	

	
	
	

	8.3.1 Turn heater full on.  Check and valve is closed.
	
	

	NOTE:  Slight leakage is permitted.
	

	8.4 Inspect bleed air hose and tube assemblies for evidence of damage or deterioration.  Replace if any of the above exists.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0120.9 BELL BARRIER FILTER SYSTEM – AFS-BH407-IBF-KIT-ICA

	
	

	9.1 FILTER ASSEMBLY INSPECTION - Visual
	

	
	

	9.1.1 Inspect the following filter assembly components;
	

	
	

	9.1.1.1 Engine wash tube assembly seals and fasteners.
	Table 1
	

	
	
	

	9.1.1.2 Check the filter media for tears, punctures, uneven or damage plate pleats.
	
	

	
	
	

	9.1.1.3 Check seals for tears and/or damage.
	
	

	
	
	

	9.1.1.4 Check frame components or corrosion, cracks, distortion near holes.
	
	

	
	
	

	9.1.1.5 Checked for missing or damaged fasteners.
	
	

	
	
	

	9.2 STRUCTURAL COMPONENT INSPECTIONS
	

	
	

	9.2.1 Visually inspect the following components:
	

	
	

	9.2.1.1 Air induction cowling.  
	
	

	
	
	

	9.2.1.2 Access door.  
	
	

	
	
	

	9.2.1.3 Adapter frame assembly.
	 
	

	
	
	

	9.2.1.4 By-pass floor assembly.
	
	

	
	
	

	9.2.1.5 OML/IML covers and close out angles.
	
	

	
	
	

	9.3 SYSTEMS AND ELECTRICAL COMPONENT INSPECTIONS
	

	
	

	9.3.1 Visually inspect the following components for deformation, buckling, corrosion, cracks, dates, tears or other signs of damage:
	

	
	

	9.3.1.1 Wiring and wiring harness
	
	

	
	
	

	9.3.1.2 Cockpit switch / indicator
	
	

	
	
	

	9.3.1.3 Differential pressure switch
	
	

	
	
	

	9.3.1.4 Filter maintenance Aid and actuator
	
	

	
	
	

	9.3.1.5 Connectors
	
	

	
	
	

	9.3.1.6 Back shells
	
	

	
	
	

	9.3.1.7 Circuit breaker
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	9.3.2 Function check the following:
	Table 1
	

	
	
	

	9.3.2.1 Circuit breaker
	
	

	
	
	

	9.3.2.2 Cockpit switch
	
	

	
	
	

	9.3.2.3 Indicator
	
	

	
	
	

	9.3.2.4 Differential pressure switch
	
	

	
	
	

	9.3.2.5 Filter maintenance aid and actuator
	
	

	
	
	

	C  0120.10 APICAL REPLACEMENT EMERGENCY FLOATS – ICA407-1

	
	
	

	10.1 Unsnap unlace float covers.
	
	

	
	
	

	10.2 Conduct testing.
	Section 25.1.5
	

	
	
	

	10.3 Repack floats.  
	Section 25.1.7
	

	
	
	

	10.4 See bell helicopter document BHT– 407-MMS-1
	
	

	
	
	

	C  0120.11 SKY CONNECT – S200-ICA

	
	
	

	11.1 Perform a visual inspection on the following:
	
	

	
	
	

	11.1.1 Instruments
	
	

	
	
	

	11.1.2 Wiring harness and connectors
	
	

	
	
	

	11.1.3 Senders and probes
	
	

	
	
	

	C  0120.12 TANNIS HEATER

	
	
	

	12.1 Perform visual inspection for serviceability and security of attachment of the following:
	AC43.13-1B
	

	
	
	

	12.1.1 All wiring and pads.
	
	

	
	
	

	12.1.2 System Power plug, table leads and junctions.
	
	

	
	
	

	12.2 Perform all operational check of each pad.
	
	

	
	
	

	12.3 Cleaned as needed. 
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C  0120.13 TECH TOOLS BUBBLE WINDOW  -  TTP-407-ICA-002

	
	
	

	13.1 Visually inspect accessible areas of the following items for cleanliness, security of attachment, excessive wear, smooth operation of vents, gouges, dents, pitting, cracks or crazing, sealing capability, obvious damage, and general overall condition:
	
	

	
	
	

	13.1.1 Window Assembly 
	
	

	
	
	

	13.1.2 Snap Vent (-13 and -14 only) 
	
	

	
	
	

	13.2  If damage is evident, replace Snap Vent or Window Assembly including Snap Vent as appropriate.
	
	

	
	
	

	C  0120.14 AAI TAIL ROTOR PEDAL LOCKOUT KIT – AA-99032

	
	

	14.1 TAIL ROTOR PEDALS LOCKED OUT
	

	
	

	14.1.1 Inspect Lockout Bracket Assembly for condition and security of attachment.
	
	

	
	
	

	14.1.2 Verify the Expandable pins are properly positioned in the Bellcrank and Safety Clips are properly latched.
	
	

	
	
	

	14.1.3 Verify the Links are fully seated and locked on the Lockout bracket Assembly.
	
	

	
	
	

	14.2 TAIL ROTOR PEDALS ENGAGED
	

	
	

	14.2.1 Inspect Warning Decal for condition and security of attachment.
	
	

	
	
	

	14.2.2 Inspect Cable Assembly (Lanyard) for condition and security.
	
	

	
	
	

	14.2.3 Verify the Expandable Pins are seated on top of the Links.
	
	

	
	
	

	14.2.4 Verify the Safety Clips are properly latched.
	
	

	
	
	

	14.2.5 Verify there is no play between the Expandable Pins, Links and Bellcrank.
	
	

	
	
	

	14.2.6 Position each Tail Rotor Pedal, one at a time, to the full forward position. Verify there is no Pedal-to-Expandable Pin contact. Verify there is no right Expandable Pin contact with the Control Tube.
	
	

	
	
	

	C  0120.15 POST INSPECTION

	
	
	

	15.1 Inspect for operation and leaks.
	
	

	
	
	

	15.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	15.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	
	

	
	
	

	15.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – C 0120 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


