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1
INSPECTIONS EXCLUDED FROM AAIP 
Since the AAIP inspection program is not intended to prescribe maintenance functions, the following items will be tracked separately in the aircraft status report. 

A. Hand-held Fire Extinguishers
B. Static System and Altitude Reporting System per 14 CFR 91.411.
C. ATC Transponder Test and Inspections per 14 CFR 91.413.
D. Inspect Pitot-Static System per 14 CFR 91.411/413 
E. 36 Month Hydrostatic Retest of Emergency Floatation Gas Cylinder per AA-ICA407-11
F. 12 Month Servo Actuator Inspection per Bell BHT-407-MM-1 Para 5-22

G. Engine Compressor Wash – Rolls-Royce M250-C47 Series MM 72-30-00 Para 5.B

H. 600 hour Rotor Brake Assembly Inspections – BHT-407-CR&O-V
I. 1200 hour Rotor Brake Assembly Inspections – BHT-407-CR&O-V
J. 600 hour and 12 month Blade Bolts inspections/lubrications - Bell BHT-407-MM-1 Para 5-24A
K. 2500 hour inspection of Main rotor Pitch Change Link 
L. 60 Month Freewheeling Unit Inspection - Bell BHT-407-MM-1 Table 5-4
M. 60 Month Mast Inspection - Bell BHT-407-MM-1 Table 5-4
N. 60 Month Transmission Inspection - Bell BHT-407-MM-1 Table 5-4
O. Engine Wash – Rolls-Royce M250-C47 Series MM 72-00-00 Table 606
