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	1Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 4, 5, 12

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0052.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0052.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	A 0052.3  AIRFRAME

	
	
	

	3.1 Examine the forward and the transmission cowlings for condition.
	Chapter 53
	

	
	
	

	3.2 Examine the engine air inlet cowling for condition. Examine the components as follows:
	Chapter 53 and 71
	

	
	
	

	3.2.1 Screen.
	
	

	
	
	

	3.2.2 Bellmouth.
	
	

	
	
	

	3.3 Examine the forward top deck for condition and security.
	Chapter 53
	

	
	
	

	A 0052.4 CONTROLS 

	
	
	

	4.1 Examine all of the control tubes, bellcranks and the supports for condition, corrosion, security and correct operation. 
	Chapter 67
	

	
	
	

	4.2 Examine the components as follows:
	
	

	
	
	

	4.2.1 Signs of control interference.
	
	

	
	
	

	4.2.2 Inspect pitch links.
	
	

	
	
	

	4.2.3 Springs.
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0052.5 HYDRAULIC

	
	
	

	5.1 Examine the hydraulic system for condition leaks and security. Examine the components as follows:
	Chapter 29
	

	5.1.1 Hydraulic actuators.
	
	

	
	
	

	5.1.2 Fluid flexible and rigid lines.
	
	

	
	
	

	5.1.3 Filter differential pressure indicator button (two places)
	
	

	
	
	

	5.1.4 Pivot bolts of the pilot valve on the actuators for freedom of rotation.
	
	

	
	
	

	5.1.5 Reservoir.
	
	

	
	
	

	5.1.6 Pump.
	
	

	
	
	

	5.1.7 Remove the pump and inspect the input drive shaft/adapter a applicable.
	
	

	
	
	

	5.1.8 Lubricate the pump drive (as applicable to configuration) – C-525 or grease C-561
	Chapter 12
	

	A 0052.6 TRANSMISSION AND PYLON ASSEMBLY

	
	
	

	6.1 Examine the pylon assembly for condition and security.
	Chapter 63
	

	
	
	

	6.2 Examine the components as follows:
	Chapter 63
	

	
	
	

	6.2.1 Up-stops.
	
	

	
	
	

	6.2.2 Pylon beams.
	
	

	
	
	

	6.2.3 Corner mounts.
	
	

	
	
	

	6.2.4 Restraint spring assembly
	
	

	
	
	

	6.2.5 Pylon stop transmission fitting.
	
	

	
	
	

	6.2.6 Pylon stop deck fitting.
	
	

	
	
	

	6.3 Examine the transmission assembly for damage, leaks, and security.
	
	

	
	
	

	6.4 Examine the components as follows:
	
	

	
	
	

	6.4.1 Fluid flexible and rigid lines.
	
	

	
	
	

	6.4.2 Electrical harness.
	Chapter 96
	

	
	
	

	6.4.3 Impending bypass valve indicator,
	Chapter 63
	

	
	
	

	6.4.4 Oil press system manifold.
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.4.5 Filter manifold.
	
	

	
	
	

	6.5 Examine the transmission lower and upper (mast bearing) chip detectors for metal particles.
	Chapter 63
	

	
	
	

	6.6 Examine the electrical circuit of the chip detectors for continuity.
	Chapter 96
	

	
	
	

	A 0052.7 POST INSPECTION

	
	
	

	7.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	7.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0052 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




