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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 4, 5, 12

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0054.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0054.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	A 0054.3  AIRFRAME

	
	
	

	3.1 Examine the aft fairing for condition.
	Chapter 53
	

	
	
	

	3.2 Examine the aft top deck for condition, leaks and security.
	
	

	
	
	

	A 0054.4 TAILBOOM STRUCTURE

	
	
	

	4.1 Examine the tail rotor driveshaft cover and the gearbox cowling for condition, corrosion and security.
	Chapter 53
	

	CAUTION
ANY CRACK, CORROSION, OR LOOSE OR SHEARED RIVET IS CAUSE FOR IMMEDIATE GROUNDING OF THE HELICOPTER UNTIL THE PROBLEM IS CORRECTED.
	

	4.2 Examine the tailboom assembly for condition and security. Examine the components as follows:
	
	

	
	
	

	4.2.1 Tailboom skins for chafing damage or cracks from the tail rotor driveshaft covers and the tail rotor gearbox covers.
	
	

	
	
	

	4.2.2 Tailboom skins at the horizontal stabilizer for cracks, loose rivets and fasteners. 
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.2.3 Hanger bearing supports for cracks and security.
	
	

	
	
	

	4.2.4 Horizontal stabilizer and the attachment supports for cracks and security.
	
	

	
	
	

	4.2.5 Auxiliary fins for condition and security.
	
	

	
	
	

	4.2.6 Slat assemblies for condition and security. 
	
	

	
	
	

	4.2.7 Vertical fin for condition and security.
	
	

	
	
	

	4.2.8 Tail rotor gearbox support where it attaches to tailboom and at the attachment of the tail rotor gearbox.
	
	

	
	
	

	A 0054.5 TAIL ROTOR GEARBOX

	
	
	

	5.1 Do a torque check of the tail rotor gearbox attachment nuts (140 to 160 in-pounds). 
	Chapter 65
	

	
	
	

	5.2 Examine the tail rotor gearbox for condition, leaks, and security.
	
	

	
	
	

	5.3 Examine the chip detector of the tail rotor gearbox for metal particles.
	Chapters 65 & 96
	

	
	
	

	5.4 Examine the electrical circuit of the chip detector for continuity. 
	
	

	
	
	

	A 0054.6 TAIL ROTOR PITCH CHANGE CONTROL

	
	
	

	6.1 Examine the tail rotor pitch control mechanism for condition and security. 
	Chapter 67
	

	
	
	

	6.2 Examine the components as follows:  
	Chapter 65
	

	
	
	

	6.2.1 Boot.
	
	

	
	
	

	6.2.2 Pitch links.
	
	[bookmark: _GoBack]

	
	
	

	6.2.3 Crosshead sliding seal.
	
	

	
	
	

	6.3 Lubricate tail rotor pitch change mechanism – C-001
	
	

	NOTE: Grease every 300 hours or when a new component is installed.
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0054.7 POST INSPECTION

	
	
	

	7.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	7.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0054 – 300 Hour / 12 Month and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




