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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 5
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0055.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0055.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0055.3 INSTRUMENTS

	
	
	

	3.1 Inspect instruments for condition and security. Inspect for correct markings. 
	BHT-407-FM-1 or FM-2
	

	A 0055.4 CORROSION CONTROL

	4.1 Perform corrosion inspection in accordance with the Corrosion Guide for areas accessed by this inspection.
	CSSD-PSE-87-001 Para 30-4
	

	A 0055.5 EQUIPMENT AND FURNISHINGS

	
	
	

	5.1 Examine the cabin floor for condition.
	Chapter 53
	

	
	
	

	5.2 Examine the seat cushions, seat backs, and interior trim for condition and security.
	 Chapter 25
	

	
	
	

	5.3 Examine the restraints for condition, security, and correct operation. 
	
	

	
	
	

	5.4 Examine the ventilation system for condition and security.
	Chapter 21
	

	
	
	

	5.5 Make sure the fuel valve switch guard operates correctly. 
	
	

	
	
	

	5.6 Examine the fire extinguisher and quick-release for condition and security. 
	Chapter 26
	

	
	
	

	5.7 Examine the heating system of the pitot and static ports for correct operation.
	Chapter 96
	

	
	
	

	5.8 On 407 helicopters S/N 53000 through 54299, make sure the FADEC Fault Code – Maintenance Mode system operates correctly. 
	Chapter 76
	

	
	
	

	5.9 On 407GX helicopters S/N 54300 and subsequent, make sure the Bell Maintenance Pages can be accessed.
	Chapter 95
	

	
	
	

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0055.6 CONTROLS

	
	
	

	6.1 Examine the cyclic and the collective control sticks and pedals for condition and security. Examine the directional control pedal for correct operation.
	Chapter 67
	

	
	
	

	6.2 Examine components of airspeed-actuated pedal stop for condition, security, and correct operation. Examine components that follow:
	
	

	
	
	

	6.2.1 Solenoid
	
	

	
	
	

	6.2.2 Cam
	
	

	
	
	

	6.2.3 Release Cable
	
	

	
	
	

	6.3 Make sure there is a minimum of friction on the components that follow:
	
	

	
	
	

	6.3.1 Cyclic
	
	

	
	
	

	6.3.2 Collective
	
	

	
	
	

	6.3.3 Directional Control
	
	

	
	
	

	A 0055.7 ELECTRICAL

	
	
	

	7.1 Perform operational check of airspeed-actuated pedal stop system.
	Chapter 96
	

	
	
	

	A 0055.8 FORWARD FUSELAGE

	
	
	

	8.1 Examine the forward fuselage for condition and security. Examine the components as follows:
	
	

	
	
	

	8.1.1 Doors, door hinges and latches. 
	Chapter 52
	

	
	
	

	8.1.2 Complete litter door caution light operational check. 
	
	

	
	
	

	8.1.3 Battery door.
	
	

	
	
	

	8.1.4 Any fluid leaks.
	
	

	
	
	

	8.1.5 Windows.
	
	

	
	
	

	8.1.6 Side body fairings. 
	Chapter 53
	

	
	
	

	8.1.7 Upper fairings and cowlings.
	
	

	
	
	

	8.1.8 Upper roof deck.
	
	

	
	
	

	8.1.9 Lower forward shell.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	8.2 Examine the battery compartment for condition and security. Examine the vent line. Do a functional test of the battery hot annunciator circuit. Install a serviceable battery.
	Chapter 96
	

	
	
	

	8.3 Examine the External Power Receptacle for condition and security. 
	
	

	
	
	

	8.4 Examine the components as follows:
	Chapter 95
	

	
	
	

	8.4.1 The pitot and the static ports for condition and security. :
	
	

	
	
	

	8.4.2 The Pitot tube for discoloration and visible obstruction. 
	
	

	
	
	

	8.5 Drain moisture from the pitot and the static piping installation.
	
	

	
	
	

	8.6 Examine the antenna(s) for condition and security. Restore broken or missing sealant at antenna base as required. 
	Chapter 97
	

	
	
	

	A 0055.9 POST INSPECTION

	
	
	

	9.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	9.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	9.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	9.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _GoBack]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0055 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




