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	2
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	SECTION:
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	
	


Reference:  BHT 407 MM-1 Chapter 4, 5, 12  BHT 407 MMS-6
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0056.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0056.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	A 0056.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide for areas accessed by this inspection.
	CSSD-PSE-87-001 Para 30-4
	

	3.2 
	
	

	A 0056.4 AIRFRAME

	CAUTION
ANY CRACK, CORROSION, OR LOOSE OR SHEARED RIVET IS CAUSE FOR IMMEDIATE GROUNDING OF THE HELICOPTER UNTIL THE PROBLEM IS CORRECTED
	
	

	4.1 Examine the aft fuselage structure for condition and security. Examine the components as follows:
	Chapter 53
	

	
	
	

	4.1.1 Engine upper cowling and doors. 
	
	

	
	
	

	4.1.2 Upper longeron.
	
	

	
	
	

	4.1.3 All engine mounts and sway bar to airframe attachment points.
	
	

	
	
	

	4.1.4 Mid fuselage lower longerons. 
	
	[bookmark: _GoBack]

	
	
	

	4.1.5 Floor of the baggage compartment.
	
	

	
	
	

	4.1.6 Walls of the baggage compartment.
	
	

	
	
	

	4.1.7 Examine the auxiliary fuel tank installation for condition and security (if Installed)
	Chapter 99
	

	
	
	

	4.1.8 Baggage compartment door.
	Chapter 52
	

	
	
	

	4.1.9 Aft lower fairing.
	
	

	
	
	


	MARITIME HELICOPTERS
	Bell 407 AAIP

	
	

	Page No:
	1

	Revision:
	2

	Issue Date:
	01/15/15

	SECTION:
	
	A 0056 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	







	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.1.10 Oil cooler fairing.
	
	

	
	
	

	4.1.11 Oil cooler deck.
	
	

	
	
	

	4.1.12 Aft fuselage skins.
	
	

	
	
	

	4.1.13 Aft lower shell. 
	
	

	
	
	

	4.2 Examine the interior of the structure for condition.
	Chapter 53
	

	
	
	

	4.3 Examine the condition of the rivets that attach the composite skins to the structure.
	
	

	
	
	

	4.4 Examine the electrical components, the mounts, and the electrical harness for condition and security. 
	Chapter 96
	

	
	
	

	4.5 Examine the transmission oil lines and other drain lines for condition and security.
	Chapter 63
	

	
	
	

	4.6 Examine the tail rotor control system for condition, security, and correct operation.
	Chapter 67
	

	
	
	

	4.7 Examine the antenna(s) for condition and security. Restore broken or missing sealant at antenna base as required.
	Chapter 97
	

	
	
	

	4.8 Do an operational check of the baggage door annunciator circuit. 
	Chapter 96
	

	
	
	

	A 0056.5 HYDRAULIC

	
	
	

	5.1 Examine the tail rotor hydraulic system for condition, leaks, and security. Examine the components as follows:
	Chapter 29
	

	
	
	

	5.1.1 Pivot bolts of the pilot valve on the actuators for freedom of rotation.
	
	

	
	
	

	5.1.2 Actuator support.
	
	

	
	
	


	A 0056.6 LANDING GEAR

	
	
	

	6.1 Examine the landing gear assembly for condition and security. Examine the components as follows:
	Chapter 32
	

	
	
	

	6.1.1 Skid tubes.
	
	

	
	
	

	6.1.2 Skid saddles.
	
	

	
	
	

	6.1.3 Skid shoes. 
	
	

	
	
	

	6.1.4 Retaining strap and rubber cushions.
	
	

	
	
	

	6.1.5 Rocking beam.
	
	

	
	
	

	6.1.6 Crosstubes.
	
	

	
	
	

	6.1.7 Attachment fittings. 
	
	

	
	
	


	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0056.7 POST INSPECTION

	
	
	

	7.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	7.2 Perform a FADEC manual mode check
	Rolls-Royce
	

	
	Operation & MM
	

	7.3 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.4 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	7.5 [bookmark: _Hlk512334435]Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	












	MARITIME HELICOPTERS
	Bell 407 AAIP

	
	

	Page No:
	3

	Revision:
	5

	Issue Date:
	11/01/18

	SECTION:
	
	A 0056 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0056 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




