	MARITIME HELICOPTERS
	AgustaWestland Model AW119 AAIP

	
	

	Page No:
	3

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	A 3200RT – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	3200 HOUR INSPECTION

	NOTE:
	
	This Inspection is Restricted to +60 Hours



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII Maintenance Planning Manual Chapter 05-40

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3200.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 3200.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	A 3200.3 FUEL

	
	
	

	3.1 Inspect fuel tanks for debris, water, contamination, cleanliness and presence of fungus.
	28-11-10
	

	
	
	

	3.2 Inspect fuel tank and internal components for condition.
	
	

	
	
	

	3.3 Perform tank pressure test.
	28-12-4
	

	
	
	

	A 3200.4 DOORS

	
	
	

	4.1 Inspect cowlings, fairings, doors and access panels, service steps for condition, cracks, distortions, defective and/or missing rivets and correct hinge operation.
	
	

	
	
	

	A 3200.5 FUSELAGE

	
	

	5.1 Inspect the following:
	

	
	

	5.1.1 Visible electrical and electronic component supports for condition and security.
	
	

	
	
	

	5.1.2 Fuselage for general condition, visual evidence of distortions, nicks, scratches, corrosion, defective and/or missing rivets particularly in the area surrounding attachment points of main transmission, transmission supports, engine mounts, fan supports, tail boom and landing gear.
	
	

	
	
	

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.3 Fuselage/tail boom attachment holes for corrosion, wear and elongation.
	53-31-9
	

	
	
	

	5.1.4 Fuel tank bays for cracks and distortions.
	
	

	
	
	

	5.2 Check transmission antitorque plate and deck structure attaching bolt holes for corrosion, wear and elongation.
	63-21-17
	

	
	
	

	A 3200.6 TAILBOOM

	
	

	6.1 Remove the following:
	

	
	

	6.1.1 L/H Stabilizer
	
	

	
	
	

	6.1.2 R/H Stabilizer
	
	

	
	
	

	6.1.3 Lower Fin
	
	

	
	
	

	6.1.4 90° Gearbox
	
	

	
	
	

	6.2 Visually inspect externally and internally for the following;
	

	
	

	6.2.1 General condition, distortions, cracks, corrosion.
	
	

	
	
	

	6.2.2 Defective and/or missing rivets particularly area surrounding fuselage attachment points, stabilizers, lower fin, tail skid and 90° gearbox.
	
	

	
	
	

	6.2.3 Stabilizers
	
	

	
	
	

	6.2.4 Lower fin
	
	

	
	
	

	6.2.5 90° Gearbox
	
	

	
	
	

	6.3 Reinstall the following:
	

	
	

	6.3.1 L/H Stabilizer
	
	

	
	
	

	6.3.2 R/H Stabilizer
	
	

	
	
	

	6.3.3 Lower Fin
	
	

	
	
	

	6.3.4 90° Gearbox
	
	

	
	
	

	A 3200.7 MAIN DRIVE SHAFT

	
	
	

	7.1 Inspect main transmission components.
	63-21-18
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3200.8 POST INSPECTION

	
	
	

	8.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	
	

	
	
	

	8.3 Perform Functional Check Flight if required per AW119MKII MPM Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	8.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

[bookmark: _GoBack]At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

[bookmark: _Hlk529367719]I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk529367746]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – A 3200RT – 3200 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	


	

