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	Page No:
	3

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	A 2410RT – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	2400 HOUR INSPECTION 

	
	
	(OCCURES AFTER 1200 HOURS OF COMPONENT OPERATION)

	NOTE:
	
	This Inspection is Restricted to +30 Hours



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII Maintenance Planning Manual Chapter 05-50

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 2410.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 2410.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	A 2410.3 TAIL ROTOR DRIVE 90° GEARBOX

	
	

	3.1 Inspect gears for the following;
	

	
	

	3.1.1 Abnormal patterns, pitting and scoring.
	65-21-14
	

	
	
	

	3.1.2 Fretting, damage, wear, corrosion on input pinion teeth and output shaft.
	65-21-14
	

	
	
	

	3.1.3 Integrity of the packing carriers.
	65-21-14
	

	
	
	

	3.1.4 Gearing teeth for unusual prints, pitting, scoring, damage and bearings for freedom of rotation and roughness.
	65-21-14
	

	
	
	

	3.2 Perform tail rotor (90°) gearbox backlash check.
	65-21-9
	

	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

[bookmark: _Hlk529367719]I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



[bookmark: _GoBack]I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk529367746]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – A 2410RT – 1200 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	


	



