	MARITIME HELICOPTERS
	AgustaWestland Model AW119 AAIP

	
	

	Page No:
	1

	Revision:
	Orig

	Issue Date:
	12/01/18

	SECTION:
	
	B 0000 – ENGINE INSPECTION PROGRAM

	TYPE:
	
	000 HOUR / 00 MONTH INSPECTION

	NOTE:
	
	NO TOLERANCE 

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Pratt & Whitney Canada Maintenance Manual Model PT6B-37A Chp 05-20-00
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0051.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Pratt & Whitney PT6B-37A Operations and Maintenance Manual).
	PT6B-37A MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Pratt & Whitney PT6B-37A Operations and Maintenance Manual).
	PT6B-37A MP
	

	
	
	

	B 0051.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	B 0051.3 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	3.1 Inspect the following:
	

	
	

	3.1.1 Engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	
	

	
	
	

	3.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	

	3.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened
	
	

	
	
	

	3.1.4 Compressor impeller leading edges for damage
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	3.1.5 Examine the engine cowling and doors for condition and security. Replace anti-chaff tape as needed.  
	
	

	
	
	

	3.1.6 Fluid flexible and rigid lines.
	
	

	
	
	

	3.1.7 Electrical harness.
	
	

	
	
	

	3.1.8 Exhaust stack.
	
	

	
	
	

	3.1.9 Engine mounts fittings and legs.
	
	

	
	
	

	3.2 Examine the firewalls for condition and security.
	
	

	
	
	

	3.3 Examine the engine pan drains. Make sure that they are not clogged. Restore broken or missing sealant from engine pan.
	
	

	
	
	

	3.4 Examine the engine controls for condition, correct operations and security.
	
	

	
	
	

	3.5  Examine the components as follows:
	

	NOTE: Refer to Chapter 76, “Throttle/Fly Detent Rigging Procedure” for acceptable limits.
	

	3.5.1 
	
	

	
	
	

	3.5.2 All linkages for any looseness, condition and security.
	
	

	
	
	

	3.6 Check oil supply level.
	
	

	NOTE: If the engine has been idle for more than 15 minutes, motor the engine for 30 seconds to scavenge any oil that may have drained into the gearbox from the oil tank. Failure to completely scavenge the oil from the gearbox will cause a false indication of high oil consumption.
	
	

	CAUTION: NORMAL ENGINES USE A MINIMAL AMOUNT OF OIL. HOWEVER, ANY SUDDEN INCRREASE IN OIL CONSUMTION IS INDICATIVE OF OIL SYSTEM PROBLEMS AND MUST BE CORRECTED.
	

	NOTE: Check oil supply level within 15 minutes of engine shutdown.


	

	3.7 Inspect for extension of scavenge oil filter bypass indicator on CEFA
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	If the bypass indicator is extended, examine/clean the engine oil filter and the scavenge oil filter.  If contamination is found, replace the scavenge oil filter.  If no contamination is found, reinstall the scavenge oil filter with new packing and manually reset the indicator.

If the CEFA bypass indicator is extended and contamination is found in the scavenge oil filter, replace/clean the oil cooler, oil tank and lubrication lines (Ref. The airframe manual instructions). Drain and replace the engine oil and manually reset the indicator
	
	

	NOTE:   If metal contamination is found in the scavenge oil filter in CEFA and a chip light occurred within the previous 50 hours, take the applicable maintenance steps (Ref. 72-00-00, para 8.E.(2), Engine Servicing or 72-60-00 para 4.B.(2)).

NOTE: The scavenge oil filter cannot be cleaned.


	

	B 0051.4 

	
	
	

	4.1 Remove fuel filter canister.
	
	

	
	
	

	4.2 Remove and inspect fuel filter for any contaminants.
	
	

	
	
	

	4.3 Install new filter and o-rings.
	
	

	
	
	

	4.4 Reinstalled fuel filter canister.
	
	

	
	
	

	4.5 Remove fuel nozzle.
	
	

	
	
	

	4.6 Disassemble fuel nozzle.
	
	

	
	
	

	4.7 Cleaned and inspected fuel nozzle filter assembly.
	
	

	
	
	

	4.8 Visually inspect the outer combustion case butt weld areas near the braze patch for cracks.  Use a bright light and mirror as necessary.
	
	

	Note: removal of the outer combustion case is not required.
	

	4.9 Assemble fuel nozzle.
	
	

	
	
	

	4.10 Install fuel nozzle with proper number of spacers.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0051.5 POST INSPECTION

	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.2 Ground run aircraft - Inspect for operation and leaks.
	BHT-407-FM-1/2
	

	
	
	

	5.3 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	5.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters AgustaWestland AW119 AAIP 000 Hour / 12 Month – B 0000 – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


