	MARITIME HELICOPTERS
	AgustaWestland Model AW119 AAIP

	
	

	Page No:
	1

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	B 0100 – ENGINE INSPECTION PROGRAM

	TYPE:
	
	100 HOUR INSPECTION

	NOTE:
	
	

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Pratt & Whitney Canada Maintenance Manual Model PT6B-37A Chp 05-20-00
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0100.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Pratt & Whitney Maintenance Manual Airworthiness Limitations ).
	PT6B-37A MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Pratt & Whitney Maintenance Manual Chp 05-20-00 Para 2).
	PT6B-37A MP
	

	CAUTION

BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	B 0100.2 P3 AIR FILTER

	
	
	

	2.1 Remove filter bowl assembly.
	72.00.24
	

	
	5.A.
	

	2.2 Remove filter.
	
	

	
	
	

	2.3 Remove drain valve.
	72.00.24
	

	
	6.B.
	

	2.4 Inspect filter element.
	72.00.24
	

	
	7.A.
	

	2.5 If the filter is corrosion free, clean and re-install in assembly.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	2.6 If corrosion is noted in filter (if none, mark N/A);
	
	

	
	
	

	2.6.1 Over a white sheet of paper, lightly tap the P3 filter to release any loose particles from the inside portion of the filter
	
	

	
	
	

	2.6.2 If corrosion particles drop out from the filter, remove FCU and send in for inspection and cleaning of the air passages.
	
	

	
	
	

	2.7 Clean drain valve.
	72.00.24
	

	
	6.B
	

	2.8 Reinstall drain valve in bottom of housing.
	72.00.24
	

	
	5.C
	

	2.9 Reinstall filter bowl assembly.
	72.00.24
	

	
	5.C
	

	B 0100.3 POST INSPECTION

	
	
	

	3.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	3.2 Ground run aircraft - Inspect for operation and leaks.
	AW119-FM
	

	
	
	

	3.3 Perform Functional Check Flight if required per Pratt & Whitney MM, or RFM as appropriate.
	
	

	
	
	

	3.4 Perform ground idle check.
	71-00-00
	

	Effectivity:  Post-SB39014 fuel control units with Post-SB39027 Fuel Pump
	
	

	3.5 Perform an EEC engine trim check.
	71-00-00
	

	
	
	

	3.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AgustaWestland AW119 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters AgustaWestland AW119 AAIP 100 Hour – B 0100 – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


