	MARITIME HELICOPTERS
	AgustaWestland Model AW119 AAIP

	
	

	Page No:
	1

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	B 0600 – ENGINE INSPECTION PROGRAM

	TYPE:
	
	600 HOUR INSPECTION

	NOTE:
	
	

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Pratt & Whitney Canada Maintenance Manual Model PT6B-37A Chp 05-20-00
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0600.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Pratt & Whitney Maintenance Manual Airworthiness Limitations ).
	PT6B-37A MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Pratt & Whitney Maintenance Manual Chp 05-20-00 Para 2).
	PT6B-37A MP
	

	
	
	

	B 0600.2 ENGINE FUEL SYSTEM

	CAUTION

EXTREME CARE MUST BE EXERCISED WHEN HANDLING, SINCE EVEN FINGERPRINTS ON NOZZLE ORIFICES MAY PRODUCE POOR SPRAY PATTERNS. CLEAN LINT-FREE COTTON GLOVES OR SURGICAL GLOVES SHOULD BE WORN AT ALL TIMES WHEN HANDLING COMPONENTS. ASSEMBLIES WHICH ARE NOT TO BE IMMEDIATELY REINSTALLED SHOULD BE PLACED IN A COVERED CONTAINER TO PREVENT EXPOSURE TO DIRT AND DUST. 
	

	2.1 Install new:
	

	
	

	2.1.1 Low pressure fuel filter.
	72-00-23
	

	
	
	

	2.1.2 High pressure fuel filter.
	72-00-22
	

	Effectivity:  Post SB39027
	
	

	2.2 Remove fuel manifold adapters and fuel nozzle sheaths.
	72-00-04
	

	
	5.A
	

	2.3 Check fuel pump coupling in-situ for fretting and corrosion.
	72-00-22
	

	
	FUEL PUMP –

MAINTENANCE PRACTICES
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	2.4 Inspect and clean fuel manifold adapter assemblies.
	72-00-04
	

	
	7.A
	

	2.5 Inspect and clean fuel nozzles.
	72-00-04
	

	
	7.B
	

	2.6 Function Check nozzles.
	72-00-04
	

	
	6.D
	

	2.7 Install nozzles in manifold adapters.
	72-00-04
	

	
	5.B
	

	2.8 Installed manifold adapter assemblies
	72-00-04
	

	
	5.B
	

	2.9 Check fuel pump coupling in-situ for fretting and corrosion
	72-00-22
	

	
	
	

	B 0600.3 ENGINE COMPONENTS

	
	
	

	3.1 Disassemble and inspect compressor bleed valve.
	72-00-01
	

	Effectivity: Pre-SB39024
	
	

	3.2 T5 Temperature Sensing System
	

	
	

	3.2.1 Check security of all accessible connections, clamps and brackets and for evidence of wear, chafing, cracks and corrosion.
	
	

	
	
	

	3.2.2 Carry out functional check.
	05-50-00
	

	
	4.A
	

	3.3 Inspect turbine exhaust duct for cracks or distortion.
	
	

	
	
	

	B 0600.4 ENGINE OIL SYSTEM

	
	
	

	4.1 Remove oil filter housing assembly.
	
	

	
	
	

	4.2 Inspect and replace oil filter.
	
	

	
	
	

	4.3 Reinstall oil filter housing assembly.
	
	

	
	
	

	4.4 Remove, inspect and clean accessory gearbox chip detector.
	
	

	
	
	

	4.5 Remove, inspect and clean both reduction gearbox chip detectors.
	
	

	
	
	

	4.6 Check for continuity of electrical circuit on accessory gearbox chip detector, perform lift test to check magnetism.
	72-00-19
	

	
	
	

	4.7 Check for continuity of electrical circuit on reduction gearbox chip detector, perform lift test to check magnetism.
	72-00-19
	

	
	
	

	4.8 Reinstall accessory gearbox chip detector
	
	

	
	
	

	4.9 Reinstall reduction gearbox chip detectors
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0600.5 POST INSPECTION

	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.2 Perform FCU Manual Override Functional Check
	71-00-00
	

	
	
	

	5.3 Ground run aircraft - Inspect for operation and leaks.
	
	

	
	
	

	5.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AgustaWestland AW119 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters AgustaWestland AW119 AAIP 600 Hour – B 0600 – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



