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	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-117 Series MM Appendix A
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0040.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	A 0040.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 0040.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 0040.4 MAIN TRANSMISSION

	4.1 Use magnifying glass to inspect underside of rotor mast flange in the area of bores as well as webs between bores for cracks.
	
	

	Effectivity; If washers P/N 105--13101.16 are installed
	

	4.2 
	
	

	4.3 
	
	

	A 0040.5 ROTOR BRAKE SYSTEM

	5.1 Inspect brake pads for movability by hand (Rotor brake not applied)
	12-3, step 2
	

	5.2 Change oil.
	12-16 
thru 12-18
	

	A 0040.6 MAIN ROTOR SYSTEM

	6.1 
	
	

	6.2 
	
	

	A 0040.7 MAIN ROTOR BLADE

	7.1 
	
	

	A 0040.8 FUSELAGE

	
	
	

	8.1 
	
	

	
	
	

	A 0040.9 COWLINGS

	
	
	

	9.1 Visually inspect goosenecks P/N 117-23236-01, P/N 117-23237-01of transmission cowling for cracks
	22-9 thru 22-11
	

	
	
	

	A 0040.10 TAIL BOOM

	
	
	

	10.1 Visually inspect tail rotor transmission mounting brackets in the vertical fin for loose rivets and cracks and adjacent areas for cracks.
	31-2, step 6
	

	
	
	

	10.2 
	
	

	
	
	

	A 0040.11 TAIL ROTOR DRIVE

	
	
	

	11.1 Remove magnetic plug of intermediate gear box and tail rotor transmission and inspect for deposits.
	32-32, step 3
	

	Effectivity; All BK117 if SB MBB--BK117--90--119 has not been implemented 

	

	11.2 Inspect tail rotor transmission hardware for proper torque and tighten as necessary.
	32-37
	

	Effectivity; MBB--BK117 up to and including S/N 7261, if ASB MBB--BK117--30--104 has not been implemented
	

	A 0040.12 TAIL ROTOR

	
	
	

	12.1 Without disassembly, inspect spherical bearings in fork end of tail rotor shaft for play, corrosion and binding.
	33-21, step 1
	

	
	

	12.2 Inspect flapping hinge function.
	33-4, step 3
	

	12.3 Dynamically balance the tail rotor.
	33-3
	

	12.4 Inspect the bearings of the pitch links.
	33-7 step 3
	

	A 0040.13 TAIL ROTOR BLADE

	
	
	

	13.1 Remove the tail rotoblades. Inspect erosion protection for debonds. Inspect attachment area for damages. Inspect tail rotor blades for cracks in surface protection. It is not necessary to remove the cover tape in the nose shell area.
	34-2 step 2
and 7
	

	13.2 Inspect tail rotor blade for impact damage and cracks in surface protection. The cover tape in the nose area does not have to removed.
	34-2, steps 2. 
	

	Effectivity; All tail rotor blades except P/N: 117-31743, 117-317411, 
B641M1001 101
	




	
	
	

	13.3 
	
	

	
	
	

	A 0040.14 MAIN ROTOR FLIGHT CONTROLS

	
	
	

	14.1 Inspect attachment bolts between rotating control rods and control levers of main rotor head for security of mounting.
	41-3 step 4e
	

	Effectivity; If lock washers P/N 117--142041.04 or P/N 105--13101.25 are not installed.

	

	14.2 
	
	

	A 0040.15 TAIL ROTOR FLIGHT CONTROLS

	
	
	

	15.1 Inspect yaw actuator
	
	

	Effectivity; Actuator P/N 741B 0000--05 and P/N 741C 0000--05 only
	

	15.2 
	
	

	15.3 
	
	

	A 0040.16 HYDRAULIC SYSTEM

	
	
	

	16.1 
	
	

	A 0040.17 LANDING GEAR

	
	
	

	17.1 
	
	

	A 0040.18 FUEL SYSTEM

	
	
	

	18.1 
	
	

	A 0040.19 LUBRICATION SYSTEM

	
	
	

	19.1 
	
	

	A 0040.20 FIRE WALLS

	
	
	

	20.1 
	
	

	A 0040.21 ENGINE OPERATION AND CONTROL

	
	
	

	21.1 
	
	

	A 0040.22 STANDARD EQUIPMENT

	
	
	

	22.1 
	
	

	A 0040.23 INSTRUMENT SYSTEMS

	
	
	

	23.1 
	
	

	
	

	A 0040.24 ELECTRICAL SYSTEMS

	
	
	

	24.1 
	
	

	A 0040.25 DC SUPPLY SYSTEM

	
	
	

	25.1 
	
	

	
	

	A 0040.26 EMERGENCY FLOAT SYSTEM

	
	
	

	26.1 
	
	

	A 0040.27 CARGO HOOK SYSTEM

	
	
	

	27.1 
	
	

	A 0040.28 SETTLING PROTECTORS

	
	
	

	28.1 
	
	

	A 0040.29 FIXED LANDING LIGHT -- FUSELAGE

	
	
	

	29.1 
	
	

	29.2 
	
	

	A 0040.30 FIXED LANDING LIGHT -- CROSS TUBE

	
	
	

	30.1 .
	
	

	A 0040.31 STROBE LIGHT SYSTEM

	
	
	

	31.1 .
	
	

	A 0040.32 BOARDING STEP -- LONG

	
	
	

	32.1 .
	
	

	A 0040.33 MAIN ROTOR BLADE FOLDING SYSTEM

	
	
	

	33.1 .
	
	

	A 0040.34 EXTERNAL LOUDSPEAKER SYSTEM

	
	
	

	34.1 .
	
	

	A 0040.35 AFT BATTERY

	
	
	

	35.1 .
	
	

	A 0040.36 RADOM

	
	
	

	36.1 .
	
	

	A 0040.37 PROTECTIVE COVERS FOR DUAL CONTROLS

	
	
	

	37.1 .
	
	

	A 0040.38 SNOW SKIDS

	
	
	

	38.1 .
	
	

	A 0040.39 SEARCHLIGHT

	
	
	

	39.1 .
	
	

	A 0040.40 EXTERIOR MIRROR

	
	
	

	40.1 .
	
	

	A 0040.41 CARTRIDGE--TYPE FUEL PUMP

	
	
	

	41.1 .
	
	

	A 0040.42 P/R CSAS SYSTEM

	
	
	

	42.1 .
	
	

	A 0040.43 COPILOT‘S FLIGHT INSTRUMENTS

	
	
	

	43.1 .
	
	

	A 0040.44 DUAL AC SYSTEM

	
	
	

	44.1 .
	
	

	A 0040.45 INSTANTENOUS VERTICAL SPEED INDICATOR

	
	
	

	45.1 .
	
	

	A 0040.46 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	46.1 .
	
	

	A 0040.47 HF--ANTENNA

	
	
	

	47.1 .
	
	

	A 0040.48 LANDING AND SEARCHLIGHT SYSTEM 450W

	
	
	

	48.1 .
	
	

	A 0040.49 ENGINE CLEANING PROVISION

	
	
	

	49.1 .
	
	

	A 0040.50 SAND FILTER

	
	
	

	50.1 .
	
	

	A 0040.51 DIGITAL AUTOMATIC FLIGHT CONTROL SYSTEM (DAFCS)

	
	
	

	51.1 .
	
	

	A 0040.52 EMERGENCY FLOAT SYSTEM, MAX TOW 3350 KG

	
	
	

	52.1 .
	
	

	A 0040.53 SCAVENGE OIL FILTER SYSTEM

	
	
	

	53.1 .
	
	

	A 0040.54 HIGH LANDING GEAR

	
	
	

	54.1 .
	
	

	A 0040.55 WIRE STRIKE PROTECTION SYSTEM (WSPS)

	
	
	

	55.1 .
	
	

	55.2 
	
	

	A 0040.56 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	56.1 
	
	

	Note; 
	

	56.2 
	
	



	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0040.57 POST INSPECTION

	
	
	

	57.1 Ensure applicable servicing requirements have been carried out.
	
	

	57.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	57.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	57.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	57.5 Perform Functional Check Flight if required per BK-117 Maintenance Manual  or RFM as appropriate.
	
	

	57.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series AAIP – A 0040 – 50 Hour / 24 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	





