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	Page No:
	3

	Revision:
	Original

	Issue Date:
	01/01/16

	SECTION:
	
	A0050 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	50 HOUR / 24 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-117 Series MM Appendix A
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0050.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	A 0050.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 0050.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 0050.4 MAIN TRANSMISSION

	4.1 
	
	

	4.2 
	
	

	A 0050.5 ROTOR BRAKE SYSTEM

	5.1 
	
	

	5.2 
	
	

	A 0050.6 MAIN ROTOR SYSTEM

	6.1 
	
	

	6.2 
	
	

	A 0050.7 MAIN ROTOR BLADE

	7.1 Inspect main rotor blades for bulges in the vicinity of the lead balance weights.
	14--2, step 5
	

	Effectivity: Blade fittings P/N 117--15854.05, 117--15860.05, 117--15854.06 and 117--15860.06
	

	7.2 
	
	

	7.3 
	
	

	A 0050.8 FUSELAGE

	
	
	

	8.1 
	
	

	
	
	

	A 0050.9 COWLINGS

	
	
	

	9.1 
	
	

	
	
	

	A 0050.10 TAIL BOOM

	
	
	

	10.1 
	
	

	
	
	

	10.2 
	
	

	
	
	

	10.3 
	
	

	
	
	

	A 0050.11 TAIL ROTOR DRIVE

	
	
	

	11.1 Change oil of intermediate gear box.
	32-5
	

	11.2 Change oil of tail rotor transmission.
	32-5
	

	A 0050.12 TAIL ROTOR

	
	
	

	12.1 
	
	

	
	

	12.2 
	
	

	
	

	A 0050.13 TAIL ROTOR BLADE

	
	
	

	13.1 
	
	

	
	
	

	13.2 
	
	

	
	
	

	A 0050.14 MAIN ROTOR FLIGHT CONTROLS

	
	
	

	14.1 Inspect flight control components (boosted section of flight controls) located above hydraulic system including swash plate for condition.
	41-3 Step 4
	

	
	
	

	14.2 Clean sliding surface of swash plate on sliding guide.
	
	

	
	
	

	14.3 Inspect swash plate bearing for rough running.
	41-52
	

	
	
	

	14.4 Inspect upper rod end seals for damage.
	41-59 step 6
	

	
	
	

	14.5 Check friction forces of pitch brake.
	41-14 step 5
	

	
	
	

	14.6 Inspect bearing forks of swashplate control ring and swashplate bearing ring for cracks.
	41-3
	

	A 0050.15 TAIL ROTOR FLIGHT CONTROLS

	
	
	

	15.1 
	
	

	15.2 
	
	

	A 0050.16 HYDRAULIC SYSTEM

	
	
	

	16.1 
	
	

	A 0050.17 LANDING GEAR

	
	
	

	17.1 
	
	

	A 0050.18 FUEL SYSTEM

	
	
	

	18.1 
	
	

	A 0050.19 LUBRICATION SYSTEM

	
	
	

	19.1 
	
	

	A 0050.20 FIRE WALLS

	
	
	

	20.1 
	
	

	A 0050.21 ENGINE OPERATION AND CONTROL

	
	
	

	21.1 
	
	

	A 0050.22 STANDARD EQUIPMENT

	
	
	

	22.1 
	
	

	A 0050.23 INSTRUMENT SYSTEMS

	
	
	

	23.1 
	
	

	
	

	A 0050.24 ELECTRICAL SYSTEMS

	
	
	

	24.1 
	
	

	A 0050.25 DC SUPPLY SYSTEM

	
	
	

	25.1 
	
	

	
	

	A 0050.26 EMERGENCY FLOAT SYSTEM, MAX. TOW 2850 KG

	
	
	

	26.1 Check emergency float system for operational readiness.
	
	

	NOTE: Circuit breaker EMER FLOATS must be set and toggle switch EMER
FLOATS must be in ARMED position. If green indicator light is not on, refer to para 802--2, TROUBLESHOOTING
	

	26.2 Inspect emergency float system for condition (floats removed).
	02--4
	

	
	
	

	26.3 Perform trial inflation.
	Refer to
manufacturer
	

	
	CMM 25--60--97
	

	A 0050.27 SETTLING PROTECTORS

	
	
	

	27.1 
	
	

	A 0050.28 FIXED LANDING LIGHT -- FUSELAGE

	
	
	

	28.1 Inspect fixed landing light for condition.
	08--5
	

	A 0050.29 FIXED LANDING LIGHT -- CROSS TUBE

	
	
	

	29.1 Inspect landing light for  general condition.
	08--4
	

	A 0050.30 STROBE LIGHT SYSTEM

	
	
	

	30.1 .
	
	

	A 0050.31 BOARDING STEP -- LONG

	
	
	

	31.1 .
	
	

	A 0050.32 MAIN ROTOR BLADE FOLDING SYSTEM

	
	
	

	32.1 .
	
	

	A 0050.33 EXTERNAL LOUDSPEAKER SYSTEM

	
	
	

	33.1 .
	
	

	A 0050.34 AFT BATTERY

	
	
	

	34.1 .
	
	

	A 0050.35 RADOM

	
	
	

	35.1 .
	
	

	A 0050.36 PROTECTIVE COVERS FOR DUAL CONTROLS

	
	
	

	36.1 .
	
	

	A 0050.37 SNOW SKIDS

	
	
	

	37.1 .
	
	

	A 0050.38 SEARCHLIGHT

	
	
	

	38.1 .
	
	

	A 0050.39 EXTERIOR MIRROR

	
	
	

	39.1 .
	
	

	A 0050.40 CARTRIDGE--TYPE FUEL PUMP

	
	
	

	40.1 .
	
	

	A 0050.41 P/R CSAS SYSTEM

	
	
	

	41.1 .
	
	

	A 0050.42 COPILOT‘S FLIGHT INSTRUMENTS

	
	
	

	42.1 .
	
	

	A 0050.43 DUAL AC SYSTEM

	
	
	

	43.1 .
	
	

	A 0050.44 INSTANTENOUS VERTICAL SPEED INDICATOR

	
	
	

	44.1 .
	
	

	A 0050.45 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	45.1 .
	
	

	A 0050.46 HF--ANTENNA

	
	
	

	46.1 Inspect HF--antenna for condition.
	828--3
	

	
	
	

	46.2 Inspect antenna cable ends.
	828--4
	

	
	
	

	A 0050.47 LANDING AND SEARCHLIGHT SYSTEM 450W

	
	
	

	47.1 .
	
	

	A 0050.48 ENGINE CLEANING PROVISION

	
	
	

	48.1 .
	
	

	A 0050.49 SAND FILTER

	
	
	

	49.1 .
	
	

	A 0050.50 DIGITAL AUTOMATIC FLIGHT CONTROL SYSTEM (DAFCS)

	
	
	

	50.1 .
	
	

	A 0050.51 EMERGENCY FLOAT SYSTEM MAX. TOW 3350 KG

	
	835--4, 
without
step 9
	

	51.1 Inspect emergency float system for condition.
	
	

	
	
	

	51.2 Perform trial inflation test.
	Manufacturer’s
Component
Maintenance
Manual CMM
25--63--04
	

	
	
	

	A 0050.52 SCAVENGE OIL FILTER SYSTEM

	
	
	

	52.1 .
	
	

	A 0050.53 HIGH LANDING GEAR

	
	
	

	53.1 .
	
	

	A 0050.54 WIRE STRIKE PROTECTION SYSTEM (WSPS)

	
	
	

	54.1 .
	
	

	54.2 
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0050.55 POST INSPECTION

	
	
	

	55.1 Ensure applicable servicing requirements have been carried out.
	
	

	55.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	55.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	55.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	55.5 Perform Functional Check Flight if required per BK-117 Maintenance Manual  or RFM as appropriate.
	
	

	55.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series AAIP – A 0050 – 50 Hour / 24 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




