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	SECTION:
	
	A0070 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	50 HOUR / 24 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-117 Series MM Appendix A
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0070.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	A 0070.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 0070.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 0070.4 MAIN TRANSMISSION

	4.1 
	
	

	4.2 
	
	

	A 0070.5 ROTOR BRAKE SYSTEM

	5.1 
	
	

	5.2 
	
	

	A 0070.6 MAIN ROTOR SYSTEM

	6.1 
	
	

	6.2 
	
	

	A 0070.7 MAIN ROTOR BLADE

	7.1 Perform lead--lag check or alternatively inspect the blade thimble area.
	
	

	Effectivity: Main rotor blades (blade sweep angle 1 degree) P/N 117--150001, P/N 117--150011 and all versions, 117--150021 and all versions, 117--50061 and all versions, 117--151321 and all versions, 117--151341 and all versions, 117--151351 and all versions, 117--151361 and all versions.
	

	7.2 
	
	

	7.3 
	
	

	7.4 
	
	

	A 0070.8 FUSELAGE

	
	
	

	8.1 
	
	

	
	
	

	A 0070.9 COWLINGS

	
	
	

	9.1 
	
	

	
	
	

	A 0070.10 TAIL BOOM

	
	
	

	10.1 
	
	

	
	
	

	10.2 
	
	

	
	
	

	10.3 
	
	

	
	
	

	A 0070.11 TAIL ROTOR DRIVE

	
	
	

	11.1 
	
	

	A 0070.12 TAIL ROTOR

	
	33-4 steps 1 thru 7 and 9 thru 13
	

	12.1 Inspect tail rotor for condition.
	
	

	
	
	

	12.2 Remove bellcrank and inspect for condition.
	33-10 thru 
33-12
	

	
	
	

	12.3 Remove bolts P/N 105-31717 of bellcrank and inspect for condition.
	33-9
	

	
	
	

	12.4 Remove bolts attached to tail rotor shaft/ tail rotor head and inspect for condition.
	33-21 step 1.e
	

	
	
	

	12.5 Without disassembly, inspect spherical bearings in fork end of tail rotor shaft for play, corrosion and binding
	33-21 step 1.c
	

	
	
	

	A 0070.13 TAIL ROTOR BLADE

	
	
	

	13.1 Inspect tail rotor blades for condition.
	34-2
	

	
	
	

	13.2 
	
	

	
	
	

	A 0070.14 MAIN ROTOR FLIGHT CONTROLS

	
	
	

	14.1 
	
	

	A 0070.15 TAIL ROTOR FLIGHT CONTROLS

	
	
	

	15.1 
	
	

	15.2 
	
	

	A 0070.16 HYDRAULIC SYSTEM

	
	
	

	16.1 
	
	

	A 0070.17 LANDING GEAR

	
	
	

	17.1 
	
	

	A 0070.18 FUEL SYSTEM

	
	
	

	18.1 
	
	

	A 0070.19 LUBRICATION SYSTEM

	
	
	

	19.1 
	
	

	A 0070.20 FIRE WALLS

	
	
	

	20.1 Inspect fire walls for condition.
	64-2
	

	20.2 Inspect ejector for condition.
	64-10
	

	A 0070.21 ENGINE OPERATION AND CONTROL

	
	
	

	21.1 
	
	

	A 0070.22 STANDARD EQUIPMENT

	
	
	

	22.1 
	
	

	A 0070.23 INSTRUMENT SYSTEMS

	
	
	

	23.1 Inspect instrument panel decals and all instrument markings for presence and readability.
	
	

	
	
	

	23.2 Inspect visible parts of pitot static system for condition.
	91-23
	

	
	
	

	23.3 Compensate compasses and inspect for condition.
	91-46, 91-47,
91-56
	

	
	
	

	23.4 Inspect directional gyro for function.
	91-49
	

	
	
	

	23.5 Check the following;
	

	
	

	23.5.1 Pitot system for leakage.
	91-21 step 1
	

	
	
	

	23.5.2 Airspeed indicator for correct indication.
	91-21 step 2
	

	
	
	

	23.5.3 Static system for leakage
	91-21 step 3
	

	
	step 5
	

	23.5.4 Altimeter for correct indication
	91-21 step 4
	

	
	Step 5
	

	A 0070.24 ELECTRICAL SYSTEMS

	
	
	

	24.1 
	
	

	A 0070.25 DC SUPPLY SYSTEM

	
	
	

	25.1 
	
	

	
	

	A 0070.26 EMERGENCY FLOAT SYSTEM

	
	
	

	26.1 
	
	

	A 0070.27 CARGO HOOK SYSTEM

	
	
	

	27.1 
	
	

	A 0070.28 SETTLING PROTECTORS

	
	
	

	28.1 
	
	

	A 0070.29 FIXED LANDING LIGHT -- FUSELAGE

	
	
	

	29.1 
	
	

	29.2 
	
	

	A 0070.30 FIXED LANDING LIGHT -- CROSS TUBE

	
	
	

	30.1 .
	
	

	A 0070.31 STROBE LIGHT SYSTEM

	
	
	

	31.1 .
	
	

	A 0070.32 BOARDING STEP -- LONG

	
	
	

	32.1 .
	
	

	A 0070.33 MAIN ROTOR BLADE FOLDING SYSTEM

	
	
	

	33.1 .
	
	

	A 0070.34 EXTERNAL LOUDSPEAKER SYSTEM

	
	
	

	34.1 .
	
	

	A 0070.35 AFT BATTERY

	
	
	

	35.1 
	
	

	A 0070.36 RADOM

	
	
	

	36.1 Remove radome and inspect for condition.
	815-2
	

	A 0070.37 SNOW SKIDS

	
	
	

	37.1 .
	
	

	A 0070.38 SEARCHLIGHT

	
	
	

	38.1 .
	
	

	A 0070.39 EXTERIOR MIRROR

	
	
	

	39.1 .
	
	

	A 0070.40 CARTRIDGE--TYPE FUEL PUMP

	
	
	

	40.1 .
	
	

	A 0070.41 P/R CSAS SYSTEM

	
	
	

	41.1 .
	
	

	A 0070.42 COPILOT‘S FLIGHT INSTRUMENTS

	
	
	

	42.1 .
	
	

	A 0070.43 DUAL AC SYSTEM

	
	
	

	43.1 .
	
	

	A 0070.44 INSTANTANEOUS VERTICAL SPEED INDICATOR

	
	
	

	44.1 Inspect indicator for condition.
	825--4
	

	
	
	

	44.2 Examine indicators.
	
	

	
	
	

	A 0070.45 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	45.1 Perform discharge check..
	826--10
	

	45.2 Perform functional test after charging.
	826--4
	

	45.3 Check emergency power supply unit for condition.
	826--6
	

	A 0070.46 HF--ANTENNA

	
	
	

	46.1 .
	
	

	A 0070.47 LANDING AND SEARCHLIGHT SYSTEM 450W

	
	
	

	47.1 .
	
	

	A 0070.48 ENGINE CLEANING PROVISION

	
	
	

	48.1 .
	
	

	A 0070.49 SAND FILTER

	
	
	

	49.1 Remove and inspect bypass door actuators.
	831--15 
and
831--16
	

	A 0070.50 DIGITAL AUTOMATIC FLIGHT CONTROL SYSTEM (DAFCS)

	
	831--15
and
831--16
	

	50.1 Inspect digital automatic flight control system for condition.
	
	

	A 0070.51 EMERGENCY FLOAT SYSTEM, MAX TOW 3350 KG

	
	
	

	51.1 
	
	

	A 0070.52 SCAVENGE OIL FILTER SYSTEM

	
	
	

	52.1 .
	
	

	A 0070.53 HIGH LANDING GEAR

	
	
	

	53.1 .
	
	



	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0070.54 POST INSPECTION

	
	
	

	54.1 Ensure applicable servicing requirements have been carried out.
	
	

	54.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	54.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	54.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	54.5 Perform Functional Check Flight if required per BK-117 Maintenance Manual  or RFM as appropriate.
	
	

	54.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series AAIP – A 0070 – 50 Hour / 24 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




