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	Page No:
	1

	Revision:
	Original

	Issue Date:
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	SECTION:
	
	A 0200 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	200 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-117 Series MM Appendix A
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0200.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	A 0200.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 0200.3 

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 0200.4 ROTOR BRAKE SYSTEM

	
	
	

	4.1 
	
	

	
	
	

	A 0200.5 COWLINGS

	
	
	

	5.1 
	
	

	
	
	

	A 0200.6 MAIN TRANSMISSION

	
	
	

	6.1 
	
	

	
	
	

	6.2 
	
	

	
	
	

	6.3 
	
	

	
	
	

	A 0200.7 TAIL BOOM

	
	
	

	7.1 
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0200.8 TAIL ROTOR DRIVE

	
	
	

	8.1 
	
	

	
	

	8.2 
	
	

	
	

	A 0200.9 TAIL ROTOR 

	
	
	

	9.1 
	
	

	
	
	

	9.2 
	
	

	
	
	

	A 0200.10 TAIL ROTOR BLADE

	
	
	

	10.1 
	
	

	
	

	A 0200.11 STANDARD EQUIPMENT

	
	
	

	11.1 
	
	

	
	

	A 0200.12 ELECTRICAL SYSTEMS

	
	
	

	12.1 
	
	

	A 0200.13 CARGO HOOK SYSTEM

	
	
	

	13.1 .
	
	

	A 0200.14 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	14.1 
	
	

	Note; 
	

	14.2 
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0200.15 

	
	
	

	11.1 
	
	

	
	
	

	11.2 
	
	

	
	
	

	11.3 
	
	

	
	
	

	11.4 
	
	

	
	
	

	11.5 
	
	

	
	
	

	11.6 
	
	

	
	
	

	A 0200.16 POST INSPECTION

	
	
	

	11.7 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	11.8 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	11.9 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	11.10 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	11.11 Perform Functional Check Flight if required per BK-117 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	11.12 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series AAIP – A 0153 – 100 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




