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	SECTION:
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	TYPE:
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Airbus BO-117 Series MM Appendix A

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-117 MP
	

	A 1700.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Inspect identification and lettering for readability, placards for damage and security of attachment
	IPC -- FLM
	

	A 1700.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 1700.4 MAIN TRASMISSION

	
	
	

	4.1 Remove magnetic plug and inspect for deposits, clean and test for magnetic retaining force - Requires special weighted ball bearings
	11-14 thru 11-17,
02-14
	

	
	
	

	A 1700.5 MAIN ROTOR BLADE

	
	
	

	5.1 Inspect transmission mounting struts for condition.
	14-2, step 11 h
	

	EFFECTIVITY: Lower fitting P/N 117--80166.02:
	

	A 1700.6 FUSELAGE

	
	
	

	6.1 Check jettison device for cockpit doors and cabin doors for function.
	21-5, -7, -9(A),
	

	
	-11(A)
	

	6.2 Inspect the cabin doors for condition.
	21--3 step 2
	

	
	
	

	6.3 Inspect the door spar for the cabin doors for condition.
	21--3 step 2.a
	

	
	
	





	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.7 TAIL ROTOR DRIVE

	
	
	

	7.1 Remove magnetic plugs of intermediate gearbox and tail rotor gearbox and test their magnetic retaining force - Requires special weighted ball bearings
	32-32 step 3,
02-14
	

	A 1700.8 TAIL ROTOR

	
	
	

	8.1 Lubricate the following;
	
	

	8.1.1 Ball bearings of sliding sleeve.
	33-27 step 13
	

	8.1.2 Splines of tail rotor shaft.
	
	

	A 1700.9 MAIN ROTOR CONTROLS

	
	
	

	9.1 Inspect upper rod end seals for damage.
	41-59 step 6
	

	
	
	

	9.2 Grease Swashplate bearings.
	41-53
	

	
	
	

	A 1700.10 TAIL ROTOR CONTROLS

	
	
	

	10.1 Inspect upper rod end seals for damage.
	42-31 step 4
	

	
	
	

	A 1700.11 HYDRAULIC SYSTEM

	
	
	

	11.1 Inspect rod end seals for damage. In case of damaged seals, remove control rods, disassemble and inspect for condition.
	43-32 thru 43-37
	

	
	
	

	11.2 Bleed both reservoirs
	43-5
	

	
	
	

	11.3 Inspect hydraulic system for condition.
	43-11
	

	
	
	

	11.4 Do the leakage check of the hydraulic system.
	43-12
	

	
	
	

	11.5 Functionally test hydraulic system
	43-14
	

	
	
	

	A 1700.12 LUBRICATION SYSTEM

	
	
	

	12.1 Remove chip detector, clean and test magnetic retaining force of each plug - Requires special weighted ball bearings.
	63-21, 02-14
63-23
	

	
	
	

	A 1700.13 STANDARD EQUIPMENT

	
	

	13.1 Inspect the following:
	

	
	

	13.1.1 Inspect windshield wiper system for condition and function
	702-3, 702-4
	

	
	
	

	13.1.2 Inspect fire extinguishing system for condition and function.
	702-3, 702-4
	

	
	
	

	13.1.3 Inspect hand fire extinguisher for security of attachment and proper charge
	
	

	
	
	

	13.1.4 Inspect first aid kit for completeness of contents and security of attachment
	
	

	
	
	

	13.1.5 Identification and other markings for legibility, and adhesive-backed decals for damage and proper adhesion
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.14 INSTRUMENT SYSTEM

	
	

	14.1 Inspect the following;
	

	
	

	14.1.1 Instrument panel decals for presence and readability
	
	

	
	
	

	14.1.2 Visible parts of pitot static system for condition
	91-23
	

	
	
	

	14.1.3 Directional gyro for function
	91-49
	

	
	
	

	14.2 Check the following;
	

	
	

	14.2.1 Pitot system for leakage
	91-21 step 1
	

	
	
	

	14.2.2 Airspeed indicator for correct indication
	91-21 step 2
	

	
	
	

	14.2.3 Altimeter for correct indication
	91-21 step 4
	

	
	
	

	14.2.4 Static system for leakage
	91-21 step 3
	

	
	
	

	14.3 Compensate compasses and inspect for condition
	91-46, 91-47,
	

	
	91-56
	

	A 1700.15 ELECTRICAL SYSTEMS

	
	
	

	15.1 Inspect ground leads and ground connections of fueling nozzle and fuselage/landing gear for condition.
	
	

	
	
	

	15.2 Inspect battery connector and cable for condition.
	92--65 step 1
	

	
	
	

	A 1700.16 EMERGENCY FLOAT SYSTEM MAX. TOW 2850 KG

	
	
	

	16.1 Inspect emergency float system for condition (floats installed)
	
	

	
	
	

	16.2 Check emergency float system for operational readiness. 
	802--4
	

	NOTE: Circuit breaker EMER FLOATS must be set and toggle switch EMER FLOATS must be in ARMED position. If green indicator light is not on, refer to para 802--2, TROUBLESHOOTING
	

	16.3 Perform trial inflation.
	Refer to
	

	
	manufacturer
CMM 25--60--97
	

	A 1700.17 P/R CSAS SYSTEM

	
	
	

	17.1 Inspect P/R CSAS for condition.
	821--4
	

	
	
	

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.18 INSTANTANEOUS VERTICAL SPEED INDICATOR

	
	
	

	18.1 Examine indicators
	
	

	
	
	

	A 1700.19 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	19.1 Perform discharge check
	826--10
	

	
	
	

	A 1700.20 EMERGENCY FLOAT SYSTEM MAX. TOW 3350 KG

	
	
	

	20.1 Inspect emergency float system for condition.
	835--4, without
	

	
	step 9
	

	20.2 Perform trial inflation test.
	Manufacturer’s
Component
Maintenance
Manual CMM
25--63--04
	

	
	
	

	A 1700.21 SCAVENGE OIL FILTER SYSTEM

	
	
	

	21.1 Remove magnetic plugs of intermediate gearbox and tail rotor gearbox and test their magnetic retaining force - Requires special weighted ball bearings
	836--9, 02--14,
836--10
	

	
	
	

	A 1700.22 POST INSPECTION

	
	
	

	22.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	22.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	22.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	22.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	22.5 Perform Functional Check Flight if required per BK-117 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	22.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-117 Series AAIP – A 1700 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




