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	Issue Date:
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	SECTION:
	
	A 6072 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	6000 HOUR / 72 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-117 Series MM Appendix A
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6072.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Airbus 
	

	
	BK-117 MP
	

	A 6072.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 6072.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 6072.4 MAIN TRANSMISSION

	
	
	

	4.1 Inspect main transmission for condition.
	11-3 steps 1 and 2 and 4 thru 6
	

	
	
	

	4.2 Remove chip detector, clean and test magnetic retaining force.
	11-14 thru 11-17
	

	
	
	

	4.3 Inspect transition radius in the flange area for cracks.
	
	

	Effectivity: Slider guide P/N 4639305053, P/N 4639305030
	

	A 6072.5 ROTOR BRAKE SYSTEM

	
	
	

	5.1 Inspect rotor brake system for condition.
	2-3
	

	
	
	

	A 6072.6 FUSELAGE

	
	
	

	6.1 Inspect fuselage for condition.
	21-3
	

	
	
	

	6.2 Check jettison device of cockpit doors and cabin doors for function.
	21-5, -7,
-9(A), -11(A)
	

	
	
	

	A 6072.7 COWLINGS

	
	
	

	7.1 Visually inspect goosenecks for cracks.
	22-9 thru 22-11
	

	
	
	

	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6072.8 TAIL BOOM

	
	
	

	8.1 Inspect tail boom for condition.
	31-2
	

	A 6072.9 TAIL ROTOR DRIVE

	
	
	

	9.1 Inspect tail rotor gear box attaching hardware for proper torque and tighten as necessary.
	32-37
	

	9.2 Inspect tail rotor drive for condition.
	
	

	
	
	

	9.3 Test magnetic plugs of intermediate gear box and tail rotor transmission for magnetic retaining force.
	32-32 step 3,
02-14
	

	
	
	

	A 6072.10 TAIL ROTOR

	
	
	

	10.1 Inspect tail rotor for condition.
	33-4 steps 1 thru
	

	
	7 and 9 thru 13
	

	10.2 Remove bellcrank and inspect for condition.
	33-10 thru 33-12
	

	10.3 Remove bolts attaching tail rotor shaft to tail rotor head and inspect for condition.
	33-21 step 1
	

	
	
	

	10.4 Without disassembly, inspect spherical bearings in fork end of tail rotor shaft for play, corrosion and roughness.
	33-21 step 1
	

	
	
	

	A 6072.11 TAIL ROTOR BLADE

	
	
	

	11.1 Inspect tail rotor blades for condition.
	34-2
	

	
	
	

	A 6072.12 MAIN ROTOR FLIGHT CONTROLS 

	
	
	

	12.1 Inspect flight controls tail rotor located in front of actuator for free movement, play and condition.
	42-3
	

	12.2 Inspect upper rod end seals for damage.
	42-31 step 4
	

	A 6072.13 TAIL ROTOR FLIGHT CONTROLS 

	
	
	

	13.1 Inspect flight controls tail rotor located in front of actuator for free movement, play and condition.
	42-3
	

	13.2 Inspect upper rod end seals for damage.
	
	

	A 6072.14 HYDRAULIC SYSTEM

	
	
	

	14.1 Inspect rod end seals for damage. In case of damaged seals, remove control rods, disassemble and inspect for condition.
	43-32 thru 43-37
	

	14.2 Bleed both reservoirs.
	43-5
	

	14.3 Inspect hydraulic system for condition.
	43-11
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	14.4 Do the leakage check of the hydraulic system.
	43-12
	

	14.5 Do the functional test of the hydraulic system.
	43-14
	

	A 6072.15 LANDING GEAR

	
	
	

	15.1 Inspect landing gear for condition
	51-2
	

	A 6072.16 FUEL SYSTEM

	
	
	

	16.1 Check fuel shutoff valves for function and evidence of leakage.
	62-39 step 5
	

	16.2 Inspect fuel system for leakage.
	62-40
	

	A 6072.17 LUBRICATION SYSTEM

	
	
	

	17.1 Remove chip detectors, clean and test magnetic retaining force.
	63-21,02-14,
63-23
	

	17.2 Inspect lubrication system for condition.
	63-3
	

	A 6072.18 FIRE WALLS

	
	
	

	18.1 Inspect fire walls for condition.
	64-2
	

	18.2 Inspect ejector for condition.
	64-10
	

	A 6072.19 ENGINE OPERATION AND CONTROL

	
	
	

	19.1 Inspect engine operation and controls for condition.
	65-3
	

	A 6072.20 STANDARD EQUIPMENT

	
	
	

	20.1 Inspect the following;
	
	

	20.1.1 Identification and lettering for readability, placards for damage and security of attachment.
	IPC – FLM
	

	20.1.2 Windshield wiper system for condition and function.
	702-3, 702-4
	

	20.1.3 Fire extinguishing system for condition and function
	706-3, 706-4
	

	20.1.4 YAW system for condition
	709-3
	

	20.1.5 Hand fire extinguisher for security of attachment and proper charge.
	
	

	20.1.6 First aid kit for completeness of contents and security of attachment.
	
	

	A 6072.21 INSTRUMENT SYSTEMS

	
	
	

	21.1 Inspect instrument panel decals and all instrument markings for presence and readability.
	
	

	
	
	

	21.2 Inspect visible parts of pitot static system for condition.
	91-23
	

	
	
	

	21.3 Compensate compasses and inspect for condition.
	91-46, 91-47,
91-56
	

	
	
	

	21.4 Inspect directional gyro for function.
	91-49
	

	
	
	

	21.5 Check the following;
	

	
	

	21.5.1 Pitot system for leakage.
	91-21 step 1
	

	
	
	

	21.5.2 Airspeed indicator for correct indication.
	91-21 step 2
	

	
	
	

	21.5.3 Static system for leakage
	91-21 step 3
	

	
	
	

	21.5.4 Altimeter for correct indication
	91-21 step 4
	

	
	
	

	A 6072.22 ELECTRICAL SYSTEMS

	
	
	

	22.1 Inspect ground leads and ground connections of fueling nozzle and fuselage/landing gear for condition.
	
	

	22.2 
	
	

	A 6072.23 EMERGENCY FLOAT SYSTEM

	
	
	

	23.1 Check emergency float system for operational readiness.
	
	

	Note:  Circuit breaker EMER FLOATS must be set and toggle switch EMER FLOATS must be in ARMED position. If green indicator light is not on, refer to para 802--2, TROUBLESHOOTING
	

	23.2 Inspect emergency float system for condition (floats removed).
	802--4
	

	23.3 Perform trial inflation.
	Refer to
manufacturer
CMM 25--60--97
	

	A 6072.24 CARGO HOOK SYSTEM

	
	
	

	24.1 Inspect cargo hook system fittings for cracks.
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6072.25 SETTLING PROTECTORS

	
	
	

	25.1 Inspect settling protectors for condition.
	804--3
	

	A 6072.26 FIXED LANDING LIGHT -- FUSELAGE

	
	
	

	26.1       Inspect fixed landing light for condition.
	808--5
	

	
	
	

	A 6072.27 FIXED LANDING LIGHT -- CROSS TUBE

	
	
	

	27.1      Inspect fixed landing light for general condition.
	809--4
	

	
	
	

	A 6072.28 STROBE LIGHT SYSTEM

	
	
	

	28.1      Inspect strobe light system for condition.
	810--5
	

	
	
	

	A 6072.29 BOARDING STEP -- LONG

	
	
	

	29.1       Inspect boarding step for condition.
	811--2
	

	
	
	

	A 6072.30 MAIN ROTOR BLADE FOLDING SYSTEM

	
	
	

	30.1       Remove, clean and inspect safety lever assembly for cracks and condition.
	812--3
	

	
	
	

	A 6072.31 EXTERNAL LOUDSPEAKER SYSTEM

	
	
	

	31.1       Inspect external loudspeaker system for condition.
	813--4
	

	
	
	

	A 6072.32 AFT BATTERY

	
	
	

	32.1 Check battery power system for condition.
	814--3
	

	
	
	

	A 6072.33 RADOM

	
	
	

	33.1        Remove radome and inspect for condition.
	815--2
	

	
	
	

	A 6072.34 PROTECTIVE COVERS FOR DUAL CONTROLS

	
	
	

	34.1       Check protective covers for condition.
	816--2
	

	
	
	

	A 6072.35 EXTERIOR MIRROR

	
	
	

	35.1       Check mirror for condition.
	819--3
	

	
	
	

	A 6072.36 SEARCHLIGHT

	
	
	

	36.1       Perform functional test of searchlight
	818--4
	

	
	
	

	37.1       Inspect searchlight for condition.
	818--5
	

	
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6072.37 EXTERIOR MIRROR

	
	
	

	37.1       Check mirror for condition.
	819--3
	

	
	
	

	A 6072.38 CARTRIDGE--TYPE FUEL PUMP

	
	
	

	38.1       Check fuel pump for condition.
	820--3
	

	
	
	

	A 6072.39 P/R CSAS SYSTEM

	
	
	

	39.1        Inspect P/R CSAS for condition.
	821--4
	

	
	
	

	A 6072.40 COPILOT‘S FLIGHT INSTRUMENTS

	
	
	

	40.1        Inspect instrument lighting -- copilot for condition
	822--5
	

	
	
	

	A 6072.41 DUAL AC SYSTEM

	
	
	

	41.1        Inspect system for condition
	823--5
	

	
	
	

	42.1        Test conducting and blocking function of diodes.
	
	

	
	
	

	Effectivity: Only applicable to helicopters S/N 7183 and prior, equipped with DAFCS system
	

	A 6072.42 INSTANTENOUS VERTICAL SPEED INDICATOR

	
	
	

	42.1         Check indicator for condition.
	825--4
	

	
	
	

	42.2         Examine indicators
	
	

	
	
	

	A 6072.43 EMERGENCY POWER SUPPLY -- STANDBY HORIZON

	
	
	

	43.1        Perform discharge check
	826--10
	

	
	
	

	A 6072.44 HF--ANTENNA

	
	
	

	44.1        Inspect HF--Antenna for condition.
	
	

	
	
	

	44.2        Inspect antenna cable ends.
	
	

	
	
	

	A 6072.45 LANDING AND SEARCHLIGHT SYSTEM 450W

	
	
	

	45.1        Check condition of the system..
	829--4
	

	
	
	

	45.2         Carry out functional test on system.
	829--5
	

	
	
	

	A 6072.46 ENGINE CLEANING PROVISION

	
	
	

	46.1         Inspect engine water washing provision for condition.
	830--2
	

	
	
	




	


	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6072.47 SAND FILTER

	
	
	

	47.1          Remove and inspect bypass door actuators.
	831--15 and
831--16
	

	
	
	

	A 6072.48 DIGITAL AUTOMATIC FLIGHT CONTROL SYSTEM (DAFCS)

	
	
	

	48.1          Inspect digital automatic flight control system for condition.
	833--4
	

	
	
	

	A 6072.49 EMERGENCY FLOAT SYSTEM, MAX TOW 3350 KG

	
	
	

	49.1          Inspect emergency float system for condition.
	835--4
	

	
	
	

	49.2          Perform trial inflation test.
	Manufacturer’s
Component
Maintenance
Manual CMM
25--63--04
	

	
	
	

	A 6072.50 SCAVENGE OIL FILTER SYSTEM

	
	
	

	50.1          Remove chip detector and test magnetic retaining force.
	836--9, 02--14,
836--10
	

	
	
	

	A 6072.51 HIGH LANDING GEAR

	
	
	

	51.1          Inspect high landing gear for condition.
	840--3
	

	
	
	

	A 6072.52 WIRE STRIKE PROTECTION SYSTEM (WSPS)

	
	
	

	52.1          Inspect WSPS for condition.
	844--3
	

	
	
	

	A 6072.53 POST INSPECTION

	
	
	

	53.1           Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	53.2           Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	53.3           Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	53.4           Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	53.4           Perform Functional Check Flight if required per BK-117 Maintenance Manual  or  RFM as appropriate.
	
	

	
	
	

	53.6           Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Airbus MBB BK-117 Series AAIP – A 6072 – 6000 Hour / 72 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




