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	Issue Date:
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	SECTION:
	
	A 1700 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 1700.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 1700.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 1700.4 MAIN TRANSMISSION

	
	11-17, 11-19,
	

	4.1 Remove magnetic plug and test magnetic retaining force.
	11-18, 02-14
	

	Note: Special tooling required - Weighted ball bearings
	

	4.2 Inspect transmission mounting struts for condition.
	
	

	Effectivity: Transmission mounting struts P/N 105--10161 and 105--10162: 
	

	4.3 Visually inspect area of support tube flange for cracks.
	11-3, step 12
	

	
	
	

	A 1700.5 FUSELAGE

	
	
	

	5.1 Inspect landing gear mounting brackets and surrounding fuselage area for condition.
	21-3, step 10.
	

	
	
	

	5.2 Clean, grease and functionally check jettison device of cockpit doors. Renew lead wire seal
	21-4
	

	
	
	

	A 1700.6 TAIL ROTOR DRIVE

	
	
	

	6.1 Remove magnetic plugs of intermediate gearbox and tail rotor gearbox and test their magnetic retaining force.
	32-9, 02-14
	

	Note: Special tooling required - Weighted ball bearings
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.7 MAIN ROTOR CONTROLS

	
	
	

	7.1 Visually inspect seals on upper rod ends of control rods for damage.
	41-3
	

	
	
	

	The following control rods are affected:
	

	7.1.1 Vertical control rods below hydraulic unit (3 off)
	
	

	
	
	

	7.1.2 Control rods between hydraulic unit and mixing lever assy (3 off)
	
	

	
	
	

	7.1.3 Rotating control rods (4 off)
	
	

	
	
	

	7.2 Check rigging of collective control forces
	102-16, step 9.
	

	Note: Special tooling required - Hydraulic Mule
	

	7.3 Visually inspect reinforcement sleeves on control rod ends for cracks. Replace cracked control rods
	
	

	Effectivity: Rotating control rods P/N 105--13121: Distinguishing feature of control rod - O.D. of tube is 20 mm
	

	
	
	

	7.4 Clean swash plate sliding surface on support tube. Move swash plate to uppermost position to expose sliding surface. Use cleaning solvent (CM 201, 202 or 217)
	
	

	Note: Use cleaning solvent (CM 201, 202 or 217)
	

	7.5 
	
	

	
	
	

	A 1700.8 TAIL ROTOR CONTROLS

	
	
	

	8.1 Visually inspect the seals on the rod ends and clevis for damage.
	42-3
	

	
	
	

	The following rods are affected:
	

	8.1.1 Control rod in the tail boom
	
	

	
	
	

	8.1.2 Control rod in vertical fin (upper clevis)
	
	

	
	
	

	8.2 Control rod in vertical fin: Visual inspect sealing of blind hole in fork end for damage.
	
	

	
	
	

	8.2.1 
	
	

	
	
	

	A 1700.9 HYDRAULIC SYSTEM

	
	
	

	9.1 Inspect hydraulic system for condition. 
	43-11
	

	
	
	

	9.2 Spray-coat N2-lever (droop-compensation) with corrosion preventive compound (CM 508)
	
	

	
	
	

	9.3 Check filter contamination indicator (lateral indicator pin configuration)
	43-14
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	9.4 Functionally test hydraulic system
	43-15
	

	
	
	

	9.5 Perform ground run check of selector valve setting.
	43-16 or 43-16A
	

	Note: Write up and sign off AD separately in the aircraft logbook.
	AD 98 08 04
	

	9.6 Inspect system 1 selector valve for corrosion
	
	

	
	
	

	A 1700.10 FUEL SYSTEM

	
	
	

	10.1 Check fuel differential pressure switch for function.
	62-39
	

	
	
	

	10.2 Perform functional test and leakage test of fuel shutoff valves.
	92-82, 92-83
	

	
	
	

	A 1700.11 STANDARD EQUIPMENT

	
	
	

	11.1 Inspect cabin equipment for condition.
	02-2
	

	
	
	

	11.2 Inspect cabin ventilation for condition, check for function
	704-2
	

	
	
	

	11.3 Inspect identification and other markings for legibility, and adhesive-backed decals for damage and proper adhesion
	
	

	
	
	

	11.4 Inspect harnesses, buckles and inertia reels for condition
	701-2
step 5, 6 and 7
	

	
	
	

	A 1700.12 INSTRUMENT SYSTEM

	
	
	

	12.1 Ventilate dual torque indication system.
	91-57
	

	
	
	

	12.2 Inspect instruments for condition.
	91-4
	

	
	
	

	12.3 Clean and drain pitot-static system, inspect for condition and check for function
	91-9 thru 91-12
	

	
	
	

	12.4 Inspect magnetic compass for condition and function and compensate magnetic compass.
	91-24 thru 91-26
	

	Note: Requires Master Compass
	

	12.5 Calibrate TOT indication system.
	91-45
	

	Note: Requires Barfield Tester
	

	12.6 Inspect instrument panel, center panel and overhead panel for presence, legibility and security of labels and placards.
	
	

	Note: Replace missing placards and rebond separated placards
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.13 ELECTRICAL SYSTEMS

	
	
	

	13.1 Inspect socket of anti-collision light for condition.
	92-116
	

	
	
	

	13.2 Inspect battery--temparature warning.
	92--34E
	

	
	
	

	13.3 Inspect battery connector and cable.
	92--28 step 1
	

	
	
	

	A 1700.14 CHIP WARNING INDICATION

	
	
	

	14.1 Remove chip detector and test magnetic retaining force.
	
	

	Note: Special tooling required - Weighted ball bearings
	

	14.2 
	
	

	
	
	

	A 0051.7 POST INSPECTION

	
	
	

	7.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	7.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	7.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	7.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.5 Perform Functional Check Flight if required per Bell 206L Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	7.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 1700 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




