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	SECTION:
	
	B 0192NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	150 HOUR INSPECTION

	NOTE:
	
	NO TOLERANCE 

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C47B Operation and Maintenance Manual Table 606
NOTE: This inspection is for ONLY for engines operating with 3rd Generation oil 

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0192.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce M250-C47B Operations and Maintenance Manual).
	250-C47B MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce M250-C47B Operations and Maintenance Manual).
	250-C47B MP
	

	
	
	

	B 0192.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	B 0192.3 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	3.1 Inspect the following:
	

	
	

	3.1.1 Engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	
	

	
	
	

	3.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	

	3.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened
	
	

	
	
	

	3.1.4 Compressor impeller leading edges for damage.
	
	

	
	
	

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	3.1.5 Without disassembly, turbine, exhaust collector supports and the air tubes for cracks, buckling and general condition.
	
	

	
	
	

	3.2 Examine the duct and the clamp for condition and security.
	
	

	
	
	

	3.2.1 Without disassembly, turbine, exhaust collector supports and the air tubes for cracks, buckling and general condition.
	
	

	
	
	

	3.2.2 Fuel system for evidence of leakage – Check condition and security of fittings and tubing
	
	

	
	
	

	3.2.3 Engine mount, fittings and legs for condition and security.
	Chapter 71
	

	
	
	

	3.2.4 Electrical harness for loose, chafed, frayed, or broken wires, loose connectors.
	
	

	
	
	

	3.2.5 Fuel system for evidence of leakage – Check condition and security of fittings and tubing
	
	

	
	
	

	3.2.6 Engine mount for condition and security.
	
	

	
	
	

	3.2.7 Electrical harness for loose, chafed, frayed, or broken wires, loose connectors.
	
	

	
	
	

	B 0192.4 FREEWHEEL ASSEMBLY

	
	
	

	4.1 Examine the freewheel assembly for condition, leaks and security.
	Chapter 63
	

	4.2 Examine the freewheel chip detector for metal particles.
	
	

	
	
	

	4.3 Examine the electrical circuit of the chip detectors for continuity.
	Chapter 96
	

	
	
	

	B 0192.5 ENGINE TO TRANSMISSION DRIVSHAFT

	
	
	

	5.1 Examine the engine to transmission driveshaft for condition and security.
	Chapter 63
	

	5.2 Examine the components as follows:
	
	

	
	
	

	5.2.1 Driveshaft for corrosion, surface damage and cracked spring.
	
	

	
	
	

	5.2.2 Flexframe and bolts for condition and signs of slippage.
	
	

	
	
	

	B 0192.6 ROTOR BRAKE DISC

	
	
	

	6.1 Examine the rotor brake disc for condition and security.
	Chapter 63
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.2 Check oil supply level.
	
	

	
	
	

	NOTE
If the engine has been idle for more than 15 minutes, motor the engine for 30 seconds to scavenge any oil that may have drained into the gearbox from the oil tank. Failure to completely scavenge the oil from the gearbox will cause a false indication of high oil consumption.
	72-00-00,Table 101
Troubleshooting items 11 and 12
	

	CAUTION: NORMAL ENGINES USE A MINIMAL AMOUNT OF OIL. HOWEVER, ANY SUDDEN INCRREASE IN OIL CONSUMTION IS INDICATIVE OF OIL SYSTEM PROBLEMS AND MUST BE CORRECTED.
	

	NOTE

Check oil supply level within 15 minutes of engine shutdown.
	

	6.3 Inspect for extension of scavenge oil filter bypass indicator on CEFA
	72-60-00 para 1.E
	

	
	
	

	If the bypass indicator is extended, examine/clean the engine oil filter and the scavenge oil filter.  If contamination is found, replace the scavenge oil filter.  If no contamination is found, reinstall the scavenge oil filter with new packing and manually reset the indicator.

If the CEFA bypass indicator is extended and contamination is found in the scavenge oil filter, replace/clean the oil cooler, oil tank and lubrication lines (Reef. The airframe manual instructions). Drain and replace the engine oil and manually reset the indicator
	
	

	NOTE

If metal contamination is found in the scavenge oil filter in CEFA and a chip light occurred within the previous 50 hours, take the applicable maintenance steps (Ref. 72-00-00, para 8.E.(2), Engine Servicing or 72-60-00 para 4.B.()).
	

	NOTE

The scavenge oil filter cannot be cleaned.
	

	6.4 Inspect for extension of impending fuel filter bypass indicator.  If indicator is extended, replace fuel filter. Ground run engine to assure proper operation of control system.
	73-10-02, para 2.B
	

	6.5 Remove and disassemble fuel nozzle. Clean and inspect fuel nozzle filter assembly. Assemble and install fuel nozzle.
	73-10-03
	

	
	
	

	6.6 Install fuel nozzle with proper number of spacers.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0192.7 POST INSPECTION

	
	
	

	7.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.2 Ground run aircraft - Inspect for operation and leaks.
	
	

	
	
	

	7.3 Perform HMU MANUAL MODE Operation Function.
	72-00-00 para 7.C.(1), MANUAL MODE CHECK
	

	
	
	

	NOTE

Record must indicate that shutdown per referenced section has been performed at least once each 150 hours
	

	7.4 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	7.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	7.6 Enter in the log book any torque checks that may be due.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 407 AAIP 150 Hour – B 0191NT – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


