	MARITIME HELICOPTERS
	Bell Model 407 AAIP

	
	

	Page No:
	2

	Revision:
	Rev. Orig

	Issue Date:
	03/01/14

	SECTION:
	
	B 0301NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 6 MONTH ENGINE OIL CHANGE

	NOTE:
	
	No  Tolerance



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C47B Operation and Maintenance Manual.

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

INITIALS

	B 0301.1 GENERAL

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C47B MP
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C47B MP
	

	B 0301.2 ENGINE

	
	
	

	2.1 Drain the oil system and refill.


	72-00-00, Para 8.D., Engine Servicing.
	

	Applicability – For engines not running Third Generation oils
	

	B 0301.3 POST INSPECTION

	3.1 Inspect for operation and leaks.
	
	

	3.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	3.3 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	3.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	3.5 Enter in the log book any torque checks that may be due. 
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Bell 407 AAIP 300 Hour / 6 Month – B 0301NT – Engine oil change and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


