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	TYPE:
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	1Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0353.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 0353.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 0353.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 0353.4 MAIN TRANSMISSION

	
	
	

	4.1 Inspect magnetic plug of main transmission for deposits and clean magnetic plug
	11-18
	

	
	
	

	4.2 Inspect filter element for deposits. Clean filter if applicable.
	11-13
	

	
	
	

	A 0353.5 TAIL BOOM ASSEMBLY

	
	
	

	5.1 Remove tail rotor shaft fairing and visually inspect in the vicinity of the three bearing brackets (P/N 105--30251.17/.18/.19) for cracks. Refer to AB 15 for further limitations
	
	

	Effectivity; Tail boom assemblies up to S/N 350, if AB 15 not accomplished:
	

	5.2 Inspect tail rotor gearbox attach fitting in vertical fin for loose rivets and cracks
	31-2, step 5.
	

	
	
	

	A 0353.6 TAIL ROTOR DRIVE

	
	
	

	6.1 Visually inspect flange housing transition area for cracks and conditions indicating presence of cracks, such as oil leakage and accumulation of dirt
	32-56
	

	Effectivity; “Single webbed” type of gearbox housing (see Fig. 32-23): 
	





	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0353.7 TAIL ROTOR 

	
	
	

	7.1 Without disassembly, inspect spherical bearings in fork end of tail rotor shaft for play
	33-21, step 1.c
	

	
	
	

	7.2 Inspect flapping hinge function.
	33-4, step 3
	

	
	
	

	7.3 Remove bolt connecting tail rotor shaft to tail rotor head, and clean and inspect bolt for condition
	33-21, step 1.e.
	

	
	
	

	A 0353.8 TAIL ROTOR BLADE

	
	
	

	8.1 Inspect tail rotor blade for impact damage and cracks in surface protection. The cover tape in the nose area does not have to removed.
	34-2, steps 2., 4., 6. thru 9., 12., 13.
	

	Effectivity; Pre SB BO 105--30--112: all tail rotor blades except P/N: 105-31791, 105--317915, 105--31793, 105--31970, 105--31980 Post SB BO 105--30--112: all tail rotor blades except BO 105 CBS--5KLH and BO 105 CB--3
	

	A 0353.9 LUBRICATION SYSTEM

	
	
	

	9.1 Visually inspect baffle plate, located between oil cooler and fan, and attaching clamps for cracks
	
	

	Effectivity; Ram air ventilation not installed
	

	A 0353.10 CHIP WARNING INDICATION

	
	
	

	10.1 Inspect electrical chip detector on main transmission for deposits, then clean and functionally check chip detector
	845-5
	

	10.2 Inspect magnetic plugs of tail rotor gearbox and intermediate gearbox for deposits and clean magnetic plugs
	32-56
	

	A 0353.11 CONTINUOUS IGNITION SYSTEM

	
	
	

	11.1 Check spark igniters for condition
	857-4
	

	A 0353.12 HYDRAULIC SYSTEM

	
	
	

	12.1 Change hydraulic fluid.
	43-6
	

	
	
	

	12.2 Inspect flat springs of hydraulic system II for correct functioning.
	43-19
	

	
	
	

	12.3 Grease splines of hydraulic pump drive shaft.
	43-27, 43-29
	

	
	
	

	12.4 Change filter elements
	43-31, 43-32
	

	Note: If the hydraulic unit was not returned to service after filter replacement, the filter need not be replaced again until 2 years after return to service
	

	A 0353.13 MAIN ROTOR CONTROLS

	
	
	

	13.1 Inspect bearing forks of swashplate control ring and swashplate bearing ring for cracks
	41-3 step 4.d
	

	13.2 Grease swashplate bearing
	41-74
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0353.14 POST INSPECTION

	
	
	

	14.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	14.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	14.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	14.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	14.5 Perform Functional Check Flight if required per BO 105 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	14.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 0353 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




