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	Page No:
	4

			Revision:
	Orig
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	12/30/14

	SECTION:
	
	A 1700 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 1700.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 1700.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 1700.4 MAIN TRASMISSION

	
	
	

	4.1 Visually inspect area of support tube flange for cracks
	11-3, step 12.
	

	
	
	

	4.2 Remove magnetic plug and inspect for deposits, clean and test for magnetic retaining force - Requires special weighted ball bearings
	11-17, 11-18,
11-19, 02-14
	

	
	
	

	4.3 Inspect transmission mounting struts for condition.
	11-3, step 10.
	

	EFFECTIVITY: Transmission mounting struts P/N 105--10161 and 105--10162:
	

	A 1700.5 FUSELAGE

	
	
	

	5.1 Inspect landing gear mounting brackets and surrounding fuselage area for condition
	21-3, step 10.
	

	
	
	

	5.2 Clean, grease and functionally check jettison device of cockpit doors. Renew lead wire seal
	21-4
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.6 TAIL ROTOR DRIVE

	
	
	

	6.1 Remove magnetic plugs of intermediate gearbox and tail rotor gearbox and test their magnetic retaining force - Requires special weighted ball bearings
	32-9, 02-14
	

	A 1700.7 MAIN ROTOR CONTROLS

	
	
	

	7.1 Check rigging of collective control forces - Requires hydraulic mule.
	102-16, step 9.
	

	
	
	

	7.2 Clean swash plate sliding surface on support tube. Move swash plate to uppermost position to expose sliding surface. Use cleaning solvent (CM 201, 202 or 217)
	
	

	
	
	

	7.3 Visually inspect the seals on the upper rode ends of the following control rods for damage/condition;
	

	
	

	7.3.1 Vertical control rods below hydraulic unit (3 off)
	41-3
	

	
	
	

	7.3.2 Control rods between hydraulic unit and mixing lever assy (3 off)
	
	

	
	
	

	7.3.3 Rotating control rods (4 off)
	
	

	
	
	

	7.4 Visually inspect reinforcement sleeves on control rod ends for cracks. Replace cracked control rods.
	
	

	EFFECTIVITY: Distinguishing feature of control rod: O.D. of tube is 20 mm
	

	A 1700.8 TAIL ROTOR CONTROLS

	
	

	8.1 Visually inspect the seals on rod ends and clevis for damage on the following;
	

	
	

	8.1.1 Control rod in the tail boom
	42-3
	

	
	
	

	8.1.2 Control rod in vertical fin (upper clevis)
	
	

	
	
	

	8.2 Visual inspect sealing of blind hole in fork end for damage in control rod in vertical fin.
	
	

	
	
	

	A 1700.9 HYDRAULIC SYSTEM

	
	
	

	9.1 Inspect hydraulic system for condition.
	43-11
	

	
	
	

	9.2 Spray-coat N2-lever (droop-compensation) with corrosion preventive compound (CM 508).
	
	

	
	
	

	9.3 Check filter contamination indicator (lateral indicator pin configuration).
	43-14
	

	
	
	

	9.4 Perform ground run check of selector valve setting.
	43-16 or 43-16A
	

	
	
	

	9.5 Inspect system 1 selector valve for corrosion.
	3-13
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.10 FUEL SYSTEM

	
	
	

	10.1 Check fuel differential pressure switch for function.
	62-39
	

	
	
	

	10.2 Perform functional test and leakage test of fuel shutoff valves.
	92-82, 92-83
	

	
	
	

	A 1700.11 LUBRICATION SYSTEM

	
	
	

	11.1 Remove oil drain plugs of oil tank and test magnetic retaining force of each plug - Requires special weighted ball bearings.
	63-4, step 1.b.,
02-14
	

	
	
	

	A 1700.12 STANDARD EQUIPMENT

	
	

	12.1 Inspect the following:
	

	
	

	12.1.1 Harnesses, buckles and inertia reels for condition
	701-2
step 5, 6 and 7
	

	
	
	

	12.1.2 Cabin equipment for condition
	702-2
	

	
	
	

	12.1.3 Cabin ventilation for condition, check for function
	704-2
	

	
	
	

	12.1.4 Interior paneling and floor covering for condition
	703-2
	

	
	
	

	12.1.5 Identification and other markings for legibility, and adhesive-backed decals for damage and proper adhesion
	
	

	
	
	

	A 1700.13 INSTRUMENT SYSTEM

	
	
	

	13.1 Ventilate dual torque indication system.
	91-57
	

	
	
	

	13.2 Inspect instruments for condition.
	91-4
	

	
	
	

	13.3 Clean and drain pitot-static system, inspect for condition and check for function
	91-9 thru 91-12
	

	
	
	

	13.4 Inspect magnetic compass for condition and function and compensate magnetic compass - Requires master compass
	91-24 thru 
91-26
	

	
	
	

	13.5 Calibrate TOT indication system - Requires Barfield
	91-45
	

	
	
	

	13.6 Inspect instrument panel, center panel and overhead panel for  presence, legibility and security of labels and placards
	
	

	NOTE: Replace missing placards and rebond separated placards
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.14 ELECTRICAL SYSTEMS

	
	
	

	14.1 Inspect socket of anti-collision light for condition.
	92-116
	

	
	
	

	14.2 Inspect battery--temperature warning.
	92--34E
	

	
	
	

	14.3 Inspect battery connector and cable.
	92--28 step 1
	

	
	
	

	A 1700.15 CHIP WARNING INDICATION

	
	
	

	15.1 Remove chip detector and test magnetic retaining force - Requires special weighted ball bearings.
	845-4, 845-6,
	

	
	02-14
	

	A 0051.16 POST INSPECTION

	
	
	

	16.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	16.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	16.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	16.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	16.5 Perform Functional Check Flight if required per BO-105 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	16.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 1700 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




