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	Page No:
	1

	Revision:
	1

	Issue Date:
	01/15/16

	SECTION:
	
	A 3049 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	3000 HOUR / 48 MONTH HYD PACK INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3049.1 HYDRAULIC SYSTEM

	
	
	

	1.1 Remove, disassemble and inspect control rods for condition. S/N _____________
	43-36, 43-37
	

	
	41-79, 41-80
	

	A 3049.2 POST INSPECTION

	
	
	

	2.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	2.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	2.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	2.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	2.5 Perform Functional Check Flight if required per BO-105 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	2.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	







Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 3049 – 3000 Hour / 48 Month Hyd Pack Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




