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Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	[bookmark: _GoBack]
	

	A 6090.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 6090.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 6090.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s accessed during this AAIP inspection.
	
	

	A 6090.4 MAIN TRASMISSION

	
	
	

	4.1 Inspect main transmission and attached parts for condition.
	11-3
	

	
	step 1. thru 16.
	

	4.2 Remove magnetic plug and inspect for deposits, clean and test for magnetic retaining force.
	11-17, 11-18,
11-19, 02-14
	

	
	
	

	4.3 Inspect underside of rotor mast flange in the area of bores, including webs between the bores, for cracks, using a magnifying glass
	AD 97 26-02
	

	A 6090.5 ROTOR BRAKE SYSTEM

	
	
	

	5.1 Inspect rotor brake system for condition
	12-3
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	A 6090.6 MAIN ROTOR SYSTEM

	
	
	

	6.1 Inspect main rotor system for condition
	13-3
	

	
	
	

	6.2 Remove primary bolts and secondary bolts, clean and inspect for condition; crack inspection not necessary
	13-10, -11, -14,
-16, -17, -18
	

	
	
	

	A 6090.7 MAIN ROTOR BLADE

	
	
	

	7.1 Inspect main rotor blade for condition
	14-2 or 14-3
	

	NOTE: Note following when inspecting erosion protective shells for debonding: When first-time debonds are found, or existing debonds have increased in area, the inspection shall be repeated after 50Fh. Only when an inspection has revealed no further debonding do the periodic inspection intervals re-apply
	

	A 6090.8 FUSELAGE

	
	

	8.1 Inspect following frames for cracks:
	

	
	

	8.1.1 Upper corners of frames 7, 8, 9, forward and aft, and diagonal frame and frame 10.
	
	

	
	
	

	8.1.2 Lower frame segments 7 and 8.
	
	

	
	
	

	NOTE: Stop-drill cracks. Repair any cracks in the upper area of frames 7 and 9 and diagonal frame within the next 50Fh. Repair any cracks in the upper area of frames 8 and 10 and in the lower area of frames 7 and 8 within the next 600Fh. Check for crack propagation every 200Fh. Repair cracks which show propagation within the next 50Fh.
	

	8.2 Inspect landing gear mounting brackets and surrounding fuselage area for condition
	21-3, step 10.
	

	
	
	

	8.3 Inspect transmission strut attach fittings and engine mount attach fittings for condition and inspect fuselage area adjacent to attach fittings for loose rivets and cracks
	21-3,
step 5 and 7
	

	
	
	

	8.4 Clean, grease and functionally check jettison device of cockpit doors. Renew lead wire seal.
	21-4
	

	
	
	

	8.5 Ensure drain holes are not obstructed.
	21-3, step 4.
	

	
	
	

	A 6090.9 TAILBOOM

	
	
	

	9.1 Inspect tail boom assembly for condition.
	31-2
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6090.10 TAIL ROTOR DRIVE

	
	
	

	10.1 Inspect tail rotor drive for condition
	33-4, step 1 -- 7
	

	
	
	

	10.2 Remove magnetic plugs of intermediate gearbox and tail rotor gearbox and test their magnetic retaining force
	32-9, 02-14
	

	
	
	

	A 6090.11 TAIL ROTOR

	
	
	

	11.1 Inspect tail rotor for condition
	33-4, step 
1 -- 7
	

	
	
	

	11.2 Remove and inspect blade mounting forks for condition.
	33-14 thru 33-18
	

	EFFECTIVITY: Tail rotor blade mounting forks made from aluminum alloy P/N 105--31711, 105--31722
	

	11.3 Remove bellcrank assy and inspect for condition
	33-9 thru 33-12
	

	
	
	

	11.4 Check ball bearings of sliding sleeve for proper running and absence of play.
	33-27, step 14
	

	
	
	

	11.5 Inspect balance weight and control lever for condition.
	33-12C
	

	NOTE: Enter AD 2013-16-13 as separate entry in logbook and sign off
	
	

	A 6090.12 TAIL ROTOR BLADE

	
	
	

	12.1 Inspect tail rotor blades for condition.
	34-2
	

	
	
	

	A 6090.13 MAIN ROTOR CONTROLS

	
	
	

	13.1 Inspect all flight control components for condition
	41-3
	

	
	
	

	13.2 Check swash plate bearing for proper running.
	41-73
	

	
	
	

	13.3 Check rigging of collective control forces.
	102-16, step 9.
	

	NOTE: Hydraulic mule required.
	

	13.4 Clean swash plate sliding surface on support tube. Move swash plate to uppermost position to expose sliding surface. Use cleaning solvent (CM 201, 202 or 217)
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6090.14 TAIL ROTOR CONTROLS

	
	
	

	14.1 Visually inspect the seals on rod ends and clevis for damage on the following;
	

	
	

	14.1.1 Control rod in the tail boom
	42-3
	

	
	
	

	14.1.2 Control rod in vertical fin (upper clevis)
	
	

	
	
	

	14.2 Visual inspect sealing of blind hole in fork end for damage in control rod in vertical fin.
	
	

	
	
	

	A 6090.15 HYDRAULIC SYSTEM

	
	
	

	15.1 Inspect switchover control linkage for play.
	43-17 or 43-17A
	

	
	
	

	15.2 Inspect hydraulic system for condition.
	43-11
	

	
	
	

	15.3 Spray-coat N2-lever (droop-compensation) with corrosion preventive compound (CM 508).
	
	

	
	
	

	15.4 Check filter contamination indicator (lateral indicator pin configuration).
	43-14
	

	
	
	

	15.5 Functionally test hydraulic system
	43-15
	

	
	
	

	15.6 Perform ground run check of selector valve setting.
	43-16 or 43-16A
	

	
	
	

	15.7 Inspect system 1 selector valve for corrosion.
	3-13
	

	
	
	

	A 6090.16 LANDING GEAR

	
	
	

	16.1 Inspect landing gear for condition.
	51-2
	

	
	
	

	A 6090.17 ENGINE

	
	
	

	17.1 Remove anti-icing valve actuators and inspect mounting brackets for condition.
	61-37, 61-38,
61-39
	

	
	
	

	A 6090.18 FUEL SYSTEM

	
	
	

	18.1 Inspect fuel lines in the engine compartment for condition
	62-3
	

	
	
	

	18.2 Check fuel differential pressure switch for function.
	62-39
	

	
	
	

	18.3 Perform functional test and leakage test of fuel shutoff valves.
	92-82, 92-83
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6090.19 LUBRICATION SYSTEM

	
	
	

	19.1 Inspect lubrication system for condition
	63-3
	

	
	
	

	19.2 Remove oil drain plugs of oil tank and test the magnetic retaining force of their respective magnetic plugs.
	63-4, step 1.b,
02-14
	

	
	
	

	19.3 Visually inspect baffle plate, located between oil cooler and fan, and attaching clamps for cracks
	
	

	EFFECTIVITY:  Ram air ventilation not installed:
	
	

	A 6090.20 FIREWALLS

	
	
	

	20.1 Inspect fire walls for condition.
	64-2
	

	
	
	

	A 6090.21 ENGINE OPERATION AND CONTROL

	
	
	

	21.1 Inspect engine operation and control linkages for condition.
	65-3
	

	
	
	

	A 6090.22 STANDARD EQUIPMENT

	
	

	22.1 Inspect the following:
	

	
	

	22.1.1 Pilot and copilot seats for condition
	701-2
	

	
	
	

	22.1.2 Cabin equipment for condition
	702-2
	

	
	
	

	22.1.3 Cabin ventilation for condition, check for function
	704-2
	

	
	
	

	22.1.4 Identification and other markings for legibility, and adhesive-backed decals for damage and proper adhesion
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	A 6090.23 INSTRUMENT SYSTEM

	
	
	

	23.1 Ventilate dual torque indication system.
	91-57
	

	
	
	

	23.2 Inspect instruments for condition.
	91-4
	

	
	
	

	23.3 Clean and drain pitot-static system, inspect for condition and check for function
	91-9 thru 91-12
	

	
	
	

	23.4 Inspect magnetic compass for condition and function and compensate magnetic compass - Requires master compass
	91-24 thru 
91-26
	

	
	
	

	23.5 Calibrate TOT indication system - Barfield Required
	91-45
	

	
	
	

	23.6 Inspect instrument panel, center panel and overhead panel for  presence, legibility and security of labels and placards.
	
	

	NOTE: Replace missing placards and rebond separated placards
	
	

	A 6090.24 ELECTRICAL SYSTEMS

	
	
	

	24.1 Inspect battery bonding jumper for tight installation and unimpaired surface protection
	
	

	
	
	

	24.2 Check voltage regulator setting - Requires calibrated Volt Meter
	92-17
	

	
	
	

	24.3 Inspect socket of anti-collision light for condition.
	92-116
	

	
	
	

	24.4 Inspect battery--temperature warning.
	92--34E
	

	
	
	

	24.5 Remove chip detector, check, clean, test for function and test magnetic retaining force - Weighted ball bearings required.
	845-4 thru 6,
02-14
	

	
	
	

	A 6090.25 MAIN ROTOR BLADE FOLDING SYSTEM

	
	
	

	25.1 Remove locking lever assembly, clean and inspect for condition (crack inspection not required)
	854-3, step 1.
	

	
	
	

	25.2 Remove locking lever assembly.
	
	

	
	
	

	25.2.1 Clean and inspect nickel-plated bolts for condition, and provide with corrosion protection (crack inspection not required)
	854-3, step 1.a
854-4, step 2.f
	

	
	
	

	25.2.2 Clean and inspect solid film lubricant-coated bolts for condition (crack inspection not required). Coat bolt with lubricant (CM146}
	854-3, step 1.b
854-4, step 2.g
	

	
	
	


	MARITIME HELICOPTERS
	EUROCOPTER  BO-105 SERIES AAIP

	
	

	Page No:
	6

	Revision:
	1

	Issue Date:
	01/15/16

	SECTION:
	
	A 6090 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	6000 HOUR / 96 MONTH INSPECTION

	NOTE:
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 6090.26 CONTINUOUS IGNITION SYSTEM

	
	
	

	26.1 Check spark igniters for condition
	857-4
	

	
	
	

	26.2 Visually inspect noise suppressor and accessible parts of wiring for condition.
	857-4
	

	
	
	

	A 6090.27 POST INSPECTION

	
	
	

	27.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	27.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	27.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	27.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	27.5 Perform Functional Check Flight if required per Bell 206L Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	27.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 6090 – 6000 Hour / 96 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




