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	SECTION:
	
	A 3048 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	3000 HOUR / 48 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3048.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 3048.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 3048.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 3048.4 MAIN TRANSMISSION

	
	
	

	4.1 Remove transmission mounting struts and inspect for condition.
	11-50 thru 
	

	
	11-52
	

	A 3048.5 MAIN ROTOR SYSTEM

	
	
	

	5.1 Remove, disassemble and inspect driving link assembly for condition.
	13-20 thru 
	

	
	13-24
	

	A 3048.6 FUSELAGE

	
	
	

	6.1 Inspect spherical bearings and claw bushings in main transmission fittings for condition and play
	21-3
	

	
	
	

	6.2 Inspect bores in the engine mounting fittings for wear.
	21-3
	

	NOTE To be also performed with engine removal. 
	

	A 3048.7 TAIL ROTOR DRIVE

	
	32-11 thru
32-34
	

	7.1 Remove, disassemble and inspect forward short driveshaft, couplings, long driveshaft and aft short driveshaft in vertical fin for condition.
	
	

	EFFECTIVITY: Tail rotor drive with laminated disk coupling 

	

	7.2 Remove intermediate gearbox and tail rotor gearbox and inspect for condition
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3048.8 MAIN ROTOR CONTROLS

	
	

	8.1 Remove, disassemble and inspect the following control rods;
	

	
	

	8.1.1 Control rods between hydraulic unit and mixing lever assembly (3 off)
	41 -76 
thru 
41-83
	

	
	
	

	8.1.2 Rotating control rods (4 off)
	
	

	
	
	

	8.2 Remove compression springs of longitudinal and lateral trimmers, clean and inspect for condition. 
	41-27 
thru 
41-34
	

	
	
	

	8.3 Lubricate spring case
	
	

	
	
	

	8.4 Remove all bolts from the boosted section of the main rotor controls (i.e. above hydraulic unit) and inspect for condition and cracks. The following bolts are affected:
	

	NOTE: Crack inspection per dye penetrant method ASTM-E-1417 or magnetic particle method ASTM-E-1444. Perform inspections 8.4 and 8.5 on the occasion of the main transmission overhaul if possible.
	

	8.4.1 Lower and upper bolts of the 3 control rods between tandem hydraulic unit and mixing lever assembly
	
	

	
	
	

	8.4.2 lower and upper bolts of the 2 control rods between mixing lever assembly and swash plate
	
	

	
	
	

	8.4.3 Lower and upper bolts of the 4 rotating control rods
	41 -65 
thru 
41-70
	

	
	
	

	8.5 Remove, disassemble mixing lever assembly and inspect for condition
	
	

	
	
	

	8.6 Inspect swash plate for condition
	REM 403
	

	
	
	

	8.7 Remove control rods between mixing lever assembly and swash plate and inspect for condition
	41-78, 41-80
	

	
	
	

	A 3048.9 HYDRAULIC SYSTEM

	
	
	

	9.1 Remove, disassemble and inspect control rods for condition.
	43-36, 43-37
	

	
	41-79, 41-80
	

	A 3048.10 ENGINE

	
	
	

	10.1 Remove engine stub shaft and inspect for condition
	61-40
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 3048.11 POST INSPECTION

	
	
	

	11.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	11.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	11.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	11.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	11.5 Perform Functional Check Flight if required per BO-105 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	11.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	







Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 3048 – 3000 Hour / 48 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




