	MARITIME HELICOPTERS
	EUROCOPTER  BO-105 SERIES AAIP

	
	

	Page No:
	3

	Revision:
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	Issue Date:
	12/30/14

	SECTION:
	
	B 0354NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	300 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	NO TOLERANCE 

	
	
	



	1Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C20 Series Operation and MM Table 602, Eurocopter B0-105 Series MM Chapter 101, ASB 105 60 107
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0354.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce M250-C20 Operations and Maintenance Manual).
	250-C20 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce M250-C20 Operations and Maintenance Manual).
	250-C20 MP
	

	
	
	

	B 0354.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	
	
	

	CAUTION

INSPECTION FREQUENCY MUST BE BASED ON THE NATURE OF THE EROSIVE AND/OR CORROSIVE ENVIRONMENT. THE OPERATING ENVIRONMENT CAN DICTATE A MORE FREQUENT INSPECTION INTERVAL.WHEN OPERATING IN A CORROSIVE AND/OR EROSIVE ENVIRONMENT FOR NON--COATED COMPRESSOR WHEELS, THE INSPECTION MUST NOT EXCEED 300 HOURS OR 6 MONTHS. FOR COATED COMPRESSOR WHEELS, INSPECTION MUST NOT EXCEED 300 HOURS OR 12 MONTHS. IF ANY PARENT METAL IS EXPOSED DUE TO CORROSION AND/OR EROSION, THE INSPECTION REQUIREMENT MUST REVERT BACK TO 300 HOURS OR 6 MONTHS.
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0354.3 ENGINE

	CAUTION: BEFORE UNDERTAKING ANY INSPECTION OR MAINTENANCE ACTION, CONSULT THE REFERENCED PARAGRAPHS OF THE OPERATION AND MAINTENANCE MANUAL. FAILURE TO FOLLOW THE RECOMMENDED INSTRUCTIONS IN THE MANUAL COULD RESULT IN EQUIPMENT DAMAGE OR DESTRUCTION, POSSIBLY RESULTING IN PERSONNEL DEATH OR INJURY.
	

	3.1 Inspect the following:
	

	
	

	3.1.1 Entire engine for loose bolts, broken or loose connections, security of mounting accessories and broken or missing safeties.
	N/A
	

	
	
	

	3.1.2 Check accessible areas for obvious damage and evidence of fuel and oil leakage.
	
	

	
	
	

	3.1.3 Slippage marks on all fuel, oil and air tub B-nuts to make sure that all nuts have not loosened. If a slippage mark is missing, loosen “B” nut, retighten and apply torque paint.
	PARA 9.B
72-00-00
	

	
	Eng Servicing
	

	3.1.4 Engine cowling and doors for condition and security. Replace anti-chaff tape as needed.  
	
	

	
	
	

	3.1.5 Fluid flexible and rigid lines.
	
	

	
	
	

	3.1.6 Turbine support assemblies.
	PARA 8.A.,

72--50--00

BO 105 MM

61-34
	

	
	
	

	3.1.7 Exhaust stacks and ducts for condition of welded joints, cracks and buckling.  clamps for proper installation, condition, corrosion, cracks and torque.
	
	

	
	
	

	3.1.8 Exhaust clamps for cracks, particularly near latches.
	61-3
	

	
	ASB 105 60 107
	

	3.1.9 Visually check the compressor discharge air tubes for damage or deterioration.
	PARA 4.A., 
	

	
	72--40--00
	

	3.1.10 Discharge air tube inserts that are cocked or backing out of the scroll.
	PARA 1 D. (2),
	

	NOTE: If cocked or loose inserts are detected, check engine for possible vibration causes
	This Section.
	

	3.1.11 Compressor inlet guide vanes and visible blades and vanes for foreign object damage.
	
	

	
	
	

	3.1.12 Compressor mount inserts, bolts and nuts for looseness, fretting or oil leakage, replace or retighten as required. Check engine for possible vibration causes.
	PARA 4.D., 

72--60--00 and

PARA 1.D.(2),
	

	
	this section
	

	3.1.13 Compressor scroll for cracks or breaks at the anti--ice air valve and customer bleed port. If cracks or breaks are detected, check engine for possible vibration causes.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.1.14 Electrical harness and spark igniters.
	BO 1-5 MM
	

	
	857-4
	

	3.1.15 Remove all foreign material which might be drawn into the compressor inlet.
	
	

	
	
	

	3.1.16 Anti--ice valve for security, worn parts and proper operation.
	PARA 4.,
	

	NOTE: Valve need not be removed or disassembled unless a problem is detected.
	75--10--01
	

	3.1.17 Security of screws and rivets.
	
	

	
	
	

	3.1.18 Mounting and support bolts to be sure they are tight, lockwired and in good condition.
	
	

	
	
	

	3.1.19 Condition of the bleed valve gasket, without removing bleed valve. Replace gasket if air leaks (blowouts) can be detected.
	PARA 2., 

75--10--02
	

	
	
	

	3.1.20 Magnetic chip detector plugs.
	PARA 11.G.,

72--00--00, 
	

	
	Engine--Servicing
	

	3.1.21 Remove chip detector and test their magnetic retaining force.
	BO 105 MM

02-14
	

	NOTE: For removal and installation procedures, see Allison OMM 10W2 or 5W2 as applicable
	

	3.1.22 Inspect quick disconnect magnetic chip detector plugs and flanged inserts for wear, if installed.
	PARA 11.G.,

72--00--00, Engine--Servicing
	

	
	
	

	3.1.23 Ignition lead for burning, chafing, or cracking of conduit and loose connectors and broken lockwire.
	
	

	
	
	

	3.1.24 Accessible fuel system components, lines, and connections for security, damage or leakage with boost pumps ON - Remove, visually inspect and clean if visual condition dictates.
	PARA 2.

73-00-00
	

	
	
	

	3.1.25 Engine pan drains. Make sure that they are not clogged. Restore broken or missing sealant from engine pan.
	.
	

	
	
	

	3.1.26 Firewalls for condition and security.
	
	

	
	
	

	3.1.27 Inspect the thermocouple assembly.
	PARA 2.B., 
77--20--01
	

	
	
	

	3.1.28 Fuel control and power turbine governor linkage for freedom of operation, full travel and proper rigging.
	PARA 3.C.,

73--20--02,

3.B., 73--20--03,

3.C., 73--20--04

PARA 2.C. 

73--20--01
	

	
	
	

	3.1.29 Security of linkage for loose or worn linkage and linkage bolt.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0354.4 ENGINE AIR SYSTEM

	
	
	

	4.1 Inspect Pc filter for proper clamping.
	73--20--06
	

	
	
	

	4.2 Remove, clean and inspect engine Pc filter every 300 hours or earlier as engine performance dictates.
	PARA 3., 
73--20--06
	

	
	
	

	4.3 Remove the Scroll--to--Pc Filter Tube Assembly at both ends and inspect for cracks using 10x power glass. Pay particular attention to the flared ends of the tube for cracks, and to the areas beneath the floating ferrules for fretting damage. Tubes--found to contain cracks and/or excessive fretting damage are to be replaced by new parts of the same part number as removed
	
	

	NOTE: Excessive fretting is present when the ferrule has chafed the tube sufficiently to wear a step in the tube that can be felt with a thumbnail or other inspection aid.
	

	4.4 With the Scroll--to--Pc Tube Assembly still removed and using a 10x power glass, inspect the elbow in the compressor scroll for distress/cracks/proper alignment. No cracks are permissible.
	
	

	
	
	

	B 0354.5 ENGINE OIL SYSTEM

	
	
	

	5.1 Inspect and clean the No. 1 bearing oil pressure reducer..
	PARA 3., 

72--30--00
	

	5.2 Visually inspect external sump.
	PARA 7. E.,

72--50--00
	

	
	
	

	5.3 Clean internal carbonous deposits and build up from sump or replace if necessary.
	PARA 7. E.,

72--50--00
	

	
	
	

	5.4 Inspect scavenge oil strut in the power turbine support.
	PARA 7. E.,

72--50--00
	

	
	
	

	5.5 Clean carbonous deposits from strut.
	PARA 7. E.,

72--50--00
	

	
	
	

	5.6 Inspect No. 6 and 7 bearing pressure oil nozzle.
	PARA 7. E.,

72--50--00
	

	
	
	

	5.7 Clean carbonous deposits from nozzle.
	PARA 7. E.,

72--50--00
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	B 0354.6 POST INSPECTION

	
	
	

	6.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.2 Make sure applicable servicing requirements have been carried out.
	Chapter 101
	

	
	
	

	6.3 Clean compressor with chemical wash solution.
	PARA 6., 

72--30--00
	

	
	
	

	6.4 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	6.5 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	
	

	
	
	

	6.6 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	
	
	

	6.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Eurocopter BO-105 Series AAIP 300 Hour / 12 Month – B 0354NT – Engine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


