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	SECTION:
	
	B 1000NT – ENGINE INSPECTION PROGRAM

	TYPE:
	
	1000 HOUR INSPECTION

	NOTE:
	
	No  Tolerance



	 Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  Rolls-Royce M250-C20 Series Operation and MM Table 602, Eurocopter B0-105 Series MM Chapter 101
	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

INITIALS

	B 1000.1 GENERAL

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	1.3 Replace all life limited components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C20 MP
	

	1.4 Overhaul all components that have completed published operating limits (Refer to Rolls-Royce Operations and Maintenance Manual).
	250-C20 MP
	

	B 1000.2 ENGINE

	
	
	

	2.1 Inspect Py port on Bendix power turbine governor per M250 CEB--A--1281.
	
	

	NOTE:   The governor must be removed from the engine to perform this inspection.
NOTE:   If CEB--A--1289 or CEB 1330 have been accomplished, this inspection is not required.
	

	B 1000.3 POST INSPECTION

	3.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	3.2 Make sure applicable servicing requirements have been carried out.
	Chapter 101
	

	3.3 Check oil level of transmission, hydraulic tank, engines and rail rotor gearbox prior to running helicopter.
	
	

	3.4 Ground run aircraft for a minimum of 2 minutes to check for leaks and ensure all systems are operational and parameters are within Flight Manual limitations.
	
	

	3.5 Perform Functional Check Flight if required per Rolls-Royce MM, or RFM as appropriate.
	
	

	3.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters Eurocopter BO-105 Series AAIP 1000 Hour – B 1000NT – Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Ending Total Time:
	

	Engine S/N: 
	
	
	
	Engine Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


