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	SECTION:
	
	C 9971 – ICA OF INSTALLED EQUIPMENT

	TYPE:
	
	50 HOURS INSPECTION – NICAD BATTERY – IN AIRCRAFT 

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  Marathon Power Technologies Battery Products Instruction Manual No. BA-24-32-00 or The SAFT Operating and Maintenance Manual No. 24-30-99.
	
	
	

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

	
	
	INITIALS

	C 9971.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	 
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	 
	

	
	
	

	C 9971.2 NOTE

	
	
	

	2.1 Due to the various operating conditions at each base location, it is the responsibility of the base mechanic to set the proper maintenance intervals for their aircraft NiCad battery usage.  The maintenance interval will be the determination which Inspection Form is used.  The chosen maintenance interval will be entered on the status reports for each individual aircraft.  If for any reason these intervals need to be changed, the proper form will need to be submitted along with a logbook entry stating the change of interval.  Floater aircraft will have the most restrictive intervals assigned.
	
	

	
	
	

	C 9971.3 VISUAL INSPECTION

	
	
	

	3.1 Visual inspection of Marathon Battery in the Aircraft. 
	BA-24-32-00 Para. 1-2
	

	
	
	

	3.2 Visual inspection of SAFT Battery in the Aircraft.
	24-30-99
Visual inspection
	

	
	
	

	C 9971.4 NiCAD BATTERY INSPECTION – VOLTAGE REGULATOR INSPECTION

	
	
	

	4.1 Functional check of Voltage Regulator with Marathon Battery.
	BA-24-32-00 Para. 1.2.5
	

	
	
	

	C 9971.5 POST INSPECTION

	
	
	

	5.1 Inspect for operation and leaks.
	
	

	
	
	

	5.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.3 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Air Methods’ AS 350 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Air Methods’ AS 350 Series AAIP ICA – 50 Hours NiCad Battery In Aircraft Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


