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Reference:  DHC-6 Maintenance Program
	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0500.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6-400
MP
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6-400

MP
	
	

	
	
	
	

	B 0500.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	B 0500.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection
	Appendix

C
	
	

	B 0500.4  PREPARATION

	
	
	
	

	4.1 Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	B 0500.5 21 – AIR CONDITIONING 

	
	
	
	

	5.1 Cabin exhaust outlet or, if pneumatic package is installed, heat exchange for condition and clear of obstructions.
	
	
	

	
	
	
	

	5.2 Cabin exhaust outlet vent for condition and obstruction.
	
	
	

	
	
	
	

	5.3 STA 111 Cabin fans for condition and security, standoff mounting brackets for security.
	
	
	

	Effectivity: SOO 6378
	
	
	

	5.4 STA 332 Blower for condition and security, standoff mounting brackets for security.
	
	
	

	Effectivity: SOO 6379
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	B 0500.6 22 – AUTO FLIGHT 

	
	
	
	

	6.1 Autopilot (all models) for condition and security of mounting, altitude hold or controller for condition, static line for condition and security, attitude heading selector and turn and slip sensor (if installed) for condition and security. Clean as required.
	
	
	

	
	
	
	

	6.2 Autopilot (all models) aileron servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security.  Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	
	
	
	

	6.3 Autopilot rudder (all models) servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security.  Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	
	
	
	

	6.4 Rudder (all models) autopilot servo for condition and security of mounting.
	
	
	

	6.5 Autopilot elevator (all models) servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security.  Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	6.6 Elevator (all models) autopilot servo for condition and security of mounting.
	
	
	

	6.7 VOR dual selector relay for condition and security.
	
	
	

	
	
	
	

	6.8 Automatic pitch trim (all models) system cables for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drive for condition, security and freedom of operation. Clamps for security and no evidence of movement on elevator flight control cable clamp.
	
	
	

	6.9 Autopilot (all models) electrical wiring for condition and connectors for security, bonding wires for condition and security. Clean as required.
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	6.10 AFCS (autopilot) system, inspect as follows;

Effectivity: Mod 6/2302, SOO 6221
	

	6.10.1 Pilot and co-pilot Go Around (G/A) and Touch Control Switches for security and clean as required. Function test.
	
	
	

	
	
	
	

	6.10.2 Pilot and Co-Pilot; AP Disconnect (AP DISC) Switch for security and clean as required
	
	
	

	
	
	
	

	6.10.3 Function Test
	
	
	

	
	
	
	

	6.10.4 Autopilot aileron servo for condition and security.
	
	
	

	
	
	
	

	6.10.5 Autopilot pitch trim servo actuator for condition and security. Clean as required.
	
	
	

	
	
	
	

	6.10.6 Autopilot pitch trim servo system pitch trim switch. Inspect for condition and security. Clean as required.
	
	
	

	
	
	
	

	B 0500.7 23 – COMMUNICATIONS 

	
	
	
	

	7.1 Audio system control units and power panels for condition and security of mounting.  Flight compartment speakers and speaker panel assembly for condition and security.
	
	
	

	
	
	
	

	7.2 VHF upper aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	Effectivity: Mod 6/2003
	
	
	

	7.3 VHF forward antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	Effectivity: Mod 6/2003
	
	
	

	7.4 VHF lower aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	Effectivity: Mod 6/2003, SOO 6231
	
	
	

	7.5 VHF-FM antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6296
	
	
	

	7.6 VHF and VHF standby antennas for loose connections, fiberglass cover for cracks and deterioration, wire whip for bending or misalignment.
	
	
	

	Effectivity: Pre Mod 6/2003
	
	
	

	7.7 HF mast for cracks and security, wire for proper tension and loose connections, cable covering for cracks and deterioration. Lead-in sleeves for cracks and security.  Insulators for condition, connections for security. Clean as required.
	
	
	

	
	
	
	

	7.8 HF antenna tension unit at vertical stabilizer tip for cracks, corrosion and security.
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	7.9 Power distribution and generator control box for condition and security; terminals, connectors and relays for condition and security, signs of overheat, arcing, torque of large terminal posts. Clean as required. Current Limiters (Mod 6/1651) for condition and serviceability.
	
	
	

	
	
	
	

	7.10 HF antenna tension unit at vertical stabilizer tip for cracks, corrosion and security
	
	
	

	
	
	
	

	7.11 Static discharge wicks for condition and security, minimum length of one-inch wick extension from sheath.
	
	
	

	
	
	
	

	7.12 GPS/IRIDIUM/WiFi antenna for condition, security and corrosion, condition of external fillet seal, condition of coaxial cables and connectors and security of attachment of coaxial cables.
	
	
	

	
	
	
	

	7.13 Diodes CR 141 thru CR 146 – check diodes.  Replace if required.
	
	
	

	
	
	
	

	7.14 Static inverters for condition and security, mounting installation for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2028

Note: Refer to Service Bulletin No. 6/263 and A.D. 71-21-07 and 75-34-15
	
	
	

	7.15 All aircraft accessible wiring and connectors for condition and security.
	
	
	

	
	
	
	

	7.16 Check condition and security of cables at STA 111 cabin floor cut-out. Refer to PSM 1-64-2 Chp 24-30-00.
	
	
	

	Effectivity: SOO 6371
	
	
	

	B 0500.8 25 - EQUIPMENT/FURNISHINGS 

	
	

	8.1 Inspect pilots and co-pilots seats as follows;
	

	
	

	8.1.1 Seat structure and seat pan for condition and security, freedom of movement.
	
	
	

	
	
	
	

	8.1.2 Seat rails for condition and security of stops.
	
	
	

	
	
	
	

	8.1.3 Chock cords for condition and security.
	
	
	

	
	
	
	

	8.1.4 Safety harness for condition and security, quick release for proper operation. Clean as required.
	
	
	

	
	
	
	

	8.1.5 Inertia reel for condition and security, proper operation.
	
	
	

	
	
	
	

	8.1.6 Portable ELT mounting provision for security, condition, proper operation and retention. Install safety wire as required.
	
	
	

	Effectivity: SOO 6270
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	8.2 Cabin side rail and floor for condition and security.
	
	
	

	Note: Refer to Service Bulletin No. 6/302 and A.D. 74-08-11
	
	
	

	8.3 Baggage restraints (if installed) for condition and security. Slimeline commissary (if installed) for condition and obstruction.
	
	
	

	Effectivity: SOO 6175
	
	
	

	B 0500.9 27 – FLIGHT CONTROLS 

	
	
	
	

	9.1 Trim cables for condition, graying, corrosion, flattening, proper attachment and security.
	
	
	

	
	
	
	

	9.2 Control column boot for condition and security.
	
	
	

	
	
	
	

	9.3 Nylon cable jacket for condition, cracking and necking down in diameter.
	
	
	

	
	
	
	

	9.4 Pulleys (bulkhead and elevator torque tube) for condition and freedom of movement, pulley brackets for condition and security.
	
	
	

	
	
	
	

	9.5 Lubricate pulley bracket bushings at elevator torque tube.
	
	
	

	
	
	
	

	9.6 Rudder and elevator trim screw jacks for condition of cable drum grooves, freedom of operation and security.  Lubricate.
	
	
	

	
	
	
	

	9.7 Flap selector valve and follow-up cables for condition, corrosion, fraying, flattening and security of attachment, turnbuckles for security, pulleys for condition and freedom of operation.
	
	
	

	
	
	
	

	9.8 Do a detailed visual inspection of cable terminals as follows;
	
	

	
	
	

	9.8.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	9.8.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	9.8.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	9.8.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	9.8.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 9.7.1, rig the control system.
	
	
	

	
	
	
	

	9.8.6 If the lockwire was removed, secure the cable terminals with lockwire.
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	9.9 Flap/elevator interconnect ball screw jack for condition of cable drum grooves, freedom of operation and security.  Lubricate
	
	
	

	
	
	
	

	9.10 Elevator flap interconnect screw jack for condition of cable drum grooves, freedom of operation and security.  Lubricate.
	
	
	

	
	
	
	

	9.11 Aft fuselage elevator quadrant for condition, distortion, loose toque tube bolts, freedom of movement and mounting brackets for condition, cracks and security.
	
	
	

	Note: Refer to Service Bulletins S.B. 6/379 & 6/511 and A.D.’s 79-14-01 & 89-24-06 if applicable.
WARNING: Inspect within 25 flight hours if parked aircraft subjected to ground winds with a mean velocity of 35 MPH or greater. Mean wind speeds of 35 MPH will generate wind gusts up to 65 MPH.
	
	
	

	
	
	
	

	9.12 Stall warning light for condition and security.
	
	
	

	
	
	
	

	9.13 Stall warning horn for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	B 0500.10  28 – FUEL 

	
	
	
	

	10.1 L/H Wing fuel emergency shutoff valve for leakage and security.
	
	
	

	
	
	
	

	10.2 R/R Wing fuel emergency shutoff valve for leakage and security.
	
	
	

	
	
	
	

	10.3 Remove and inspect motive line check valve strainer for contamination. Clean as required and install serviceable unit. Leak check.
	
	
	

	Note: Drain fuel before removing strainers.
	
	
	

	10.4 L/H Wing fuel vent outlet for condition and free from obstruction.
	
	
	

	Note: Refer to Service bulletin No. 6/211, if applicable
	
	
	

	10.5 R/H Wing fuel vent outlet for condition and free from obstruction.
	
	
	

	Note: Refer to Service bulletin No. 6/211, if applicable
	
	
	

	B 0500.11  29 – HYDRAULIC POWER 

	
	
	
	

	11.1 Accumulator air charging valves for condition and security. Clean as required.
	
	
	

	
	
	
	

	11.2 Hydraulic pump (electric motor driven) for security and leakage.
	
	
	

	
	
	
	

	11.3 Hydraulic pressure switch security and leakage.
	
	
	

	
	
	
	

	11.4 Drain holes in hydraulic power package tray clear of obstruction. Clean as required.
	
	
	

	
	
	
	

	11.5 Emergency hydraulic hand pump for security and leakage.
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	11.6 Hydraulic pipes and connections for condition, connections for security.
	
	
	

	
	
	
	

	11.7 Remove hydraulic filter element and replace with new element. Leak check.
	
	
	

	
	
	
	

	B 0500.12  30 – ICE AND RAIN PROTECTION 

	
	
	
	

	12.1 Horizontal stabilizer deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	
	
	
	

	12.2 L/H Wing deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	
	
	
	

	12.3 R/H Wing deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	
	
	
	

	12.4 Horizontal stabilizer deicing system water separator drain holes and lines for obstruction and security. Water separator filter for condition and replace as necessary.
	
	
	

	
	
	
	

	12.5 L/H Wing deicing system water separator drain holes and lines for obstruction and security. Airframe deicing water separator filter for condition and replace as necessary.
	
	
	

	
	
	
	

	12.6 R/H Wing deicing system water separator drain holes and lines for obstruction and security. Airframe deicing water separator filter for condition and replace as necessary.
	
	
	

	
	
	
	

	12.7 Windshield wiper blades for condition and security, drive arms for tension, tie rods for wear, distortion and security.
	
	
	

	
	
	
	

	12.8 Windshield washer pump and fluid lines for condition, deterioration
	
	
	

	Note: Refer to Service bulletin No. 6/422 and A.D. 82-26-06, if applicable.
	
	
	

	12.9 Windshield washer system reservoir for leakage, fluid lines for deterioration, cracks and security, vent for obstruction.
	
	
	

	Note: Refer to Service bulletin No. 6/422 and A.D. 82-26-06, if applicable.
	
	
	

	12.10 L/H Engine air intake anti-icing boot for deterioration, proper adhesion and evidence of burning, wiring for condition, condition for security.
	
	
	

	Effectivity: Mod SOO 6062
	
	
	

	12.11 R/H Engine air intake anti-icing boot for deterioration, proper adhesion and evidence of burning, wiring for condition, condition for security.
	
	
	

	Effectivity: Mod SOO 6062
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	B 0500.13 32 – LANDING GEAR  

	
	

	13.1 Nose Gear
	

	
	

	13.1.1 Thoroughly clean nose gear shock strut and inspect for condition, security and leakage, service as necessary.
	
	
	

	
	
	
	

	13.1.2 Remove steering actuator external filter, clean and reinstall.
	
	
	

	
	
	
	

	13.1.3 Lubricate nose gear torque arms.
	
	
	

	Effectivity: Mod 6/1377
	
	
	

	13.1.4 Nose leg taxi light for condition and security, electrical connection for security.
	
	
	

	
	
	
	

	13.2 Wheel brake pedal linkage, springs, levers and linkage for condition, wear and security.
	
	
	

	
	
	
	

	B 0500.14 33 - LIGHTS 

	
	
	
	

	14.1 Taxi light for condition and security, electrical connection for security.
	
	
	

	
	
	
	

	B 0500.15 34 - NAVIGATION 

	
	
	
	

	15.1 Pitot heads for security and corrosion.
	
	
	

	
	
	
	

	15.2 Drain the pitot static moister traps at the following locations:
	
	

	
	
	

	15.2.1 Adjacent to pitot masts.
	
	
	

	
	
	
	

	15.2.2 Below static valve on center pylon
	
	
	

	
	
	
	

	15.2.3 Autopilot computer static line.
	
	
	

	
	
	
	

	15.3 Pitot head heat electrical wiring for condition and connections for security.
	
	
	

	
	
	
	

	15.4 Lower transponder antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6381 and Mod 6/2003
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	15.5 Lower transponder antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6381 and Mod 6/2003
	
	
	

	15.6 Upper transponder antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6381 & 6/2003
	
	
	

	15.7 Upper transponder antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6381 & 6/2003
	
	
	

	15.8 GPS antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.9 GPS antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.10 DME center fuselage antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.11 DME antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.12 Radar altimeter antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.13 Radar altimeter antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.14 TCAS upper antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6382, 6/2003
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	15.15 TCAS upper antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6219, 6/2003
	
	
	

	15.16 TCAS lower antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6382, 6/2003
	
	
	

	15.17 ADF antenna #1 covers for condition, moisture ingress, cracks deterioration and security, connectors and insulators for security, masts for cracks and security.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6209, 6/2003
	
	
	

	15.18 ADF antenna #2 covers for condition, moisture ingress, cracks deterioration and security, connectors and insulators for security, masts for cracks and security.  Clean as required.
	
	
	

	Effectivity: Mod SOO 6209, 6/2003
	
	
	

	B 0500.16 36 - PNEUMATIC 

	
	
	
	

	16.1 Cabin exhaust outlet or, if pneumatic package is installed, heat exchange for condition and clear of obstruction.
	
	
	

	
	
	
	

	16.2 Remove pneumatic system strainer element, clean and install. Leak check.
	
	
	

	
	
	
	

	16.3 Remove bleed air strainers, clean and install. Leak check.
	
	
	

	Effectivity: Mod SOO 6/1046
	
	
	

	B 0500.17 44 – CABIN SYSTEMS 

	
	
	
	

	17.1 Condition and security of mounting, cabin speakers for condition and security.
	
	
	

	Effectivity: Mod SOO 6/2049
	
	
	

	B 0500.18 52 – DOORS

	
	
	
	

	18.1 Flight compartment door hinges and locks for condition and security, freedom of operation and proper locking. Lubricate and clean as required.
	
	
	

	
	
	
	

	18.2 Inspect the cabin doors as follows:
	
	
	

	
	
	
	

	18.2.1 Hinges and lock for condition, security, freedom of operation and proper locking
	
	
	

	
	
	
	

	18.2.2 Close cabin LH rear cargo door and position both lower and upper latches in the locked condition. Make sure each latch pin makes positive engagement with door frame and holes.
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	18.2.3 Make sure the lower latch pin remains positively engaged when the locked latch is lifted to the top of its vertical play.
	
	
	

	
	
	
	

	18.2.4 Clean as required.
	
	
	

	
	
	
	

	18.3 Inspect the airstair door as follows:
	
	

	18.3.1 Hinge and lock for condition, security, corrosion, freedom of operation and proper locking, witness marks for correct alignment. Lubricate.
	
	
	

	
	
	
	

	18.3.2 Inward opening cargo door for condition and security, hinges for condition and freedom of operation.  Lubricate.
	
	
	

	
	
	
	

	18.3.3 Retention straps for condition.
	
	
	

	
	
	
	

	18.3.4 Clean as required.
	
	
	

	
	
	
	

	18.3.5 Door guard assembly for condition, check spring engagement against inner handle, ensure the guard assembly is in contact with the handle. Replace damaged springs as required.
	
	
	

	Effectivity: Mod 6/2326 & 6/2386
	
	
	

	18.4 Inspect rear baggage compartment door as follows;
	
	

	
	
	

	18.4.1 Hinge for condition, freedom of operation.
	
	
	

	
	
	
	

	18.4.2 Stay bar for condition of fastener and security in stowed position.
	
	
	

	
	
	
	

	18.4.3 Door handle and lock for condition and proper operation.
	
	
	

	
	
	
	

	18.4.4 Lubricate.
	
	
	

	
	
	
	

	18.5 Inspect nose compartment door as follows 
	
	

	
	
	

	18.5.1 Hinges for condition and freedom of operation. 
	
	
	

	
	
	
	

	18.5.2 Stay bar for condition of fastener and security in stowed position.
	
	
	

	
	
	
	

	18.5.3 Latches for proper operation.
	
	
	

	
	
	
	

	18.5.4 Lubricate.
	
	
	

	
	
	
	

	18.6 Cabin roof hatch for condition and security.
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	B 0500.19 54 – NACELLE - LH

	
	
	
	

	19.1 Inspect lower longeron for condition, buckling, cracking, corrosion and fasteners for security at the following locations; 
	
	
	

	CAUTION: INSPECTION APPLIES TO ALL AIRCRAFT CONFIGURATIONS

AND MUST BE CARRIED OUT PRIOR TO NEXT FLIGHT, IF AIRCRAFT HAS ENCOUNTERED HARD LANDING CONDITION.
	
	
	

	19.1.1 Forward engine mount fittings.
	
	
	

	
	
	
	

	19.1.2 Forward and at intersection with the wing.
	
	
	

	
	
	
	

	B 0500.20 54 – NACELLE - RH

	
	
	
	

	20.1 Inspect lower longeron for condition, buckling, cracking, corrosion and fasteners for security at the following locations; 
	
	
	

	CAUTION: INSPECTION APPLIES TO ALL AIRCRAFT CONFIGURATIONS

AND MUST BE CARRIED OUT PRIOR TO NEXT FLIGHT, IF AIRCRAFT HAS ENCOUNTERED HARD LANDING CONDITION.
	
	
	

	20.1.1 Forward engine mount fittings.
	
	
	

	
	
	
	

	20.1.2 Forward and at intersection with the wing.
	
	
	

	
	
	
	

	B 0500.21 57 – WING – LH 

	
	
	
	

	21.1 Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	
	
	
	

	21.2 Wing leading edge and shroud skins for condition, dents, scores, fasteners for security
	
	
	

	Note: Refer to Service Bulletin Nos. 6/517 if applicable.
	
	
	

	21.3 Electrical wiring and where visible, for condition, connectors for security.
	
	
	

	
	
	
	

	B 0500.22 57 – WING – RH 

	
	
	
	

	22.1 Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	
	
	
	

	22.2 Wing leading edge and shroud skins for condition, dents, scores, fasteners for security
	
	
	

	Note: Refer to Service Bulletin Nos. 6/517 if applicable.
	
	
	

	22.3 Electrical wiring and where visible, for condition, connectors for security.
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	B 0500.23 61 – PROPELLERS – LH 

	
	
	
	

	23.1 Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	
	
	
	

	23.2 Beta range backup system limit switch and mechanism for condition and security, wiring for condition and connectors for security.  Clean as required.
	
	
	

	
	
	
	

	23.3 Propeller spinner for dents and security, hub for grease or oil leakage and attach bolts for condition and security.
	
	
	

	Note: Refer to A.D. 68-18-01 and 83-08-01, if applicable.
	
	
	

	23.4 Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	
	
	
	

	23.5 Inspect propeller synchronizer system as follows;
	

	
	

	23.5.1 Speed setting actuator.
	
	
	

	
	
	
	

	23.5.2 Rod end trimmer.
	
	
	

	
	
	
	

	23.5.3 Flexible shaft.
	
	
	

	
	
	
	

	23.5.4 Electrical wiring for condition and connectors for security.
	
	
	

	
	
	
	

	B 0500.24 61 – PROPELLERS – RH 

	
	
	
	

	24.1 Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	
	
	
	

	24.2 Beta range backup system limit switch and mechanism for condition and security, wiring for condition and connectors for security.  Clean as required.
	
	
	

	
	
	
	

	24.3 Propeller spinner for dents and security, hub for grease or oil leakage and attach bolts for condition and security.
	
	
	

	Note: Refer to A.D. 68-18-01 and 83-08-01, if applicable.
	
	
	

	24.4 Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	
	
	
	

	24.5 Inspect propeller synchronizer system as follows;
	

	
	

	24.5.1 Speed setting actuator.
	
	
	

	
	
	
	

	24.5.2 Rod end trimmer.
	
	
	

	
	
	
	

	24.5.3 Flexible shaft.
	
	
	

	
	
	
	

	24.5.4 Electrical wiring for condition and connectors for security.
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	B 0500.25 71 – POWERPLANT - LH

	
	

	25.1 Inspect intake deflector system as follows;
	

	
	

	25.1.1 Exit door for condition and security.
	
	
	

	
	
	
	

	25.1.2 Actuators for condition security and leakage.
	
	
	

	
	
	
	

	25.1.3 Locking and release levers for condition, security and leakage, pipes for condition and leakage.
	
	
	

	
	
	
	

	25.1.4 Air control valves for condition, security and leakage, pipes for condition and leakage.
	
	
	

	
	
	
	

	25.1.5 Cables for fraying, kinks and wear, connectors for security, rod ends and bearings for condition and security, linkage for condition. Brackets for condition.
	
	
	

	
	
	
	

	25.2 Perform a detailed visual inspection of cable terminals as follows;
	
	

	Note: If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with a new cable assembly.
	
	

	25.2.1 Remove and discard the lockwire from cable terminals. If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed, rig the control system.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip. If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	25.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	25.2.3 Cable terminals for signs of cracks in all expose parts of the terminals.
	
	
	

	
	
	
	

	B 0500.26 71 – POWERPLANT - RH

	
	

	26.1 Inspect intake deflector system as follows;
	

	
	

	26.1.1 Exit door for condition and security.
	
	
	

	
	
	
	

	26.1.2 Actuators for condition security and leakage.
	
	
	

	
	
	
	

	26.1.3 Locking and release levers for condition, security and leakage, pipes for condition and leakage.
	
	
	

	
	
	
	

	26.1.4 Air control valves for condition, security and leakage, pipes for condition and leakage.
	
	
	

	
	
	
	

	26.1.5 Cables for fraying, kinks and wear, connectors for security, rod ends and bearings for condition and security, linkage for condition. Brackets for condition.
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	26.2 Perform a detailed visual inspection of cable terminals as follows;
	

	Note: If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with a new cable assembly.
	

	26.2.1 Remove and discard the lockwire from cable terminals. If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed, rig the control system.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip. If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	26.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	26.2.3 Cable terminals for signs of cracks in all expose parts of the terminals.
	
	
	

	
	
	
	

	B 0500.27 73 – ENGINE FUEL AND CONTROL – LH 

	
	
	
	

	27.1 Remove fuel pump outlet filter.
	
	
	

	Note: Refer to PWC Service Bulletin No. 1155.
	
	
	

	27.2 Install new filter and leak check.
	
	
	

	
	
	
	

	27.3 Remove and discard HP fuel filter element between fuel pump and fuel control unit.
	
	
	

	Note: If excessive contamination is found on filter elements, remove and inspect the main fuel strainer elements.
	
	
	

	27.4 Install new element and leak check.
	
	
	

	
	
	
	

	B 0500.28 73 – ENGINE FUEL AND CONTROL – RH 

	
	
	
	

	28.1 Remove fuel pump outlet filter.
	
	
	

	Note: Refer to PWC Service Bulletin No. 1155.
	
	
	

	28.2 Install new filter and leak check.
	
	
	

	
	
	
	

	28.3 Remove and discard HP fuel filter element between fuel pump and fuel control unit.
	
	
	

	Note: If excessive contamination is found on filter elements, remove and inspect the main fuel strainer elements.
	
	
	

	28.4 Install new element and leak check.
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	B 0500.29 76 – ENGINE CONTROLS 

	CAUTION

With engine stopped 1) DO NOT move power lever in either direction if blades latches are engaged.  2) DO NOT select reverse power if power if propeller is at feather.
	

	29.1 Power control mechanisms and linkages, including beta backup for condition, chafing, fouling and security.
	
	
	

	
	
	
	

	29.2 Inspect overhead console power controls follows;
	
	
	

	Note: Refer to Service Bulletin n. 6/309, if applicable.
	
	
	

	29.2.1 Mechanism and linkages for condition and freedom of movement.
	
	
	

	
	
	
	

	29.2.2 Power and propeller levers for smooth operation and propeller/power lever interlock mechanism for operation.
	
	
	

	
	
	
	

	29.2.3 Fuel shutoff control lever for smooth operation and proper detent action.
	
	
	

	
	
	
	

	29.2.4 Friction damper for operation, power lever Beta arming switch condition.
	
	
	

	
	
	
	

	B 0500.30 77 – ENGINE INDICATING - LH

	
	
	
	

	30.1 Engine indicating instrument wiring for condition, connectors for security. Clean as required.
	
	
	

	
	
	
	

	B 0500.31 79 – ENGINE INDICATING - RH

	
	
	
	

	31.1 Engine indicating instrument wiring for condition, connectors for security. Clean as required.
	
	
	

	
	
	
	

	B 0500.32 79 – OIL - LH

	
	
	
	

	32.1 Oil temperature bulb for leakage and security, Connection for security.
	
	
	

	
	
	
	

	B 0500.33 79 – OIL - RH

	
	
	
	

	33.1 Oil temperature bulb for leakage and security, Connection for security.
	
	
	

	
	
	
	

	B 0500.34 80 – STARTING – LH 

	
	
	
	

	34.1 Starter generator brushes for condition and wear.
	
	
	

	
	
	
	

	34.2 Drive splines for wear. Lubricate
	
	
	

	
	
	
	

	34.3 Spark igniters (Mod SOO 6180) for condition and security. Check for operation.
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	34.4 Spark ignitor box for condition and security.
	
	
	

	
	
	
	

	34.5 Starter generator electrical wiring for condition, insulation for deterioration and connectors for security. Clean as required.
	
	
	

	
	
	
	

	B 0500.35 80 – STARTING – LH 

	
	
	
	

	35.1 Starter generator brushes for condition and wear.
	
	
	

	
	
	
	

	35.2 Drive splines for wear. Lubricate
	
	
	

	
	
	
	

	35.3 Spark igniters (Mod SOO 6180) for condition and security. Check for operation.
	
	
	

	
	
	
	

	35.4 Spark ignitor box for condition and security.
	
	
	

	
	
	
	

	35.5 Starter generator electrical wiring for condition, insulation for deterioration and connectors for security. Clean as required.
	
	
	

	
	
	
	

	B 0500.36 OPERATIONAL CHECKS

	
	

	36.1 Perform the following Operational Checks;
	

	NOTE

Electrical power for the following tests is obtained by

connecting a ground power source or by running the

engines, whichever is more convenient
	

	36.1.1 Oil pressure indicator, oil temperature indicator (Pre Mod 6/2012)
	
	
	

	36.1.2 Autopilot system
	
	
	

	36.1.3 Doors unlocked warning lights, including limit switch operation
	
	
	

	
	
	
	

	36.1.4 Fuel leak check after installation of motive line check valve strainers
	
	
	

	
	
	
	

	36.1.5 Run engine(s) and check the following;
	

	
	

	36.1.5.1 Autofeather system
	
	
	

	
	
	
	

	36.1.5.2 Beta backup system
	
	
	

	
	
	
	

	36.1.5.3 Propeller/power interlock
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	36.1.5.4 Propeller synchronization
	
	
	

	
	
	
	

	36.1.5.5 H14 Autopilot pneumatic system filters (after removing and installing new element).
	
	
	

	
	
	
	

	36.1.6 Emergency cabin lights (Mod SOO 6098, 6179 and 6208).
	
	
	

	36.1.7 Windshield wipers
	
	
	

	CAUTION: DO NOT OPERATE WIPERS ON DRY WINDSHIELD SURFACE
	
	
	

	36.1.8 The following items, as applicable, for leaks after installation.
	

	
	

	36.1.8.1 Hydraulic filter unit
	
	
	

	
	
	
	

	36.1.8.2 Instrument pneumatic system (bleed air) strainers
	
	
	

	
	
	
	

	36.1.8.3 Pneumatic package strainer
	
	
	

	
	
	
	

	36.1.8.4 Steering actuator filter
	
	
	

	
	
	
	

	36.1.8.5 HP fuel filter element replacement
	
	
	

	
	
	
	

	36.1.9 Heated windscreen
	
	
	

	
	
	
	

	36.1.10 Aileron trim tab position indicator (Pre Mod 6/2047).
	
	
	

	
	
	
	

	36.1.11 Position indication (Mod 6/2047), do a display indication function test, neutral and full range of travel.
	
	
	

	36.1.12 Alignment of mechanical rudder trim pointer and EFIS rudder trim display (Mod 6/2047).
	
	
	

	
	
	
	

	36.1.13 Alignment of mechanical pitch trim pointer and EFIS pitch trim display (Mod 6/2047).
	
	
	

	
	
	
	

	36.1.14 AFCS (Autopilot) (Mod SOO 6221) - KS 272A Pitch trim servo system.
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	B 0500.37 POST INSPECTION

	
	
	
	

	37.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	37.2 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	37.3 Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	37.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – B 0500 – 500 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



