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Non-Essential Furnishing (NEF) Deferral Program
Authorized personnel shall comply with the following procedures for the deferral on Non-Essential Furnishings (NEF).
1. Record the discrepancy in the aircraft discrepancy record.

2. Determine whether the item is an MEL item. If it is, defer it according to MEL procedures.

3. If the item is not listed in the MEL, determine if it is included in the following NEF list:

General Items
a) Carper worn, torn, scratch or soiled

b) Trim pieces on ceiling, walls, floors, seats, are worn, torn, scratched, delaminated or soiled.

c) Materials on ceiling, floors, seats, worn, torn, scratched, delaminated or soiled.

Cockpit

a) Window Shades

b) Cup Holders 

c) Velcro straps for goggles and chart boxes

d) Foot Rests

e) Overhead lights including both lap and dome lights

Cabin

a) Speaker Select

b) Cabin Temp

c) Single Seat Control Panel to include:

i) Reading Light

ii) Entertainment Source/Volume Selector

iii) Headset Selector

d) Passenger Headphones

e) Cup Holders

f) Ash Tray Dispenser

4. If the item is included in this list, defer if according to the NEF program.

5. If the item is not included in this list, determine if the inoperative item will not have an adverse affect on the safe conduct of the flight.  If there is an obvious safety-of-flight issue, the inoperative item must be repaired prior to flight.
6. If possible diagnose the source of the discrepancy to determine whether the underlying cause affects the safety of flight. This step may or may not apply to the item under consideration.

7. Once the source is identified, determine if the source affects equivalent levels of safety.

a) If the source of the discrepancy affects equivalent levels of safety, determine if isolation of the source of the discrepancy alleviates the safety concern.

NOTE: In making this determination, very close coordination between the flight crew, maintenance and operations personnel may be required.

b) If, after review, the source is determined to create a safety-of-flight issue, the item must be repaired prior to flight.

8. If applicable, the source of the discrepancy must be isolated from all other systems with applicable maintenance procedures so as to alleviate the safety-of-flight concern. If the source cannot be sufficiently isolated, then the item must be repaired prior to flight. If isolated, the isolation of the source must pass the above NEF criteria.
9. If these conditions are satisfied, the item may be deferred according to the NEF program.

Non-Essential Furnishing (NEF) Deferral Program (Continued)
10. The item must be evaluated to determine:
a) If the item is required for operational rules in which the aircraft is operated.

b) If it creates the potential for fire/smoke, or other hazardous conditions.

c) Could it have an adverse effect on other required systems or components?

d) Doe its condition potentially affect the safety of passengers, crew or other service personnel?
e) Could it have a negative impact on emergency or abnormal procedures?

f) Does it create additional workload for the crew at critical times of fight or in flight preparation, and

g) Will any of these conditions become an issue for future flights?

NOTE: This evaluation process must be accomplished for the inoperative, damaged or missing items at its face value and also for the underlying cause of the discrepancy.

11. If an NEF list is being maintained, add the item to the list to preclude the item from future NEF criteria evaluation.

12. The initial NEF list shall be provided to the FAA along with initial MEL approval.  The updated list shall be included with all subsequent MEL revisions.
13. NOTE: This review I not to be conceived as a requirement o approve NEF items.  It is merely a means to provide oversight to ensure the program is effective.

Placarding Procedures

14. Items will be placarded on its face or as close as possible to it affected control, using appropriate terminology to describe the condition such as “INOP”, “REMOVED”, or “DO NOT OCCUPY.”
15. If the placement of the placard does not make is readily apparent which item is inoperative, then the name of the inoperative item must also appear on the placard as in “Light switch INOP.”

(M) Maintenance Procedures

16. If possible, deactivate the item and/or its source by disengaging the circuit breaker or disconnecting and stowing the electrical connector.

(O) Operations Procedures

17. Include notation of the inoperative items in the passenger briefing if applicable.

Definitions

1. System Definitions.

System numbers are based on the Air Transport Association (ATA) Specification Number 100 and items are numbered sequentially.

a.
"Item" (Column 1) means the equipment, system, component, or function listed in the "Item" column. Repair interval categories (A, B, C, and D) are listed on right side of column 1. Repair intervals are described in definition 22.

b.
"Number Installed" (Column 2) is the number (quantity) of items normally installed in the aircraft. This number represents the aircraft configuration considered in developing this MMEL. Should the number be a variable (e.g., passenger cabin items) a number is not required.

c.
"Number Required for Dispatch" (Column 3) is the minimum number (quantity) of items required for operation provided the conditions specified in Column 4 are met.

NOTE:    Where the MMEL shows a variable number required for dispatch, the MEL must reflect the actual number required for dispatch or an alternate means of configuration control approved by the Administrator.

d.
"Remarks or Exceptions" (Column 4) in this column includes a statement either prohibiting or permitting operation with a specific number of items inoperative, provisos (conditions and limitations) for such operation, and appropriate notes.

e.
A vertical bar (change bar) in the margin indicates a change, addition or deletion in the adjacent text for the current revision of that page only. The change bar is dropped at the next revision of that page.

2.
"Airplane/Rotorcraft Flight Manual" (AFM/RFM) is the document required for type certification and approved by the responsible FAA Aircraft Certification Office. The FAA approved AFM/RFM for the specific aircraft is listed on the applicable Type Certificate Data Sheet.

3.
"As required by FAR" means that the listed item is subject to certain provisions (restrictive or permissive) expressed in the Federal Aviation Regulations operating rules. The number of items required by the FAR must be operative. When the listed item is not required by FAR it may be inoperative for time specified by repair category. The term “14 CFR” may be substituted for “FAR” in MMELs or operator MELs.

4.
Each inoperative item must be placarded to inform and remind the crewmembers and maintenance personnel of the equipment condition.

NOTE:   To the extent practical, placards should be located adjacent to the control or indicator for the item affected; however, unless otherwise specified, placard wording and location will be determined by the operator.

5.
"-" symbol in Column 2 and/or Column 3 indicates a variable number (quantity) of the item installed.

6.
"Deleted" in the remarks column after a sequence item indicates that the item was previously listed but is now required to be operative if installed in the aircraft.

7. 
As used in MMELs, "ER" refers to Extended Operations (ETOPS) of an airplane with operational approval to conduct ETOPS in accordance with the applicable regulations.

8.
"Federal Aviation Regulations" (FAR) means the applicable portions of the Federal Aviation Act and Federal Aviation Regulations.

9.
"Flight Day" means a 24 hour period (from midnight to midnight) either Universal Coordinated Time (UCT) or local time, as established by the operator, during which at least one flight is initiated for the affected aircraft.
Definitions (Continued)
10.
"Icing Conditions" means an atmospheric environment that may cause ice to form on the aircraft (structural) or in the engine(s) (induction).

11.
Alphabetical symbol in Column 4 indicates a proviso (condition or limitation) that must be complied with for operation with the listed item inoperative.

12.
"Inoperative" means a system and/or component malfunctions to the extent that it does not accomplish its intended purpose and/or is not consistently functioning normally within its approved operating limit(s) or tolerance(s).

13.
"Notes:" in Column 4 provides additional information for crewmember or maintenance consideration. Notes are used to identify applicable material which is intended to assist with compliance, but do not relieve the operator of the responsibility for compliance with all applicable requirements. Notes are not a part of the provisos.

14.
Inoperative components of an inoperative system: Inoperative items which are components of a system which is inoperative are usually considered components directly associated with and having no other function than to support that system. (Warning/caution systems associated with the inoperative system must be operative unless relief is specifically authorized per the MMEL).

15.
"(M)" symbol indicates a requirement for a specific maintenance procedure which must be accomplished prior to operation with the listed item inoperative. Normally these procedures are accomplished by maintenance personnel; however, other personnel may be qualified and authorized to perform certain functions. Procedures requiring specialized knowledge or skill, or requiring the use of tools or test equipment should be accomplished by maintenance personnel. The satisfactory accomplishment of all maintenance procedures, regardless of who performs them, is the responsibility of the operator. Appropriate procedures are required to be published as part of the operator's manual or MEL.

16.
"(O)" symbol indicates a requirement for a specific operations procedure which must be accomplished in planning for and/or operating with the listed item inoperative. Normally these procedures are accomplished by the flight crew; however, other personnel may be qualified and authorized to perform certain functions. The satisfactory accomplishment of all procedures, regardless of who performs them, is the responsibility of the operator. Appropriate procedures are required to be published as a part of the operator's manual or MEL.

NOTE: The (M) and (O) symbols are required in the operator's MEL unless otherwise authorized by the Administrator.

17.
"Deactivated" and "Secured" means that the specified component must be put into an acceptable condition for safe flight. An acceptable method of securing or deactivating will be established by the operator.

18.
"Visual Flight Rules" (VFR) is as defined in FAR Part 91. This precludes a pilot from filing an Instrument Flight Rules (IFR) flight plan.

19.
"Visual Meteorological Conditions" (VMC) means the atmospheric environment is such that would allow a flight to proceed under the visual flight rules applicable to the flight. This does not preclude operating under Instrument Flight Rules.

20.
"Visible Moisture" means an atmospheric environment containing water in any form that can be seen in natural or artificial light; for example, clouds, fog, rain, sleet, hail, or snow.

21.
"Passenger Convenience Items" Deleted see NEF #30

Definitions (Continued)
22.
Repair Intervals: All users of an MEL approved under FAR 121, 125, 129 and 135 must effect repairs of inoperative systems or components, deferred in accordance with the MEL, at or prior to the repair times established by the following letter designators:

Category A.  Items in this category shall be repaired within the time interval specified in the remarks column of the operator's approved MEL.  For time intervals specified in “calendar days” or "flight days," the day the malfunction was recorded in the aircraft maintenance record/logbook is excluded.  For all other time intervals (flights, flight legs, cycles, hours, etc), repair tracking begins at the point when the malfunction is deferred in accordance with the operator's approved MEL.


Category B.  Items in this category shall be repaired within three (3) consecutive calendar days (72 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook. For example, if it were recorded at 10 a.m. on January 26th, the three day interval would begin at midnight the 26th and end at midnight the 29th.


Category C.  Items in this category shall be repaired within ten (10) consecutive calendar days (240 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook. For example, if it were recorded at 10 a.m. on January 26th, the 10 day interval would begin at midnight the 26th and end at midnight February 5th.


Category D.  Items in this category shall be repaired within one hundred and twenty (120) consecutive calendar days (2880 hours), excluding the day the malfunction was recorded in the aircraft maintenance log and/or record. The letter designators are inserted adjacent to Column 2.

An operator who has the authorization to use an MEL also has the authority to approve extensions to the maximum repair interval for category B and C items provided the responsible Flight Standards District Office (FSDO) is notified within 24 hours of the MEL extension.  The operator is not authorized to extend A and D items in the MEL. Misuse of the MEL extension authority may result in the operators OpSpecs/Mspecs being amended by removing the authority for the operator to use the MEL extension authority and/or use an MEL.

23.
Electronic fault alerting system – General

New generation aircraft display system fault indications to the flight crew by use of computerized display systems. Each aircraft manufacturer has incorporated individual design philosophies in determining the data that would be represented.

The following are customized definitions (specific to each manufacturer) to help determine the level of messages affecting the aircraft's dispatch status. When preparing the MEL document, operators are to select the proper Definition No. 23 for their aircraft, if appropriate.

NO CUSTOMIZED DEFINITIONS OF FAULT ALERTING ARE APPLICABLE TO THE BELL HELICOPTER MODEL BH-427 SERIES AIRCRAFT.

24.
Not Required
25.
Not Required

26.
"Excess Items" means those items that have been installed that are redundant to the requirements of the FARs.

Definitions (Continued)

27.
"Day of Discovery" is the calendar day an equipment/instrument malfunction was recorded in the aircraft maintenance log and or record. This day is excluded from the calendar days or flight days specified in the MMEL for the repair of an inoperative item of equipment. This provision is applicable to all MMEL items, i.e., categories "A, B, C, and D."

28.
"Considered Inoperative", as used in the provisos means that item must be treated for dispatch, taxi and flight purposes as though it were inoperative. The item shall not be used or operated until the original deferred item is repaired. Additional actions include: documenting the item on the dispatch release (if applicable), placarding, and complying with all remarks, exceptions, and related MMEL provisions, including any (M) and (O) procedures and observing the repair category.

29.
"Is not used" in the provisos, remarks or exceptions for an MMEL item may specify that another item relieved in the MMEL “is not used.” In such cases, crewmembers should not activate, actuate, or otherwise utilize that component or system under normal operations. It is not necessary for the operators to accomplish the (M) procedures associated with the item. However, operational requirements must be complied with, and an additional placard must be affixed, to the extent practical, adjacent to the control or indicator for the item that is not used to inform crewmembers that a component or system is not used under normal operations.

30.
Nonessential equipment and furnishings (NEF) are those items installed on the aircraft as part of the original type certification, supplemental type certificate, or other form of alteration that have no effect on the safe operation of flight and would not be required by the applicable certification rules or operational rules. They are those items that if inoperative, damaged or missing have no effect on the airplane’s ability to be operated safely under all operational conditions. These nonessential items may be installed in areas including, but not limited to, the passenger compartment, flight deck area, service areas, cargo areas, crew rest areas, lavatories, and galley areas. NEF items are not items already identified in the MEL or CDL of the applicable airplane. They do not include items that are functionally required to meet the certification rule or for compliance with any operational rule. Operator’s NEF process shall not provide for deferral of items within serviceable limits identified in the manufacture’s maintenance manual or operator’s approved maintenance program such as wear limits, fuel/hydraulic leak rates, oil consumption, etc. Cosmetic items that are fully serviceable but worn or soiled may be deferred under an operator’s NEF process.

31.     As used in MMELs, Heavy Maintenance Visit (HMV) is a scheduled C-check/D-check or airworthiness maintenance program inspection where the aircraft is scheduled to be out of service for 4 or more days.

Preamble

The following is applicable for authorized certificate holders operating under Federal Aviation Regulations (FAR) Parts 121, 125, 129, and 135: The FAR require that all equipment installed on an aircraft in compliance with the Airworthiness Standards and the Operating Rules must be operative. However, the Rules also permit the publication of a Minimum Equipment List (MEL) where compliance with certain equipment requirements is not necessary in the interests of safety under all operating conditions. Experience has shown that with the various levels of redundancy designed into aircraft, operation of every system or installed component may not be necessary when the remaining operative equipment can provide an acceptable level of safety. A Master Minimum Equipment List (MMEL) is developed by the FAA, with participation by the aviation industry, to improve aircraft utilization and thereby provide more convenient and economic air transportation for the public. The FAA approved MMEL includes those items of equipment related to airworthiness and operating regulations and other items of equipment which the Administrator finds may be inoperative and yet maintain an acceptable level of safety by appropriate conditions and limitations; it does not contain obviously required items such as wings, flaps, and rudders. The MMEL is the basis for development of individual operator MELs which take into consideration the operator's particular aircraft equipment configuration and operational conditions. Operator MELs, for administrative control, may include items not contained in the MMEL; however, relief for administrative control items must be approved by the Administrator. An operator's MEL may differ in format from the MMEL, but cannot be less restrictive than the MMEL. The individual operator's MEL, when approved and authorized, permits operation of the aircraft with inoperative equipment.

Equipment not required by the operation being conducted and equipment in excess of FAR requirements are included in the MEL with appropriate conditions and limitations. The MEL must not deviate from the Aircraft Flight Manual Limitations, Emergency Procedures or with Airworthiness Directives. It is important to remember that all equipment related to the airworthiness and the operating regulations of the aircraft not listed on the MMEL must be operative.

Suitable conditions and limitations in the form of placards, maintenance procedures, crew operating procedures and other restrictions as necessary are specified in the MEL to ensure that an acceptable level of safety is maintained.

The MEL is intended to permit operation with inoperative items of equipment for a period of time until repairs can be accomplished. It is important that repairs be accomplished at the earliest opportunity. In order to maintain an acceptable level of safety and reliability the MMEL establishes limitations on the duration of and conditions for operation with inoperative equipment.

The MEL provides for release of the aircraft for flight with inoperative equipment. When an item of equipment is discovered to be inoperative, it is reported by making an entry in the Aircraft Maintenance Record/Logbook as prescribed by FAR. The item is then either repaired or may be deferred per the MEL or other approved means acceptable to the Administrator prior to further operation. MEL conditions and limitations do not relieve the operator from determining that the aircraft is in condition for safe operation with items of equipment inoperative.

When these requirements are met, an Airworthiness Release, Aircraft Maintenance Record/Logbook entry, or other approved documentation is issued as prescribed by FAR. Such documentation is required prior to operation with any item of equipment inoperative. 

Operators are responsible for exercising the necessary operational control to ensure that an acceptable level of safety is maintained. When operating with multiple inoperative items, the interrelationships between those items and the effect on aircraft operation and crew workload will be considered.

Operators are to establish a controlled and sound repair program including the parts, personnel, facilities, procedures, and schedules to ensure timely repair.

WHEN USING THE MEL, COMPLIANCE WITH THE STATED INTENT OF THE PREAMBLE, DEFINITIONS, AND THE CONDITIONS AND LIMITATIONS SPECIFIED IN THE MEL IS REQUIRED.

Guidelines for (O) & (M) Procedures

The FOEB has identified a need for certain procedures to provide an adequate level of safety while providing relief for some items. Those procedures must be established by the operator. The following guidelines specify the objectives of the required procedures:

21-3

(M)
Procedure to deactivate and secure bleed air heater.

21-4

(M)
Procedure to deactivate and secure air conditioner

21-5

(O)
Refer to RFM operating limitations


(M)
Procedure to deactivate and secure IIDS Fan(s)
23-4

(O)
Procedure to establish alternate means for passenger          

                  

notification of normal and emergency procedures.              

24-1

(M)
Procedure to deactivate and secure generator.
24-3

(M)
Procedure to determine adequate starting voltage.
27-1

(M)
Procedure to de-activate, secure and disengage the AAPS system.                                                       

.

28-1

(O)
Procedure to verify that fuel drain solenoid valve is closed.


28-3

(M)
Procedure to verify remaining fuel transfer pump and fuel     

                  

transfer control unit (FTCU) are both operative.              



(O)
Procedure to create flight plans based on a known quantity of 

                  

unusable fuel in the aft fuel cell
28-4

(O)
Procedure to determine the fuel temperature.


28-5

(O)
Dual Channel Failure                                          

                  

Procedure to verify operation of transfer pumps, the          

                  

interconnect valve, and procedure to maintain aircraft c.g.   

                  

within acceptable limits.                                     
	HELICOPTER FLIGHT SERVICES  
	
	
	
	
	

	
	
	
	
	
	
	MINIMUM EQUIPMENT LIST

	
	
	
	
	
	
	

	AIRCRAFT:
	
	
	
	
	
	REVISION NO: Original
	PAGE:

	BH-427 SERIES
	
	
	
	
	

	
	
	
	
	
	
	DATE: 10/01/13
	21-1

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	ITEM
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	21  AIR CONDITIONING
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Fresh Air Vent
	C
	2
	1
	May be inoperative

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Defog Air Blower
	C
	2
	1
	May be inoperative provided:

	
	
	
	
	
	

	
	
	
	
	1)
	Bleed Air Heater (item 21-3) is installed and operative

	
	
	
	
	
	
	

	
	
	
	
	
	or

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	Air Conditioner (item 21-4) is installed and operative

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Bleed Air Heater
	C
	1
	0
	(M)
	May be inoperative provided:  

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Maintenance will pull and collar the Heater CB

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	Disconnect the bleed air heater line at the engine scroll then cap the line and outlet with stainless steel caps.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Perform a leak check before returning to service.

	
	
	
	
	
	
	

	4
	Air Conditioner 
	C
	1
	0
	(M)
	May be inoperative provided:

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Maintenance will inspect air conditioner in accordance with manufacture’s recommendations and determine failure cause to assure no further damage will occur,

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	Maintenance will ensure drive system is not restricted by rotating compressor or removing belt,

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Maintenance will deactivate system by pulling circuit breaker and securing with collar.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	IIDS Cooling Fans
	C
	
	
	(M)
	May be inoperative provided:

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Maintenance will open Circuit barker B 2400CB2 and secure it using a tie wrap  

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	Pilot shall (RFM Operating Limitations)
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	DATE: 10/01/13
	23-1

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	23  COMMUNICATIONS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Communications Systems: 
	
	
	
	Any in excess of those required by CFR may be inoperative provided it is not powered by the, Emergency DC Bus, Battery Bus, or the DC Transfer Bus and not required for emergency procedures.

	
	(FM, HF, UHF, UHF etc.)
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	a)VHF Communications
	C
	2
	1
	One VHF Comm may be inoperative for VFR operations (except extended over water operations), provided operations are not predicated on the affected radio.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on control head.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Headset
	C
	6
	1
	Pilots must be operative.

	
	
	
	
	
	
	

	3
	ICS
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Cockpit
	C
	2
	1
	Copilot’s must be operative for single pilot operations.

	
	
	
	
	
	
	

	
	b) Cabin
	C
	1
	0
	Any in access of those required or for non passenger carrying operations may be inoperative, provided alternate procedures are established and used.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Pilot shall brief the passenger(s) regarding alternate normal and emergency procedures to be used. The Pilot briefing must include any appropriate operating restrictions.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Cabin Public Address System
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Cockpit Voice Recorder (CVR)
	A
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	6
	External Loud Speaker
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Satellite Tracking System(s), 
	D
	1
	0
	May be inoperative. 

	
	(i.e. Blue Sky, SkyConnect
	
	
	
	
	

	
	Outerlink, etc.)
	
	
	
	Place INOP placard on control head.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	8
	Satellite Phone (i.e. 
	D
	–
	0
	May be inoperative. Place INOP placard on control head.

	
	SkyConnect Satellite 
	
	
	
	
	

	
	Phone, etc.)
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	24  ELECTRICAL POWER
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Starter/Generator (Generator
	B
	2
	1
	One may be inoperative for day VFR provided the inoperative generator is deactivated and secured.

	
	Function Only)
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall:

	
	
	
	
	
	

	
	
	
	
	
	1)
	Inspect for burned or arched wires and ensure drive 

system is not restricted by rotating compressor,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Deactivate system by pulling and collaring the circuit breaker.

	
	
	
	
	
	
	

	
	
	
	
	
	
	or

	
	
	
	
	
	3)
	Remove starter/generator, remove mount plate, install blank, cap and stow cables.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Generator Voltmeter (s) 
	C
	2
	0
	May be inoperative.

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Battery Voltmeter
	C
	2
	0
	May be inoperative provided alternate means of assuring

	
	
	
	
	
	starting voltage is determined.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Ammeter
	C
	2
	1
	One may be inoperative provided operative ammeter and respective Generator (Item 24-1) are both operative.

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Generator 1 / Generator 2 
	C
	2
	0
	May be inoperative provided respective Ammeter 

(Item 24-4) and Voltmeter (Item 24-2) are operative.

	
	Caution Message (s)
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	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	25  EQUIPMENT/FURNISHINGS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Flotation Inflation System
	C
	1
	0
	May be inoperative. 

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	Except for takeoff and landings aircraft must be operated at an altitude and airspeed to reach a suitable forced landing area in the event of an engine failure.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Passenger Seat Belts and Shoulder Harnesses Devices
	C
	6
	0
	One required for each occupied seat. If inoperative 

or missing, seat must be blocked and placarded.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	NOTE: Front left seat is considered a passenger seat if dual controls are not installed.

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	First Aid Kit
	D
	1
	0
	May be missing. 

	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Emergency Locator 
	
	
	
	

	
	Transmitter (ELT)
	
	
	
	

	
	
	
	
	
	

	
	a) Survival Type ELTs
	D
	0
	​0
	Not installed.

	
	
	
	
	
	

	
	b) Fixed ELTs
	A
	​–
	0
	May be inoperative provided

	
	
	
	
	
	1)
	System is deactivated,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Repairs are made within 90 days.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Remove ELT and placard “ELT not installed” in 

	
	
	
	
	
	
	plain view of flight crew.

	
	
	
	
	
	
	

	
	
	A
	​–
	0
	May be missing provided repairs are made within 90 days.

	
	
	
	
	
	

	
	
	D
	–
	1
	Any in excess of one (1) ELT may be inoperative or missing.

	
	
	
	
	
	Placard “INOP” next to remote switch.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	EMS Equipment
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Sonic Locator
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Forward Looking Infra Red (FLIR)
	C
	0
	0
	Not installed.
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	25  EQUIPMENT/FURNISHINGS
	
	
	
	
	

	
	
	
	
	
	
	

	8
	Hoist System
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	9
	Aerial Camera System
	C
	0
	0
	Not installed.

	
	(i.e. Wescam)
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	10
	Cargo Suspension System
	C
	0
	0
	May be inoperative.

	
	
	
	
	
	
	

	
	
	
	
	
	

	11
	Non-essential Furnishings (NEF)
	
	‒
	0
	May be inoperative, damaged, or missing provided that the item(s) is deferred in accordance with the operator's NEF deferral program. The NEF program, procedures, and processes are outlined in the Helicopter Flight Services Minimum Equipment List. 

(M) and/or (O) procedures, if required, must be available to the flight crew and included in the operator's appropriate document.

NOTE: EXTERIOR LAVATORY DOOR ASH TRAYS ARE NOT CONSIDERED NEF ITEMS.
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
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	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	26  FIRE PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Fire Extinguisher Agent 
	B
	2
	1
	One Fire Extinguisher Agent bottle may be inoperative.

	
	Bottles
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Portable Fire Extinguisher
	D
	1
	1
	Any in excess of those required by FAR may be inoperative 

	
	
	
	
	
	or missing provided:

	
	
	
	
	
	

	
	
	
	
	
	1)
	The inoperative fire extinguisher is tagged inoperative, removed from the installed location, and placed out of sight so it cannot be mistaken for a functional unit,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Required distribution is maintained.
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	27  FIRE PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Airspeed Activated
	B
	1
	0
	May be inoperative provided:

	
	Pedal Stop (AAPS)
	
	
	
	

	
	
	
	
	
	
	1) AAPS System is deactivated, secured and

	
	
	
	
	
	
	    Disengaged,

	
	
	
	
	
	and

	
	
	
	
	
	
	2) Comply with RFM VNE limitations for AAPS

	
	
	
	
	
	
	    inoperative

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall
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	 2. NUMBER INSTALLED
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	28  FUEL
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Solenoid Drain Valve System
	D
	2
	0
	May be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Prior to flight, crew shall perform a visual check to verify the manual drain valve is closed. 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Fuel Flow Indicator
	C
	1
	0
	May be inoperative provided flight is not predicated on

	
	
	
	
	
	its use.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Fuel Transfer Pump
	C
	2
	1
	May be inoperative provided:

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	1) The remaining pump and its associated FTCU

	
	
	
	
	
	
	    Channel are verified operative, 

	
	
	
	
	
	
	

	
	
	
	
	
	
	2) The interconnect vale is maintained in the open

	
	
	
	
	
	
	    position

	
	
	
	
	
	
	and

	
	
	
	
	
	(O)
	3) Flight planning is based on quantity of unusable 

	
	
	
	
	
	
	    fuel in the aft tank as defined in the RFM 

	
	
	
	
	
	
	    procedures for Dual Transfer Pump Failure.

	
	
	
	
	
	
	

	4
	Fuel Temperature Display
	C
	1
	0
	May be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	(O)
	Prior to flight, crew shall perform a visual check to verify the manual drain valve is closed. 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Fuel Transfer Control Unit (FTCU)
	B
	1
	0
	Dual Channel Failure

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	May be inoperative provided:

	
	
	
	
	
	
	

	
	
	
	
	
	
	1) Both transfer pumps are verified operative,

	
	
	
	
	
	
	

	
	
	
	
	
	
	2) The interconnect valve is verified operative, 

	
	
	
	
	
	
	and

	
	
	
	
	
	
	3) An alternate procedures is used to maintain 

	
	
	
	
	
	
	    aircraft CG limits

	
	
	
	
	
	
	

	
	
	C
	1
	0
	Single Channel Failure

	
	
	
	
	
	
	

	
	
	
	
	
	
	May be inoperative provided:

	
	
	
	
	
	
	

	
	
	
	
	
	
	 1) The affected transfer pump is selected to “off”

	
	
	
	
	
	
	

	
	
	
	
	
	
	2) The remaining pump and its associated FTCU

	
	
	
	
	
	
	    channel are verified operative,

	
	
	
	
	
	
	and

	
	
	
	
	
	
	3) The interconnect valve is maintained in the open

	
	
	
	
	
	
	    position.
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	28  FUEL
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Fuel Interconnect Valve
	B
	1
	0
	May be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	(M)
	May be inoperative in the closed position provided both Transfer Pumps and both FTCU channels are
verified operative.
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	 2. NUMBER INSTALLED
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	30  ICE AND RAIN PROTECTION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Pitot Tube Heat
	C
	1
	0
	May be inoperative provided aircraft is not operated in

	
	
	
	
	
	Visible moisture with OAT below 4° C (40° F)

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Static Port Heaters
	C
	1
	0
	May be inoperative provided aircraft is not operated in

	
	
	
	
	
	Visible moisture with OAT below 4° C (40° F)
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	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	31  INDICATING/RECORDING SYSTEMS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Clock, Displaying Hours, Minutes and Seconds.
	C
	2
	1
	Operative clock displaying hours, minutes and seconds with sweep second pointer or an electric digital clock must be located on the instrument panel in a position that makes it plainly visible to, and usable by any pilot at the pilot's station.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	C
	1
	0
	May be inoperative provided Elapsed Timer (item 31-2)

	
	
	
	
	
	Is operative.

	
	
	
	
	
	
	

	2
	Elapsed Timer
	C
	1
	0
	May be inoperative provided Clock is operative.

	
	
	
	
	
	
	

	3
	Hour Meter
	C
	1
	0
	May be inoperative provided 

	
	
	
	
	
	

	
	
	
	
	
	(O)
	An alternate means is utilized for recording time in service; Davtron, wrist watch, etc.,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	All flight time with hour meter inoperative will be

recorded and entered in the aircraft logbook,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	(M)
	Adjustments to maintenance time will be recorded in the logbook when the hour meter is repaired.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on meter.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	IIDS Sensor Sources for:
	
	
	
	May be inoperative provided:

	
	Np
	
	
	
	
	

	
	or
	
	
	
	1)
	Only one sensor per engine is inoperative

	
	NG
	
	
	
	
	or

	
	or
	
	
	
	2)
	Only one Nr sensor is inoperative

	
	NR
	
	
	
	
	

	
	or
	
	
	
	
	

	
	MGT
	
	
	
	
	

	
	or
	
	
	
	
	

	
	Engine Torque
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Rotor RPM Warning Horn Mute 
	C
	1
	0
	May be inoperative provided Horn sounds properly at 70-

	
	System
	
	
	
	90% Nr, but does not sound above 95% Nr.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Aircraft/Engine Monitoring 
	D
	1
	0
	May be inoperative.

	
	System.
	
	
	
	

	
	
	
	
	
	
	

	7
	Vibration Monitoring System
	D
	0
	0
	Not installed.
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	33  LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Position Light System
	C
	1
	0
	May be inoperative for day. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Anti-Collision Light System
	B
	1
	0
	May be inoperative for day. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Landing/Search Light System
	C
	1
	0
	One or both may be inoperative for day.  One may be inoperative for night.  Both may be inoperative for night provided that a searchlight is installed and operating.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch(s).                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Cockpit/Flight Deck/Flight  

Compartment and Instrument
	C
	–
	–
	Individual light may be inoperative provided:

	
	
	
	
	
	

	
	Lighting System
	
	
	
	1)
	Remaining Lighting System lights are sufficient lighting is available to make each required instrument, control and other device for which they are provided,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	Remaining Lighting System lights are positioned to that direct rays are shielded from flight crewmembers eyes,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Lighting configuration and intensity is acceptable to the flight crew.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Note 1:
	Individual button/switch lights and/or annunciations/ indications are excluded from this relief.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Note 2:
	Unaided operation (without NVG’s) may be permitted with inoperative NVG supplemental lights: cracked or missing filters.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch(s).                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Cockpit Emergency Instrument 
	C
	1
	0
	May be inoperative for day operations. 

	
	Light
	
	
	
	or

	
	
	
	
	
	May be inoperative for night Operations provide the Cockpit/Flight Deck/Flight Compartment and Instrument Lighting System (Item 33-4) and Cockpit Emergency Light (Item 33-5) are operative.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          
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	33  LIGHTS
	
	
	
	
	

	
	
	
	
	
	
	

	7
	Cabin Lighting System
	C
	1
	0
	May be inoperative provided:                           

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	For day operations only.

	
	
	
	
	
	
	or

	
	
	
	
	
	2)
	Inoperative lights do not exceed fifty (50) percent of total installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	8
	Search Light System
	C
	–
	0
	May be inoperative. Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	9
	Supplemental Lighting System
	C
	1
	0
	May be inoperative. 

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	10
	Strobe Light System
	C
	–
	0
	May be inoperative. 

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	11
	External Utility Lights
	C
	–
	0
	May be inoperative. 

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on switch.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	12
	High Intensity Search Light
	C
	0
	0
	Not Installed.

	
	(i.e. SX5, SX16, etc.)
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	


	HELICOPTER FLIGHT SERVICES 
	
	
	
	
	

	
	
	
	
	
	
	MINIMUM EQUIPMENT LIST

	
	
	
	
	
	
	

	AIRCRAFT:
	
	
	
	
	
	REVISION NO: ORIGINAL
	PAGE:

	BH-427 SERIES
	
	
	
	
	

	
	
	
	
	
	
	DATE: 10/01/13
	34-1

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Gyroscopic Bank and Pitch 
	B
	1
	0
	May be inoperative for Day, Night VFR use.

	
	Indicator
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	2
	Gyroscopic Directional 
	B
	1
	0
	 May be inoperative for Day, Night VFR use, except for:

	
	Indicator
	
	
	
	

	
	
	
	
	
	1)
	VFR over-the-top conditions.

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Gyroscopic Rate-of-Turn 
	B
	1
	0
	May be inoperative for Day, Night VFR use.                        

	
	Indicator
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Slip-Skid Indicator
	B
	1
	0
	May be inoperative for Day, Night VFR use.                        

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Horizontal Situation Indicator
	C
	1
	0
	May be inoperative. 

	
	Indicator
	
	
	
	

	
	
	
	
	
	Place INOP placard on indicator.                        

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	6
	Slaved Compass System
	C
	1
	0
	May be inoperative.

	
	
	
	
	
	
	

	
	
	
	
	
	(O)
	The pilot MUST align the DG with wet compass at intervals not to exceed 10 Minutes.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	7
	OAT/Free Air
	C
	1
	0
	May be inoperative provided approved alternate onboard 

OAT source is installed and operative.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on gauge.                          
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	AIRCRAFT:
	
	
	
	
	
	REVISION NO: ORIGINAL
	PAGE:

	BH-427 SERIES
	
	
	
	
	

	
	
	
	
	
	
	DATE: 10/01/13
	34-2

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	8
	Navigation Equipment
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) VOR Navigation System.
	C
	1
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the VOR system(s) may be inoperative provided at least one navigation system (ADF, GPS, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the VOR(s) may be inoperative provided two of the following navigation systems are operative: (ADF, GPS, RNAV)

	
	
	
	
	
	
	

	
	b) RNAV Navigation System.
	C
	1
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the RNAV system(s) may be inoperative provided at least one navigation system (ADF, GPS, and VOR) is operative. Two navigation systems must be operative when conducting extended over water operations in which case the RNAV(s) may be inoperative provided two of the following navigation systems are operative: (ADF, GPS, VOR)

	
	
	
	
	
	
	

	
	c) ADF Navigation System.
	C
	1
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the ADF system(s) may be inoperative provided at least one navigation system (VOR, GPS, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the ADF(s) may be inoperative provided two of the following navigation systems are operative: (VOR, GPS, RNAV)

	
	
	
	
	
	
	

	
	d) GPS System.
	C
	1
	0
	One navigation system must be operative for VFR over the top or night VFR in which case the GPS system(s) may be inoperative provided at least one navigation system (ADF, VOR, and RNAV) is operative.  Two navigation systems must be operative when conducting extended over water operations in which case the GPS(s) may be inoperative provided two of the Following navigation systems are operative (ADF, VOR, RNAV)

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on affected system control head.                          
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	34-3

	
	
	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	9
	Marker Beacon
	C
	1
	0
	May be inoperative provided an instrument approach is not predicated on its use.

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	10
	DME
	C
	1
	0
	Not required for flights conducted below FL240 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	11
	Flight Director
	C
	0
	0
	Not installed.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	12
	ATC Transponder 
	C
	2
	0
	May be inoperative provided;

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Enroute operations do not require its use,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Prior to flight, approval is obtained from ATC facilities

	
	
	
	
	
	
	having jurisdiction over the planned route of flight.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	D
	2
	1
	Any in excess of one (1) may be inoperative.

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on control head.                          

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	13
	Altitude Encoding System
	C
	2
	0
	May be inoperative, except for operations in the following:

	
	
	
	
	
	
	

	
	
	
	
	
	1)
	Enroute operations do not require its use,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Prior to flight, approval is obtained from ATC facilities
having jurisdiction over the planned route of flight.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	D
	2
	1
	Any in excess of one (1) may be inoperative.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	14
	Radio Altimeter
	C
	1
	0
	May be inoperative for VFR use.

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on instrument.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	15
	Thunderstorm Detection
	
	
	
	
	

	
	Equipment
	
	
	
	
	

	
	
	
	
	
	
	

	
	a) Cockpit Weather Displays
	C
	2
	0
	May be inoperative. Place INOP placard on display.

	
	
	
	
	
	
	

	
	
	D
	2
	1
	Any in excess of one (1) may be inoperative.
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	 2. NUMBER INSTALLED
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	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	34  NAVIGATION
	
	
	
	
	

	
	
	
	
	
	
	

	16
	Traffic Alert / Advisory Systems 
	C
	–
	0
	May be inoperative provided:

	
	(i.e., TCAS, TCAD, TAS, etc.)
	
	
	
	

	
	
	
	
	
	1)
	Aircraft is not operated with a passenger configuration     
of 10 or more seats, excluding any pilot,

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	2)
	System is deactivated and secured,

	
	
	
	
	
	
	and

	
	
	
	
	
	3)
	Enroute or approach procedures do not require its use.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Secure system by pulling and collaring circuit breaker.

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on Unit.

	
	
	
	
	
	

	
	
	
	
	
	

	
	a) Traffic Alert Display System(s)
	C
	–
	–
	Display(s) may be inoperable provided: 

	
	  (TAS, TCAS I)
	
	
	
	

	
	
	
	
	
	1)
	Other Traffic Alert Display(s) are functioning properly
and displaying correct information, 

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	TA audio functions are operative. (TCAS I Only)

	
	
	
	
	
	
	

	
	
	
	
	
	
	Place INOP placard on display.

	
	
	
	
	
	

	
	b) Audio Functions (TCAS I)
	B
	–
	–
	May be inoperative provided enroute or approach procedures 

	
	
	
	
	
	do not require the use of TCAS I.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Secure system by pulling and collaring circuit breaker.
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	35  OXYGEN
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Oxygen System and Masks 

(Crew and Passengers)
	C
	0
	0
	Not Installed.
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	 2. NUMBER INSTALLED

	SYSTEM &
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	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	52  DOORS
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Baggage Door Caution System
	C
	1
	0
	May be inoperative provided all baggage is secured, and a visual check verifies that the door is closed, and latched, prior to each flight.

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard on caution light.
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	1
	 2. NUMBER INSTALLED

	SYSTEM &
	ITEM
	
	
	 3. NUMBER REQUIRED FOR DISPATCH

	SEQUENCE
	
	
	
	
	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	65  ROTORS
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Rotor Brake System
	C
	1
	0
	May be inoperative;

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall;

1) Safety the handle in the off position to prevent inadvertent use of the rotor brake, 

2) Ensure the brake pads are not contacting the rotor brake disk, 
3) Perform a visual inspection to ensure that no hydraulic leaks exist,

                                    and

4) Ensure that the rotor is free.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	Place INOP placard next to Rotor Brake.

	
	
	
	
	
	

	2
	Transmission Oil Temperature
	B
	1
	0
	May be inoperative provided:

	
	Warning Light System
	
	
	
	

	
	
	
	
	
	1)
	Transmission oil temperature indicating system is

operative,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Transmission oil pressure indicating and warning light systems are operative.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	3
	Transmission Oil Pressure
	B
	1
	0
	May be inoperative provided:

	
	Warning Light System
	
	
	
	

	
	
	
	
	
	1)
	Transmission oil pressure indicating system is
operative,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Transmission oil temperature indicating and warning light systems are operative.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	4
	Transmission Oil Temperature
	B
	1
	0
	May be inoperative provided:

	
	Indicating System
	
	
	
	

	
	
	
	
	
	1)
	Transmission oil temperature warning light systems 
are operative,

	
	
	
	
	
	
	

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Transmission oil pressure indicating and warning light systems are operative.

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	5
	Transmission Oil Pressure
	B
	1
	0
	May be inoperative provided:

	
	Indicating System
	
	
	
	

	
	
	
	
	
	1)
	Transmission oil pressure warning light system is

	
	
	
	
	
	
	Operative,

	
	
	
	
	
	
	and

	
	
	
	
	
	2)
	Transmission oil temperature indicating and warning light systems are operative.
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	1
	 2. NUMBER INSTALLED
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	4. REMARKS OR EXCEPTIONS

	NUMBERS
	
	
	
	
	
	

	
	
	
	
	
	
	

	71  POWERPLANT
	
	
	
	
	

	
	
	
	
	
	
	

	1
	Engine Air Particle Separator
	C
	1
	0
	May be inoperative provided bleed air for Particle Separator

	
	Purge System
	
	
	
	Is secured in the “closed” position.

	
	
	
	
	
	
	

	
	
	
	
	
	(M)
	Maintenance shall…….. 

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	(O)
	May be inoperative provided operations are

	
	
	
	
	
	conducted in accordance with the RFM.

	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	
	


