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MMEL Policy Letter (PL) 25, Revision 22
Date:	08/19/2021
To:	Manager, Aircraft Evaluation Division (AFS-100)
All Aircraft Evaluation Group Managers
	All Safety Assurance Offices
From:	Manager, Air Transportation Division (AFS-200)
Reply to Attn of:	Manager, New Program Implementation Branch (AFS-240)
SUBJECT:	MMEL/MEL Definitions
MMEL CODE:	00 (General)
REFERENCE:	PL-25, Revision 21, dated May 11, 2015.
	PL-25, Revision 20, dated December 17, 2012.
	PL-25, Revision 19, dated October 9, 2012.
	PL-25, Revision 18, dated July 27, 2012.
	PL-25, Revision 17, dated January 20, 2011.
	PL-25, Revision 16, dated April 2, 2010.
	PL-25, Revision 15, dated November 2, 2009.
	PL-25, Revision 14, dated August 26, 2008.
	PL-25, Revision 13, dated September 11, 2006.
	PL-25, Revision 12, dated June 5, 2006.
	PL-25, Revision 11, dated July 5, 2005.
	PL-25, Revision 10, undated.
	PL-25, Revision 9, dated August 15, 1997.
	PL-25, Revision 8, dated January 31, 1995.
PURPOSE:
To provide a list of definitions for use in Master Minimum Equipment Lists (MMEL) and minimum equipment lists (MEL).
REVISION HISTORY:
Revision 22: In general, Revision 22 clarifies, restates, or more fully presents definitions; separates a definition itself from how to apply it in an MMEL or MEL; and makes editorial changes for standardization.
Amended policy statement for clarity and to provide overarching guidance for inclusion of definitions in an operator’s MEL. Separately identifying each element as required or optional is no longer needed.
Included all instances of “instrument and equipment” as part of the more comprehensive term, “Items,” as defined below.
Standardized use of aircraft operator, remarks or exceptions versus proviso, Title 14 of the Code of Federal Regulations (14 CFR), repair category versus repair interval, and indicates versus depicts.
Spelled out numerical values where appropriate.
Reformatted content into a tabular layout to display the element and definition.
Added Pilot’s Operating Handbook (POH) to Airplane Flight Manual (AFM) as another approved flight document.
Relocated portions of previous definition 5 (as required by 14 CFR) to “Code of Federal Regulations….”
Added definition for “Contaminated Runway.”
Added definition for “Night.”
Replaced last two sentences of “Day of Discovery” with reference to sub-elements of Repair Category as they discuss exclusion of date recorded.
Expanded “Deactivated” or “Secured” to reflect manufacturer as another source for acceptable procedure.
Expanded “Deleted” or “Moved” to add “no longer addressed by the MMEL” as not all items are deleted because of now being required operative; introduced “moved.”
Replaced title of “Extended Range (ER) Operations” with “Extended Operations (ETOPS)” per 14 CFR part 1.
Changed “Excess Items” to replace use of “redundant.” Added reference to “Required by 14 CFR,” as it discusses common uses of the term “excess.”
Expanded “Icing Conditions” to include additional sources for defined icing conditions.
Clarified language in Operative to distinguish “considered” from “verified.”
Replaced “AFM” with “MMEL proviso” in Placarding as more appropriate source for placarding instructions.
Used “Day of Discovery” in place of text regarding aircraft maintenance record sub-elements for Repair Category.
Amended System Page to accommodate a Section Two in MMEL format.
Added sub-element, “Item Number.”
Clarified use of dash “-” in sub-elements, “Number Installed” and “Number Required for Dispatch.”
Amended sub-element, “Remarks or Exceptions” to clarify content or purpose.
Revised triple asterisk (***) to remove wording about an item not required by regulation.
Removed all aircraft-specific references in Electronic Fault Alerting System (EFAS); replaced with general information and referral to appropriate documentation by manufacturer.
Updated Appendix A with additional items and current 14 CFR references.
Changed use of “Considered Inoperative, Continuing Authorization, Deactivated and/or Secured, Extended Operations (ETOPS), Icing Conditions, Is Not Used,” and “Repair Category” to Optional with supporting notes. Removed all notes stating, “See PL-25 Policy Statement (page 2),” as the policy statement did not provide sufficient information for determining required versus optional.
Restructured and updated Appendix B.
Revision 21: Removed all reference to 14 CFR part 382 accessible lavatory. Definition numbers were not changed.
Revision 20: Added a third note to the “Policy” paragraph, page 2; corrected discrepancies found in definition 32.H.
Revision 19: Updated definition of “Take-off.” Added the phrase, “See PL-25 Policy Statement (page 2)” to the “Notes” of several definitions found in Appendix B of this PL.
Revision 18: Removed 14 CFR part 382 items from NEF (definition 21) and added accessible lavatory items (definition 1), listing part 382 general items, and specific §§ 382.63 and 382.71 items. Placed definitions in alphabetical order. Consolidated PL-70 into Appendix B of this PL. Also added the following definitions: Air Transport Association (ATA) System Page (definition 3), operative (definition 22), and takeoff (definition 25). Added Appendix B, MEL Definition Requirements. Aligned the definitions of this PL with the definitions found in FAA Order 8900.1, Volume 4, Chapter 4, Section 1.
NOTE:	The ATA changed its name in 2011 to “Airlines for America (A4A).” “ATA” and “A4A” are interchangeable.
Revision 17: Added a Note to definition 3, adds the Boeing Model 747-8 to definition 23a and adds Appendix A. Definitions 22 and 24 are also modified for clarity.
Revision 16: Corrected revision bar requirement in definition 1e; deleted the Passenger Convenience definition 21; revised the Electronic Fault Alerting System for Airbus aircraft (definition 23c); and added new MMEL definition 31 for Heavy Maintenance Visit (HMV).
Revision 15: Revised definition 22.A. “Category A Repair Interval” by including a reference to “calendar-days,” aligning the criteria for Day of Discovery with definition 27 “Day of Discovery.” A 380 aircraft added to definitions, 23c.
Revision 14: Revised definition 1a to include the listing of the repair interval categories (A, B, C, and D) in column 1, revised definition 7 to align with recent ETOPS rulemaking, added day of discovery to definition 22 Category A, added MEL repair interval extensions information to definition 22, added “787” to definition 23a, added G-150 and G-200 to definition 23g, corrected NEF definition 30 to align with Order 8900.1. Volume 4 (Aircraft Equipment and Operational Authorizations), Chapter 4 (MEL and CDL), Section 11 (NEF), paragraph 4-898.
Revision 13: Added clarification to definition 10. Icing Conditions for aircraft (structural) and engines (induction) icing.
Revision 12: Added definitions for “considered Inoperative,” “is not used” and “Nonessential equipment and furnishings (NEF).” Added the term “14 CFR” to Definition 3 (as required by FAR).
Revision 11: Added the Boeing 717 and MD-10 aircraft to the definitions paragraph 23b. as both aircraft are Electronic Instrument Systems (EIS)-equipped aircraft. Definition 23c (Airbus) has been revised to add A-318 to the fleet listing and clarify requirements for MAINTENANCE status (Class II) messages. Definition 23f (Embraer EMB-145) has been revises to add applicable models EMB-135/145 and ERJ‑170/190. Definition 23g (Gulfstream) has also been revised to add applicable models G-IV, GV-SP, and GIV-X. This revision also changes MMEL Definition to Revision 11.
POLICY:
Use the following definitions in MMELs. For MELs, certain MMEL definitions may be edited or may be omitted if the element is not used in the operator’s MEL. MEL definitions will be tailored, as appropriate, including content and format, dependent upon the aircraft operator’s make/model of aircraft, type of installed items, and specific operation. However, the intent of the definition must be the same and cannot be less restrictive than the MMEL. Refer to FAA Order 8900.1, Volume 4, Chapter 4 for further information.
The table that begins following Note 3 contains elements used in an MMEL or MEL, or both.
For MEL development, Appendix A may be used to identify the applicable Code of Federal Regulations (CFR) for MMEL items that use terms such as “As required by 14 CFR” or “Any in excess of those required by 14 CFR may be inoperative.” Appendix A is not a complete list of CFRs and is not to be included in the aircraft operator’s MEL. See Appendix B for MEL definition requirements; Appendix B is not to be included in operator’s MEL.
A revision of PL-25 does not require a revision of the aircraft operator’s MEL. However, applicable new or revised definitions must be incorporated at the next mandatory MEL revision. Flight Operations Evaluation Board (FOEB) Chairs will apply new policy at the next mandatory MMEL revision.
	Element
	Definition

	Administrative Control Item (ACI)
	An ACI is listed by the aircraft operator in the MEL for tracking and informational purposes. As an example, ACI may be used to track ETOPS accomplishment of required Auxiliary Power Unit (APU) cold‑soak, or in-flight verification starts. An ACI may be added to an aircraft operator’s MEL by approval of the Principal Operations Inspector (POI), provided no relief is granted, or provided conditions and limitations are contained in an approved document (e.g., Structural Repair Manual (SRM) or Airworthiness Directive (AD)). If relief other than that granted by an approved document is sought for an ACI, a request must be submitted to the Administrator. If the request results in review and approval by the FOEB, the item becomes an MMEL item rather than an ACI.

	Airplane Flight Manual (AFM), Rotorcraft Flight Manual (RFM), or Pilot’s Operating Handbook (POH)
	The FAA‑approved AFM/RFM (or POH) is the document approved by the responsible FAA Aircraft Certification Service office during type certification. The approved flight manual for the specific aircraft is listed on the applicable Type Certificate Data Sheet (TCDS). The approved flight manual is the governing document for operational limitations and performance parameters for an aircraft. The term approved flight manual can apply to an AFM/RFM (or POH). The FAA requires an approved flight manual for aircraft type certification.

	Code of Federal Regulations (CFR) and Federal Aviation Regulations (FAR)
	CFR and FAR both refer to the applicable portions of the Code of Federal Regulations and Federal Aviation Regulations.

	Considered Inoperative
	The phrase Considered Inoperative, as used in the Remarks or Exceptions column, means an item must be treated for dispatch, taxi with intent for flight, and flight purposes as though it were inoperative. The item must not be used or operated until the original deferred item is repaired. Additional actions include: documenting the item on the dispatch release, (if applicable); placarding; complying with all Remarks or Exceptions, including any (M) and (O) procedures; considering applicable notes; and observing the repair category.

	Contaminated Runway
	A runway condition where more than 25% of runway surface area (within reported length and width being used) is covered by frost, ice, and any depth of snow, slush, or water, as defined in Advisory Circular (AC) 25-31, AC 25-32, or approved flight manual (AFM, RFM or POH).




	Element
	Definition

	Continuing Authorization – Single Extension
	An aircraft operator who has authorization to use an FAA‑approved MEL may also have authority to use a continuing authorization to approve a single (one-time) extension to the repair interval for Repair Category B or C items in accordance with operations specification (OpSpec) D095. Continuing Authorization – Single Extension is not authorized for Repair Category A and D items.

	Dash (-)
	Indicates a variable number (quantity) of items may be installed or required for dispatch.

	Day of Discovery
	This is the calendar‑day an item malfunction was recorded in the aircraft maintenance record/logbook, and is excluded from the interval established by the assigned repair category. See definitions for sub‑elements of Repair Category.

	Deactivated or Secured
	When the MMEL refers to an item as “deactivated” or “secured,” or both, the specified item must be put into an acceptable condition for safe flight. An acceptable method of deactivating or securing may either be recommended by the manufacturer or established by the aircraft operator.

	Deleted or Moved
	Deleted in the Remarks or Exceptions column indicates the item was previously listed but is no longer addressed by the MMEL. Moved in the Remarks or Exceptions column indicates the item was moved within the chapter, to a different chapter in the MMEL, or another FAA-approved document.

	Electronic Fault Alerting System (EFAS)
	Many aircraft display system fault indications to the flightcrew by use of computerized display systems. Aircraft manufacturers incorporate individual design philosophies when determining the data to be presented. These systems are often referred to as Engine Indicating and Crew Alerting Systems (EICAS), Electronic Centralized Aircraft Monitoring (ECAM), Electronic Indication Systems (EIS), Central Maintenance Systems (CMS), Central Maintenance Computers (CMC), etc., depending on the aircraft and manufacturer. If the aircraft is equipped with an EFAS, refer to the applicable manufacturer’s manual for a system description, including various message levels, formats, limitations, and restrictions.

	Extended Operations (ETOPS)
	ETOPS refers to operations of an airplane with an operational approval to conduct ETOPS in accordance with the applicable regulations.

	Excess Items
	Excess items are items that have been installed in a quantity greater than that required by 14 CFR. See definition for Required by 14 CFR.

	Flight-Day
	A flight-day is a 24‑hour period (from midnight to midnight) either in Coordinated Universal Time (UTC) or local time, as established by the aircraft operator, during which at least one flight is initiated for the affected aircraft.

	Heavy Maintenance Visit (HMV)
	HMV is a scheduled inspection, such as a C-check/D-check, or airworthiness maintenance program inspection where the aircraft is scheduled to be out of service for four (4) or more consecutive calendar-days.




	Element
	Definition

	Icing Conditions
	An atmospheric environment that may cause ice to form on the aircraft (structural) or in the engine(s) (induction). Icing conditions may be known or forecast, and may be defined in the AFM, RFM, or POH.

	Inoperative
	Malfunction of an item to the extent that it does not accomplish its intended purpose or is not consistently functioning normally within its approved operating limit(s) or tolerance(s), or both.

	Inoperative Components of an Inoperative System
	Inoperative components of an inoperative system are usually considered components directly associated with and having no other function than to support that system. Warning/caution systems associated with the inoperative system must be operative unless relief is specifically authorized per the MMEL.

	Is Not Used
	The phrase Is Not Used in the Remarks or Exceptions column for an MMEL item may specify that another item is not used. In such cases, crewmembers must not activate, actuate, or otherwise use the referenced item under normal operations. If the item not to be used is located elsewhere in the MMEL, it is not necessary for aircraft operators to accomplish any (M) procedure(s) associated with the referenced item. However, operators must comply with operational requirements, and an additional placard must be affixed as close as practical to the control or indicator for the item that is not to be used. This informs crewmembers that an item is not to be used under normal operations.

	Item
	An instrument, equipment, system, component, message, or function that is installed on or exhibited by the aircraft.

	Night
	The time between the end of evening civil twilight and the beginning of morning civil twilight, as published in the Air Almanac, converted to local time.

	Nonessential Equipment and Furnishings (NEF)
	NEFs are those items installed on the aircraft as part of the original type certification (TC), Supplemental Type Certificate (STC), engineering order, or other form of alteration that have no effect on the safe operation of flight and would not be required by the applicable certification or operational rules. These are items that, if inoperative, damaged, or missing, have no effect on the aircraft’s ability to be operated safely under all operational conditions. NEF items are not items already identified in the MEL or Configuration Deviation List (CDL) of the applicable aircraft. NEF does not include items that are functionally required to meet the certification rule or for compliance with any operational rule.

	Operative
	An operative item will accomplish its intended purpose and is consistently functioning normally within its design operating limit(s) and tolerance(s). When an MMEL item specifies an item must be operative, it is not required to verify the item’s operational status. It should be considered operative unless reported or known to be malfunctioning. See definition for Verified Operative.




	Element
	Definition

	Placarding
	Each inoperative item must be placarded to inform and remind the crewmembers and maintenance personnel of the item’s condition. To the extent practical, placards should be located adjacent to the control or indicator for the item affected. Unless otherwise specified (i.e., MMEL proviso), placard wording and location will be determined by the aircraft operator.

	Repair Category
	All users of an MEL approved under 14 CFR parts 91 subpart K (part 91K), 121, 125, 129, or 135 must accomplish repairs of inoperative items, deferred in accordance with the MEL, at or prior to expiration of the repair intervals established by the following letter designators. Users of an MEL issued under § 91.213(a) (parts 91, 133, 137, 141, and 142) are not required to comply with the repair categories, but must comply with any provisos defining a repair interval (flights, flight legs, cycles, hours, etc.). See definition for Continuing Authorization – Single Extension.

	Repair Category A
	This category item must be repaired within the interval specified in the Remarks or Exceptions column of the aircraft operator’s MEL. For repair intervals specified in consecutive calendar-days or flight-days, the day of discovery is excluded. For all other time intervals (e.g., flights, flight legs, cycles, hours), the repair interval begins at the point when the item is deferred in accordance with the aircraft operator’s MEL.

	Repair Category B
	This category item must be repaired within 3 consecutive calendar‑days (72 hours) excluding the day of discovery. For example, if it was recorded at 10 a.m. on January 26, the 3‑day interval would begin at 0000 on January 27 and end at 2359 on January 29.

	Repair Category C
	This category item must be repaired within 10 consecutive calendar‑days (240 hours) excluding the day of discovery. For example, if it was recorded at 10 a.m. on January 26, the 10‑day interval would begin at 0000 on January 27 and end at 2359 on February 5.

	Repair Category D
	This category item must be repaired within 120 consecutive calendar‑days (2,880 hours) excluding the day of discovery.

	Required by 14 CFR
	When the MMEL contains statements such as “As Required by 14 CFR,” “Not required by 14 CFR,” or “Any in excess of those required by 14 CFR,” the listed item is subject to certain requirements expressed in 14 CFR operating rules. The number of items required by applicable 14 CFR operating rules must be operative. A dash may be used when the number required for dispatch is variable. When the listed item is not required by 14 CFR, it may be inoperative for the time specified by repair category.




	Element
	Definition

	System Page
	The MMEL system page is divided into columns that include sequence number, item, repair category, number installed, number required for dispatch, and remarks or exceptions, as well as provision for a vertical change bar. Section Two of a two-section MMEL includes columns for Crew Alerting System (CAS) message identification and dispatch consideration.

	[bookmark: _Hlk57819446]System Page - Item Number
	This column lists the unique identification for each MMEL item. 

	System Page - Item
	See definition for Item.

	System Page - Repair Category
	See definition for Repair Category.

	System Page - Number Installed
	This column indicates the number (quantity) of items normally installed in the aircraft. This number represents the aircraft configuration(s) considered in developing an MMEL. Should the number be a variable or impractical to exactly determine (e.g., optional equipment, fleet configuration differences, cockpit lighting items, cabin lighting items, cargo restraint components, Flight Data Recorder (FDR) recording parameters), a number is not required and the dash “‑” symbol is used instead. A dash or “N/A” (Not Applicable) may also be used for EFAS message relief.

	System Page - Number Required for Dispatch
	This column indicates the minimum number (quantity) of items required for operation, providing the conditions specified in the Remarks or Exceptions column are met. If the number required is predicated on an operating rule, see definition for Required by 14 CFR. A dash or “N/A” may also be used for EFAS message relief.

	System Page - Remarks or Exceptions
	This column may be blank, or it may include a statement permitting operation with a specific number of items inoperative. The statement may include a proviso for such operation and appropriate notes.

	System Page - Proviso
	A proviso is used to stipulate conditions or limitations that must be complied with for operation with the listed item inoperative.

	System Page - NOTE
	Notes provide additional information for crewmember or maintenance consideration. Notes are used to identify applicable material that is intended to assist with compliance, but do not relieve the aircraft operator of the responsibility for compliance with all applicable requirements. A note is not a part of the proviso.

	Takeoff
	Takeoff is the act of beginning a flight in which an aircraft is accelerated from a state of rest to that of flight. For the purposes of MEL relief, this translates to the point at which the pilot physically begins to apply power to initiate the takeoff from the runway or takeoff surface.

	Triple Asterisk (***)
	The triple asterisk (***) in the Item column indicates an item that may have been installed on some but not all aircraft covered by this MMEL. This symbol, however, must not be carried forward into the aircraft operator’s MEL. It should be noted that neither this policy nor the use of this symbol provides authority to install or remove an item from an aircraft.




	Element
	Definition

	Verified Operative
	When an MMEL item specifies an item must be verified operative or checked operative, it is required to check and confirm the item is operative at the interval(s) specified for that MMEL item (e.g., verified operative prior to each flight). If no interval is specified, verification is required only at the time of deferral of the original item.

	Vertical Bar (Change Bar “|”)
	A vertical bar indicates a change, addition, or deletion of content in the adjacent row of text for the current revision of that page only.

	Visible Moisture
	An atmospheric environment containing water, in any form, which can be seen in natural or artificial light (e.g., clouds, fog, rain, sleet, hail, or snow).

	Visual Flight Rules (VFR)
	VFR is as defined in 14 CFR part 91. If the Remarks or Exceptions state flight must be completed in VFR, the pilot is precluded from filing an instrument flight rules (IFR) flight plan.

	Visual Meteorological Conditions (VMC)
	VMC means the atmospheric environment is such that would allow a flight to proceed under VFR applicable to the flight. This does not preclude operation under IFR.

	(M)
	This symbol indicates a requirement for a specific maintenance procedure that must be accomplished prior to operation with the listed item inoperative. Normally, these procedures are accomplished by maintenance personnel. However, other personnel may be qualified and authorized to perform certain functions. Procedures requiring specialized knowledge or skill, or requiring the use of tools or test equipment, should be accomplished by maintenance personnel.

	(O)
	This symbol indicates a requirement for a specific operations procedure that must be accomplished in planning for or operating with the listed item inoperative. Normally, these procedures are accomplished by the flightcrew. However, other personnel may be qualified and authorized to perform certain functions.
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PL-25 APPENDIX A
Applicable sections in 14 CFR parts 91, 121, 125, 129, 135, and 137.
References current as of 08/19/2021.
NOTE:	This listing is for guidance only and is not all-inclusive. Any questions regarding applicability of a particular regulation should be resolved by a review of the regulation.
	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 21
	
	Ozone Converter
	§ 121.578

	ATA 22
	101
	Autopilot System
	Part 91 appendix G
§ 135.105

	ATA 23
	029
	Cockpit Voice Recorder (CVR) System
	§§ 91.609, 91.1045
§ 121.359
§ 125.227
§ 129.24
§ 135.151

	
	009
	Crewmember Interphone System
	§ 121.319
§ 135.150

	
	058
	Flight Deck Headsets/Headphones
Boom Microphones
	§ 91.511
§§ 121.318, 121.349, 121.359, 121.581
§§ 125.203, 125.227, 125.317
Part 135 appendix G
§§ 135.75, 135.151, 135.165

	
	106
	High Frequency (HF) Communication System
	§ 91.511
§§ 121.345, 121.347, 121.349, 121.351
§ 125.203
§ 129.17
§§ 135.98, 135.165

	
	009
	Passenger Address System
	§ 121.318
§ 135.150

	
	
	Satellite Communications (SATCOM) System
	§§ 121.99, 121.122, 121.345, 121.347, 121.349, 121.351
§ 125.203
§ 129.17
§§ 135.98, 135.165

	
	095
	Very High Frequency (VHF) and Ultrahigh Frequency (UHF) Communications Systems
	§§ 91.126, 91.127, 91.129, 91.130, 91.131, 91.135, 91.205, 91.511
§§ 121.345, 121.347, 121.349, 121.351
§ 125.203
§ 129.17
§§ 135.161, 135.165




	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 24
	107
	Electrical Generator
	§ 91.205
§ 125.205
§§ 135.159, 135.163

	ATA 25
	
	Crash Ax/Crow Bar
	§ 91.513
§ 121.309
§ 125.207
§ 135.177

	
	120
	Emergency Locator Transmitter (ELT)
	§§ 91.205, 91.207
§§ 121.339, 121.353
§§ 125.209

	
	132
	Emergency Medical Equipment
(Automated External Defibrillator (AED), Emergency Medical Kit (EMK), First Aid Kit (FAK))
	§ 91.513
Part 121 appendix A
§ 121.803
§ 125.207
§ 135.177

	
	
	Extended Overwater Equipment
(Emergency, Flotation, Survival)
	§§ 91.205, 91.509
§§ 121.309, 121.339, 121.340
§ 125.209
§ 135.167

	
	097
	Flight Attendant Seat Assembly
(Single or Dual Position)
	§ 91.533
§ 121.391
§ 125.269
§ 135.107

	
	130
	Flightcrew Rest Facilities
	Part 117

	
	132
	Megaphone
	§ 91.513
§ 121.309
§ 125.207

	
	056
	Observer Seat
	§ 121.581
§ 125.317
§ 135.75

	
	
	Shoulder Harness
	§§ 91.105, 91.1035
§ 121.311
§ 125.211
§ 135.171
§ 137.31

	
	079
	Underseat Baggage Restraining System
	§ 91.523
§ 121.589
§ 135.87

	
	
	Uninhabited Terrain Areas Emergency Equipment
	§ 121.353




	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 26
	132
	Portable Fire Extinguisher
	§ 91.513
§ 121.309
§ 125.119
§ 135.155

	ATA 30
	090
	Pitot Heat Indicating System
	§ 121.342
§ 125.206
§ 135.158

	
	
	Windshield Wiper
	Part 91 appendix A
§ 121.313
§ 125.213

	ATA 31
	
	Clock
	§ 91.205
§ 121.305

	
	087
	Flight Data Recorder (FDR) System
	Part 91 appendix E
§§ 91.609, 91.1045
Part 121 appendix M
§§ 121.343, 121.344
Part 125 appendix D/E
§§ 125.225, 125.226
§ 129.20
Part 135 appendices B–F
§ 135.152

	ATA 33
	
	Anti-Collision Light
	§§ 91.205, 91.209
§ 121.323
§ 135.159

	
	132
	Flashlight, Stowage/Charger Assemblies
(Including Flashlights)
	§ 91.503
§§ 121.310, 121.549
§§ 135.159, 135.178

	
	
	Landing Light
	§§ 91.205, 91.507
§ 121.323

	
	123
	Passenger Notice System
(Lighted Information Sign)
	§ 91.517
§§ 125.207, 125.217
§§ 135.127, 135.177

	
	
	Position Light
	§§ 91.205, 91.209
§ 121.323
§ 137.47

	
	72
	Wing Icing Detection Light
	§ 91.527
§ 121.341




	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 34
	
	Automatic Direction Finder (ADF) System
	§ 91.205
§§ 121.347, 121.351
§ 125.203

	
	039
	Altitude Alerting System
	Part 91 appendix G
§ 91.219

	
	076
	Air Traffic Control (ATC) Transponder/Automatic Altitude Reporting System
	Part 91 appendix G
§§ 91.130, 91.131, 91.135, 91.215
§ 121.345
§ 125.224
§ 135.143

	
	002
	Aural Speed Warning
	§ 91.603

	
	105
	Automatic Dependent Surveillance-Broadcast (ADS-B) System
	§§ 91.130, 91.131, 91.135, 91.225

	
	003
	Distance Measuring Equipment (DME)
	§ 91.205
§ 121.349
§ 125.203
§ 129.17
§ 135.165

	
	
	Flight Guidance System (FGS)
	Part 91 appendix A
§ 121.358

	
	
	Free-Air Temperature Indicator
	§ 121.305
§ 125.205
§ 135.163

	
	
	Gyroscopic Direction Indicator
	Part 91 appendix A
§ 121.305
§ 135.159

	
	
	Gyroscopic Pitch and Bank Indicator
	Part 91 appendix A
§ 91.205
§ 121.305
§§ 135.149, 135.159

	
	
	Gyroscopic Rate-of-Turn Indicator
	§ 91.205
§ 121.305
§ 135.159




	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 34
(Cont’d)
	
	Long-Range Navigation System
(Global Positioning System (GPS), Inertial Navigation System (INS), Flight Management System (FMS), Loran, Omega)
Short-Range Navigation System (Very High Frequency Omni-Directional Range (VOR))
	§§ 91.131, 91.205, 91.511
§§ 121.347, 121.349, 121.351, 121.355, 121.389
§§ 125.203, 125.267
§§ 129.17, 129.22
§§ 135.161, 135.165

	
	054
	Terrain Awareness and Warning System (TAWS)
	§§ 91.223, 91.1045
§§ 121.354, 121.358
§§ 135.154, 135.605

	
	
	Instrument Landing System (ILS)
	Part 91 appendix A
§§ 121.347, 121.349
§ 125.203
§ 129.17
§ 135.165

	
	
	Marker Beacon System
	Part 91 appendix A
§ 121.349
§ 125.203
§ 129.17
§ 135.165

	
	
	Radio Altimeter
(May Affect TAWS)
	Part 91 appendix A
§§ 91.205, 91.219
§ 135.160

	
	
	Slip-Skid Indicator
	§ 91.205
§ 121.305
§ 135.159

	
	111
	Standby Attitude Indicator
	§§ 91.205, 91.507
§ 121.305
§§ 135.149, 135.159

	
	
	Thunderstorm Detection
	§ 91.1045
§ 135.173




	ATA CH. #
	PL-#
	ITEM
	14 CFR REFERENCES

	ATA 34
(Cont’d)
	032
	Traffic Alert and Collision Avoidance System (TCAS)
	Part 91 appendix G
§§ 91.221, 91.1045
§ 121.356
§ 125.224
§ 129.18
§ 135.180

	
	
	Vertical Speed Indicator
	Part 91 appendix A
§ 121.305
§ 125.205
§ 135.163

	
	
	Weather Radar System
	§ 91.1045
§§ 121.357, 121.358
§ 125.223
§§ 135.173, 135.175

	
	067
	Windshear Warning System
	§ 121.358

	ATA 35
	
	Oxygen System
(Chemical or Gaseous)
	§ 91.211
§§ 121.327, 121.329, 121.331, 121.333, 121.574
§ 125.219
§§ 135.89, 135.91, 135.157

	
	132
	Portable Oxygen Dispensing Units (Or Equivalent)
(Bottle and Mask)
	§§ 121.329, 121.333

	
	132
	Protective Breathing Equipment (PBE)
	§ 121.337

	ATA 37
	
	Vacuum Indicator
	§ 125.205
§ 135.163

	ATA 71
	
	Carburetor Heat
	§ 135.149



PL-25 APPENDIX B
MEL Definition Requirements
NOTE:	This appendix is not required to be in an aircraft operator’s MEL.
	Definition
	Requirement
	Notes*

	Administrative Control Item (ACI)
	Optional*
	Required only if MEL contains ACI.

	Airplane Flight Manual (AFM), Rotorcraft Flight Manual (RFM), Pilot’s Operating Handbook (POH)
	Required*
	MEL must indicate applicable publication.

	Code of Federal Regulations (CFR) and Federal Aviation Regulations (FAR)
	Optional
	

	Considered Inoperative
	Required
	

	Contaminated Runway
	Optional*
	Required only if used in MEL.

	Continuing Authorization – Single Extension
	Required*
	Required if authorization included in OpSpec D095.

	Dash (-)
	Optional*
	Required only if (-) used in MEL.

	Day of Discovery
	Required
	

	Deactivated or Secured
	Required
	

	Deleted or Moved
	Optional
	

	Electronic Fault Alerting System (EFAS)
	Optional*
	Required if EFAS is incorporated in operator’s aircraft.

	Extended Operations (ETOPS)
	Required*
	Required only if operator conducts ETOPS.

	Excess Items
	Optional*
	Required only if used in MEL.

	Flight Day
	Required
	

	Heavy Maintenance Visit (HMV)
	Optional*
	Required only if used in MEL.

	Icing Conditions
	Required
	

	Inoperative
	Required
	

	Inoperative Components of an Inoperative System
	Required
	

	Is Not Used
	Required
	

	Item
	Required
	

	Night
	Required
	

	Nonessential Equipment and Furnishings (NEF)
	Required
	

	Operative
	Required
	

	Placarding
	Required
	

	Repair Category
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.




	Definition
	Requirement
	Notes*

	Repair Category A
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.

	Repair Category B
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.

	Repair Category C
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.

	Repair Category D
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.

	Required by 14 CFR
	Not used*
	This term is not used in MELs. MELs must contain the appropriate regulatory requirement and procedures supporting it.

	System Page
	Required
	

	System Page – Item Number
	Required
	

	System Page – Item
	Required
	

	System Page – Repair Category
	Required*
	Required for parts 91K, 121, 125, 129 and 135; not required for 91, 133, 137, and 142.

	System Page – Number Installed
	Required
	

	System Page – Number Required for Dispatch
	Required
	

	System Page – Remarks or Exceptions
	Required
	

	System Page – Proviso
	Required
	

	System Page – NOTE
	Required
	

	Takeoff
	Required
	

	Triple Asterisk (***)
	Not used
	

	Verified Operative
	Required
	

	Vertical Bar (Change Bar “|”)
	Required*
	Alternate means of compliance may be approved by the Administrator.

	Visible Moisture
	Required
	

	Visual Flight Rules (VFR)
	Required
	

	Visual Meteorological Conditions (VMC)
	Required
	

	(M)
	Required
	

	(O)
	Required
	



Each FOEB Chair should review the specific aircraft configuration(s) and apply this policy to affected MMELs through the normal FOEB process.
ORIGINAL SIGNED by
/s/ Elie T. Nasr for
Thomas F. Malone
Manager, Air Transportation Division
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