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5.2 Cargo Hook Inspection Schedule

The scheduled inspection interval noted below is a maximum and is not to be
exceeded. If the cargo hook is subjected to unusual circumstances, extreme
environmental conditions, etc., it is the responsibility of the operator to perform the
inspections more frequently to ensure proper operation.

Annually or 100 hours of external load operation, whichever comes first,
inspect the cargo hook and other kit components per the following.

1. Visually inspect for corrosion on the exterior of cargo hook, load cell and link
assembly components. Corrosion on the cargo hook side plates is cause for
immediate overhaul. Additionally, any exfoliation corrosion in the upper attach
Iug area of the cargo hook is cause for immediate replacement of the side plate.
Contact Onboard Systems for the latest revision of the cargo hook service
‘manual

2. Move the cargo hook throughout its full ranges of motion and observe the
‘manual release cable and electrical hamess to ensure that they have enough
slack. The release cable and harness must not be the stops that prevent the cargo
ook or suspension from moving freely in all directions

3. Visually inspect cargo hook for presence and security of fasteners, electrical
connection, and manual release cable connection.

4. Visually inspect the cargo hook for cracks, damage and corrosion.




