Highlights of Change:

Cover – Updated Revision Status to Rev 7
Page iv – Updated RECORD OF REVISIONS
Pages vi thru xi - Updated LOG OF EFFECTIVE PAGES to reflect Rev 7 – Changes indicated by dates
Preamble Pages 4-1 thru 4-4 verbiage updates
Preamble Pages 4-5 & 4-6.  Change verbiage on NOTE’s B section updated
A0051.4 Page 2 – Removed ASB Reference for Pillow Block Torque check – Incorporated into Bell MM Chp 4. Now in A0100
A0052 Page 3 – Moved A0052.7 HYDRAULIC section A0052.7 to A0054 to even out inspections
A0052 Page 4 – Cleaned up verbiage in MAIN DRIVE SHAFT to identify as greased driveshaft 
A0052 Page 5 – Moved A0052.11 Lubrications now in own A0100 100 hour insp
A0053 Page 2 - Removed Pillow Block Torque Check – Now incorporated into Bell MM Chp 4 - Now in A0100
A0054 Page 1 – Renamed A0054.5 TAIL ROTOR DRIVETRAIN to FREEWHEELING UNIT. 
A0054 Page 2 – Moved all shaft insp and lubrications to A0100
A0054 Page 2 – Added HYDRAULIC section taken from A0052
A0054 Page 1 – Changed A054.5 TAIL ROTOR DRIVETRAIN to FREEWHEELING UNIT 
A0054 Page 2 – Moved driveshaft inspections and lubs to own Insp  A0100 (Are due every 100 hours)
A0054 Page 2 – Added HYDRAULIC from A0052
A0054 Page 3 – Moved A0055.8.1 Pillow blocks to A0100 (Chp 4 - 110-hour requirement)
A0056 Page 3 – Removed A0056.7 LUBRICATION. Now C/W every 100 hours in A0100
A0100 added to track 100-hour items (bulk is lubes).
A1203 Deleted.  (Tailboom Insp) Moved to INSPECTIONS EXCLUDED FROM AAIP. Cyclic stick insp now A 1202.
A1720 Page 2 – Added Oil Cooler impeller, shaft and bearings.  Repaginated A1720
A6010 Removed – Now tracked on Status Sheets. Part comes off, overhauled, then put into rotables.

B section was revamped.  All 150 hr inspections were removed from the other inspections and put in their own AAIP section B 0150NT.  The remaining inspections were divided into 4, AAIP 300 hr / 12 Mon inspections. These are each “Stand-Alone” in they can be completed at any time, not required 50 hours after last insp.:
B0301NT
B0302NT
B0303NT
B0304NT
Removed Compressor Fresh Water Rinse from all B section and will now be tracked on the Aircraft CALM status reports at 100-hour intervals. Removed 150 hr Fuel Nozzle cleaning, now tracked in CALM Status Reports.

C0110 Added for 100-hour NVG inspection.
C0120 – 12 Mon Insp - All pages renamed to reflect correct AAIP 12-month designator, now C 1700
C0010 – C0060 (6 inspections) were consolidate into 3 inspections C 0301 – C0303
C1710 – Added for 12 Mon NVG inspection.
C1720 Page 7 – Added C1720.18 AAI TAIL ROTOR LOCKOUT KIT (currently tracked on status report)
C1720 Page 8 – Added C1720.19 AAI LOCKING FUEL CAP (currently tracked on status report)
Attachment A-1 – Added #1 ASU Night Vision Goggle Lighting System, #9 AAI TAIL ROTOR LOCKOUT KIT, #10 AAI LOCKING FUEL CAP and #26 DART AVIONICS CONSOLE (all currently tracked on status report)
Attachment B – Added Rolls-Royce Engine Wash & 150 hr Fuel Nozzle cleaning to INSPECTIONS EXCLUDED FROM AAIP; engine washes will now be tracked on MHI CALM aircraft status report at 100-hour intervals.

