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1
INSPECTIONS EXCLUDED FROM AAIP 
Since the AAIP inspection program is not intended to prescribe maintenance functions, the following items will be tracked separately in the aircraft status report. 

A. Hand-held Fire Extinguishers
B. Static System and Altitude Reporting System per 14 CFR 91.411.
C. ATC Transponder Test and Inspections per 14 CFR 91.413.
D. Inspect Pitot-Static System per 14 CFR 91.411/413 
E. 36 Month Hydrostatic Retest of Emergency Floatation Gas Cylinder per AA-ICA407-11
F. 1500 Hour Mast Overhaul BHT-206L Series MM-1  Table 5-40

G. 2250 Hour / 60 Month Transmission Overhaul BHT-206L Series MM-1  Table 5-41

H. 3000 Hour Tail Rotor Gearbox Overhaul BHT-206L Series MM-1  Table 5-42

I. 300 Hour N1 and N2 Tach Gen Spline Insp/lube BHT-206L Series MM-1  Para 5-23 Item 16

J. Engine Wash – Rolls-Royce M250-C30 Series MM 72-30-00 Para 5.B


